(footprint "2P_4.5x3_3.5_pitch" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "ReparationShave.kicad_sch")
  (property "Sheetname" "")
  (attr exclude_from_pos_files)
  (fp_text reference "L2" (at 0 -4) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d178ffda-dc16-4a76-95e0-59b3fc3be9c8)
  )
  (fp_text value "Heater" (at 2.8 0 270) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)))
    (tstamp 9c9be568-f952-45f0-a0a0-1626874087ef)
  )
  (fp_line (start -2.5 -2.75) (end -2.5 -0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 57087a65-e550-44c6-960b-836455ea3c9b))
  (fp_line (start -2.5 0.75) (end -2.5 2.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2df2430a-d167-456c-8852-15242ad20722))
  (fp_line (start -1.75 3.5) (end 1.75 3.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp aff9c1b4-0be6-4876-850d-46f2701dbdd7))
  (fp_line (start 1.75 -3.5) (end -1.75 -3.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6924cbaa-f84a-490c-a90e-237860e2a160))
  (fp_line (start 2.5 -0.75) (end 2.5 -2.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a7ce6fd4-31bf-4d0e-8371-edf984055716))
  (fp_line (start 2.5 2.75) (end 2.5 0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2cd901bf-fcfd-4e3b-ae12-fe11b65081ec))
  (fp_arc (start -2.5 -2.75) (mid -2.28033 -3.28033) (end -1.75 -3.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 72ddaad0-4faa-4dc6-87bd-29112a508210))
  (fp_arc (start -2.5 0.75) (mid -2.28033 0.21967) (end -1.75 0)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ae021488-9b13-42b8-a6b3-caf055f06cc9))
  (fp_arc (start -1.75 0) (mid -2.28033 -0.21967) (end -2.5 -0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 66fc41ae-35ec-4d41-afb9-c1aa68add06c))
  (fp_arc (start -1.75 3.5) (mid -2.28033 3.28033) (end -2.5 2.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 95bb16af-ba5e-4a28-a5aa-326c612afd20))
  (fp_arc (start 1.75 -3.5) (mid 2.28033 -3.28033) (end 2.5 -2.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6cb5c780-f65a-4754-bcf3-5fc5c6686b25))
  (fp_arc (start 1.75 0) (mid 2.28033 0.21967) (end 2.5 0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ca5b1fc7-8d9b-4572-946f-34c815871052))
  (fp_arc (start 2.5 -0.75) (mid 2.28033 -0.21967) (end 1.75 0)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0b9f463a-9e05-48d6-98e8-bd873b048968))
  (fp_arc (start 2.5 2.75) (mid 2.28033 3.28033) (end 1.75 3.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 60a165fa-c725-4ad2-b239-1be491b43933))
  (pad "1" connect roundrect (at 0 -1.75) (size 4.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.167) (tstamp 7cf398d7-347d-49d2-aec4-145670c76d11))
  (pad "2" connect roundrect (at 0 1.75) (size 4.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.167) (tstamp 8162e88e-c566-47d7-8d53-7a9a720861ec))
)
