(module Spark_Gap_1.1x2_Double_Feed_Through (layer F.Cu) (tedit 54538004)
  (solder_mask_margin 0.01)
  (solder_paste_margin -0.001)
  (attr virtual)
  (fp_text reference GA2 (at 0 -1.6) (layer F.SilkS) hide
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value Spark_Gap (at 0 0.7) (layer F.SilkS) hide
    (effects (font (size 0.2 0.2) (thickness 0.05)))
  )
  (pad 1 smd rect (at -0.45 0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (pad 1 smd rect (at -0.3 0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -0.15 0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 0 0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 0.15 0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 0.3 0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 0.45 0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at 0 0) (size 1.1 0.2) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (pad 3 smd oval (at 0 0.9) (size 1.1 0.2) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (pad 1 smd rect (at 0 0.45) (size 0.5 0.2) (layers F.Cu F.Mask)
    (solder_mask_margin 0.25))
  (pad 3 smd oval (at 0 -0.9) (size 1.1 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.45 -0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.3 -0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.15 -0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0 -0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.15 -0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.3 -0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.45 -0.45 45) (size 0.282843 0.282843) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0 -0.45) (size 0.5 0.2) (layers F.Cu F.Mask)
    (solder_mask_margin 0.25))
)
