(footprint "Micro Four Thirds Lens Mount" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "RK3588_Camcorder_Carrier.kicad_sch")
  (property "Sheetname" "")
  (fp_text reference "A6" (at 0.1 -25.3 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 27b12fca-1b69-4696-989a-a4df9d22d530)
  )
  (fp_text value "~" (at 0 23.3 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 37ebb372-10d8-404f-9e2f-c9bfb3427ecc)
  )
  (fp_text user "${REFERENCE}" (at 0 25.1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d7413e71-c1e4-4bf3-ac07-8229bf1fad4b)
  )
  (fp_rect (start -10.5 -10) (end 10.5 10)
    (stroke (width 0.12) (type default)) (fill none) (layer "Dwgs.User") (tstamp 6ac9dd56-9518-48b8-ae17-ed9453ad0734))
  (fp_line (start -2 0) (end 2 0)
    (stroke (width 0.1) (type dash)) (layer "F.Fab") (tstamp dad98202-9638-475c-80c8-f7ed78f0f50a))
  (fp_line (start 0 -2) (end 0 2)
    (stroke (width 0.1) (type dash)) (layer "F.Fab") (tstamp b21087d8-f16b-4559-b6ba-e992b1642239))
  (fp_circle (center 0 0) (end 19.3929 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.Fab") (tstamp a4af7029-6aa2-4168-a51e-53a9af8153e3))
  (fp_circle (center 0 0) (end 20.612 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.Fab") (tstamp 1f44a266-4b10-46f7-b199-c8621088dc9a))
  (fp_circle (center 0 0) (end 26.543 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.Fab") (tstamp 0c3e49b0-85ae-4f01-a05c-606880eb68fb))
  (pad "MP" thru_hole circle (at -19.5 -13) (size 4.1 4.1) (drill 2.1) (layers *.Cu *.Mask) (tstamp 22a7cbb9-370a-42b3-bb52-695583ae894a))
  (pad "MP" thru_hole circle (at -19.5 13) (size 4.1 4.1) (drill 2.1) (layers *.Cu *.Mask) (tstamp e183a9c8-1db9-45bd-b9ad-6ea048779bb5))
  (pad "MP" thru_hole circle (at 19.5 -13) (size 4.1 4.1) (drill 2.1) (layers *.Cu *.Mask) (tstamp 56624ce8-e299-4411-ac74-1b6abcde1954))
  (pad "MP" thru_hole circle (at 19.5 13) (size 4.1 4.1) (drill 2.1) (layers *.Cu *.Mask) (tstamp 2eb762a2-5600-44d3-9e9e-8f36dba3f5f4))
)
