(module C_Radial_D25_L42_P10 (layer F.Cu) (tedit 557827E1)
  (descr "Radial Electrolytic Capacitor Diameter 26mm x Length 45mm, Pitch 10mm")
  (tags "Electrolytic Capacitor")
  (fp_text reference REF** (at 0 -14.3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value C_Radial_D25_L42_P10 (at 0 14.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 11.75 -2.5) (end 12 -0.5) (layer F.SilkS) (width 1))
  (fp_line (start 12 -0.5) (end 12 0.75) (layer F.SilkS) (width 1))
  (fp_line (start 12 0.75) (end 11.75 2.5) (layer F.SilkS) (width 1))
  (fp_line (start 11.75 2.5) (end 11.5 3.5) (layer F.SilkS) (width 1))
  (fp_line (start 11.5 3.5) (end 11 4.75) (layer F.SilkS) (width 1))
  (fp_line (start 11 4.75) (end 10.5 5.75) (layer F.SilkS) (width 1))
  (fp_line (start 10.5 5.75) (end 9.75 7) (layer F.SilkS) (width 1))
  (fp_line (start 11.25 -4) (end 11 -4.75) (layer F.SilkS) (width 1))
  (fp_line (start 11 -4.75) (end 10.25 -6.25) (layer F.SilkS) (width 1))
  (fp_line (start 11.75 -2.5) (end 11.25 -4.25) (layer F.SilkS) (width 1))
  (fp_line (start 11 -3.75) (end 11 -4.75) (layer F.SilkS) (width 1))
  (fp_line (start 11.25 -2) (end 11.25 -4.25) (layer F.SilkS) (width 1))
  (fp_line (start 10.5 -5) (end 10.5 -5.75) (layer F.SilkS) (width 1))
  (fp_line (start 9.75 -6.75) (end 10 -6.75) (layer F.SilkS) (width 1))
  (fp_line (start 10.25 -4.75) (end 10.25 -6.25) (layer F.SilkS) (width 1))
  (fp_line (start 9.75 7) (end 9.75 -7) (layer F.SilkS) (width 1))
  (fp_line (start 10.75 5.25) (end 10.75 -5.25) (layer F.SilkS) (width 1))
  (fp_line (start 11.75 -2.5) (end 11.75 2.5) (layer F.SilkS) (width 1))
  (fp_circle (center 0 0) (end 0 -12.5) (layer F.SilkS) (width 0.125))
  (fp_circle (center 0 0) (end 0 -12.75) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole rect (at -5 0) (size 4 4) (drill 2.2) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 5 0) (size 4 4) (drill 2.2) (layers *.Cu *.Mask))
  (model 3D/walter/capacitors/cp_25x45mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
