(footprint "JST_SFH_SM02B-SFHRS-TF_1x02-1MP_P4.20mm_Horizontal"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(locked yes)
	(layer "F.Cu")
	(descr "JST SFH series connector, SM02B-SFHRS-TF (http://www.jst-mfg.com/product/pdf/eng/eSFH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST SFH horizontal")
	(property "Reference" "J17"
		(at 0 -3.8 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "a519948d-8125-481f-ab98-8ec546564469")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "VIN"
		(at 0 4.42 180)
		(layer "F.Fab")
		(uuid "4dc785ed-24e6-4b52-a5ad-e607226b19e8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_JST:JST_SFH_SM02B-SFHRS-TF_1x02-1MP_P4.20mm_Horizontal"
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "b0096a22-fb74-4ab2-a5bc-0eed59891423")
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify mirror)
		)
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "6197e168-c435-4168-aea5-3a9af6ba06eb")
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify mirror)
		)
	)
	(property "Description" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "214870fc-9072-4ad1-9abf-e51ea8b31b79")
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify mirror)
		)
	)
	(property "LCSC" "C265122"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "d80ab463-ce51-446c-99bf-5503624f435b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "JST"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "e995954f-50e0-423d-94af-46cc4cd8900a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "SM02B-SFHRS-TF(LF)(SN)"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "9694ef03-8208-4b62-a526-334b3b576f5b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.71 1.215)
		(end -2.71 -1.165)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9c22897e-8b9c-4b57-95ad-73ff9daee47d")
	)
	(fp_line
		(start 1.315 -2.985)
		(end -1.315 -2.985)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "310565d2-cec3-4737-ba1b-ac7a77939e62")
	)
	(fp_line
		(start 1.515 3.135)
		(end -1.515 3.135)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ea19789f-3de7-4888-9040-a094bf9b535b")
	)
	(fp_line
		(start 2.71 1.215)
		(end 2.71 -1.165)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8917c797-1823-40ab-a330-2fd74e9c4bc5")
	)
	(fp_poly
		(pts
			(xy -2.1 -3.4) (xy -2.35 -3.8) (xy -1.85 -3.8)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "fcdc622e-b28d-4695-9e32-9f9636435003")
	)
	(fp_line
		(start -2.85 -3.05)
		(end -2.85 3.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "50de8e12-ca5b-45a9-84c5-7351cc7d3c7e")
	)
	(fp_line
		(start -2.5 -3.4)
		(end 2.5 -3.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f3568709-21ad-4738-98ac-016ceae1e1d9")
	)
	(fp_line
		(start 2.5 3.4)
		(end -2.5 3.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5696120f-e45e-4980-a748-248865dbe6b4")
	)
	(fp_line
		(start 2.85 -3.05)
		(end 2.85 3.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7c1f4d50-3c4b-42bf-bbe1-709a7651d47f")
	)
	(fp_arc
		(start -2.85 -3.05)
		(mid -2.747487 -3.297487)
		(end -2.5 -3.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bd3b3370-5b81-4d1d-b7b0-fc772ca781f1")
	)
	(fp_arc
		(start -2.5 3.4)
		(mid -2.747487 3.297487)
		(end -2.85 3.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "de889fad-0199-4f2c-904a-a2e4bdbd94a1")
	)
	(fp_arc
		(start 2.5 -3.4)
		(mid 2.747487 -3.297487)
		(end 2.85 -3.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "859bc141-5a7a-4900-9f25-1627e68f54f9")
	)
	(fp_arc
		(start 2.85 3.05)
		(mid 2.747487 3.297487)
		(end 2.5 3.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7746f16e-8afb-45de-b5de-6e13ba66202c")
	)
	(fp_line
		(start -2.6 3.025)
		(end -2.6 -2.875)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "18cb52fd-89f5-4467-a744-c1e45c9b4633")
	)
	(fp_line
		(start 2.6 -2.875)
		(end -2.6 -2.875)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5972b00f-a134-4e24-b029-d22b34c7c521")
	)
	(fp_line
		(start 2.6 3.025)
		(end -2.6 3.025)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "abfdf998-d9a7-4307-a67f-1b80d1a5ab88")
	)
	(fp_line
		(start 2.6 3.025)
		(end 2.6 -2.875)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ca9f93d3-1f1d-40aa-9928-32cf561bb290")
	)
	(fp_text user "${REFERENCE}"
		(at 0 5.75 180)
		(layer "F.Fab")
		(uuid "f1822f9d-ef94-4d97-98f1-c24e7b32718b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.1 -2.325)
		(size 1.05 1.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2380952381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ca5ed8f6-838a-4aa6-a9ed-4d4f25256ec9")
	)
	(pad "2" smd roundrect
		(at 2.1 -2.325)
		(size 1.05 1.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2380952381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9d735eab-485d-4bab-aac2-78e460f12680")
	)
	(pad "MP" smd roundrect
		(at -2.2 2.35)
		(size 0.85 1.75)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9384c418-eefb-4ad7-8a3e-a2b7b28c3723")
	)
	(pad "MP" smd roundrect
		(at 2.2 2.35)
		(size 0.85 1.75)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5f7789fc-2a52-4402-ad85-a72de1958f66")
	)
	(model ":KICAD7_3DMODEL_DIR:Connector_JST.3dshapes/SM02B-SFHRS-TF.STEP"
		(offset
			(xyz 0 0.98 2.125)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)