(footprint "JST_SH_SM09B-SRSS-TB_1x09-1MP_P1.00mm_Horizontal"
	(version 20231231)
	(generator "pcbnew")
	(generator_version "7.99")
	(layer "F.Cu")
	(descr "JST SH series connector, SM09B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST SH top entry")
	(property "Reference" "J9"
		(at 0 -3.98 180)
		(layer "F.SilkS")
		(uuid "6dd214b3-b708-4e7d-a1bf-66d707ca6459")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SYS"
		(at 0 3.98 180)
		(layer "F.Fab")
		(uuid "91d87a72-50d3-4f48-a2a4-ad7cd2150667")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_JST:JST_SH_SM09B-SRSS-TB_1x09-1MP_P1.00mm_Horizontal"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "dfe94db6-0d29-4003-b072-eaaa7acc79da")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2a53b937-e555-479f-9f07-44e3a438fa3d")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" "Generic connectable mounting pin connector, single row, 01x09, script generated (kicad-library-utils/schlib/autogen/connector/)"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a1063faa-96e9-4d36-898e-5fd04628cb10")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -5.61 -1.785001)
		(end -4.56 -1.785001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3ac89c80-6f2b-4e2e-b40d-ae1fe1878104")
	)
	(fp_line
		(start -5.61 0.715)
		(end -5.61 -1.785001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "37cf8372-4d8e-4a2f-8a1d-32dbf1b061e5")
	)
	(fp_line
		(start -4.56 -1.785001)
		(end -4.56 -2.775)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dcaaa1cb-f490-48e4-b246-6d42ad9db2cd")
	)
	(fp_line
		(start -4.44 2.685)
		(end 4.44 2.685)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "70acdf01-6c5c-4016-9f8e-385fbcc15f33")
	)
	(fp_line
		(start 5.61 -1.785001)
		(end 4.56 -1.785001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "49777b81-8c05-4b30-a4cd-09a42ece80ca")
	)
	(fp_line
		(start 5.61 0.715)
		(end 5.61 -1.785001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "336c2931-4a5f-4878-bb3e-3875cafae9fa")
	)
	(fp_line
		(start -6.05 1.225)
		(end -6.05 2.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "18bb2da4-5051-44d4-820b-405cd2e7c02a")
	)
	(fp_line
		(start -5.75 -1.675)
		(end -5.753065 0.838506)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "63de15b0-811e-463c-8b3a-83afefa8836a")
	)
	(fp_line
		(start -5.65 2.925)
		(end 5.65 2.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "209f3cfc-18c6-4c00-b2a1-f236f69edef4")
	)
	(fp_line
		(start -5.5 -1.925)
		(end -4.45 -1.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5c0c58df-5714-49c2-b66d-32c0848a8d37")
	)
	(fp_line
		(start -4.45 -1.925)
		(end -4.45 -2.625)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9f8d7c58-a5e4-4329-8935-51afd269f668")
	)
	(fp_line
		(start 4.15 -2.925)
		(end -4.15 -2.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "992e317e-66e0-4721-a6cb-2d9c6d16aded")
	)
	(fp_line
		(start 4.45 -1.925)
		(end 4.45 -2.625)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0586d3b0-b27a-40a0-a2f4-2e3965cc245b")
	)
	(fp_line
		(start 5.5 -1.925)
		(end 4.45 -1.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "fb9a5ecd-1535-4b0c-a1e5-40ccf0c981ee")
	)
	(fp_line
		(start 5.75 -1.675)
		(end 5.753065 0.838506)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ac4b7dbd-3e8a-40b6-87a6-8d74ec922c38")
	)
	(fp_line
		(start 6.05 1.225)
		(end 6.05 2.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d62d6b5a-ca90-49ce-a0a2-0a2477e72eab")
	)
	(fp_arc
		(start -6.05 1.225)
		(mid -5.967196 0.981306)
		(end -5.753065 0.838506)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f818c95a-6739-46eb-989b-c661c924fdac")
	)
	(fp_arc
		(start -5.75 -1.675)
		(mid -5.676777 -1.851777)
		(end -5.5 -1.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "192aabaa-09a2-4354-8acf-c04fb1061729")
	)
	(fp_arc
		(start -5.65 2.925)
		(mid -5.932843 2.807843)
		(end -6.05 2.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e9218a41-10b7-4f29-b9b9-368604915462")
	)
	(fp_arc
		(start -4.45 -2.625)
		(mid -4.362132 -2.837132)
		(end -4.15 -2.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f3f13a63-e544-4c9b-968e-1f53f992ed75")
	)
	(fp_arc
		(start 4.15 -2.925)
		(mid 4.362132 -2.837132)
		(end 4.45 -2.625)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "fc7b83c6-ec00-46b9-9aac-4e5be2b70b59")
	)
	(fp_arc
		(start 5.5 -1.925)
		(mid 5.676777 -1.851777)
		(end 5.75 -1.675)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c53668ed-190f-4067-a45a-b43721fa4aca")
	)
	(fp_arc
		(start 5.753065 0.838506)
		(mid 5.967196 0.981306)
		(end 6.05 1.225)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cac9b825-98c6-44f2-a408-ba8cd93e1148")
	)
	(fp_arc
		(start 6.05 2.525)
		(mid 5.932843 2.807843)
		(end 5.65 2.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f80f9267-b23f-41f5-a245-d2fc8dda7a55")
	)
	(fp_line
		(start -5.5 -1.675)
		(end -5.5 2.575)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "774d499c-8b21-4818-a4c2-cfbe25522e51")
	)
	(fp_line
		(start -5.5 -1.675)
		(end 5.5 -1.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3563a21f-c7ef-4141-b401-970a449b609a")
	)
	(fp_line
		(start -5.5 2.575)
		(end 5.5 2.575)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d0ea9816-002a-4fb1-a598-6bc4a0520c51")
	)
	(fp_line
		(start -4.5 -1.674999)
		(end -4 -0.967893)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2d41f44b-bdcc-43b6-ac0d-935ced3f04e4")
	)
	(fp_line
		(start -4 -0.967893)
		(end -3.5 -1.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "93e3039b-e0ce-4f68-88b6-dfd3339e48e6")
	)
	(fp_line
		(start 5.5 -1.675)
		(end 5.5 2.575)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b15e5b96-faf6-4e54-924c-8c2bb1c6c0f6")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "f8621a4a-dbe6-4028-abba-05164fd9218e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -4.000001 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "d3932542-d026-40a4-a041-d1e9d9ef3d21")
	)
	(pad "2" smd roundrect
		(at -3 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "bd431271-2b0b-4b75-94bf-1f445b705ef6")
	)
	(pad "3" smd roundrect
		(at -2 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "cd5d0140-5c7b-4644-a189-6e97e9424921")
	)
	(pad "4" smd roundrect
		(at -1 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "37b590ac-37b6-40d1-93c1-fe378578da82")
	)
	(pad "5" smd roundrect
		(at 0 -2.000001)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "49ee5bd6-fca9-45b5-b041-79da106b934b")
	)
	(pad "6" smd roundrect
		(at 1 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "e91f2771-118e-4991-b128-5ba93fc27d3a")
	)
	(pad "7" smd roundrect
		(at 2 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "4f6f9940-2123-426d-ba85-7cdde32dff44")
	)
	(pad "8" smd roundrect
		(at 3 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "8b402fd4-0c19-405e-b109-e63a87867e90")
	)
	(pad "9" smd roundrect
		(at 4.000001 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "474f28ea-a2b7-41cc-9f90-3536e62da117")
	)
	(pad "MP" smd roundrect
		(at -5.3 1.875)
		(size 1.2 1.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.208333)
		(uuid "aa159fff-966b-43b5-a605-8ac080941398")
	)
	(pad "MP" smd roundrect
		(at 5.3 1.875)
		(size 1.2 1.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.208333)
		(uuid "48ba5a8b-c936-4a65-b4e1-fcf8e3291b08")
	)
	(model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM09B-SRSS-TB_1x09-1MP_P1.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM09B-SRSS-TB.STEP"
		(offset
			(xyz 0 -0.45 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)