(module JP1_2mm (layer F.Cu) (tedit 5489677E)
  (fp_text reference JP1_2mm (at 0 -1.75) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value VAL** (at 0 1.75) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start -1 -1) (end 1 -1) (layer F.SilkS) (width 0.127))
  (fp_line (start 1 -1) (end 1 1) (layer F.SilkS) (width 0.127))
  (fp_line (start 1 1) (end -1 1) (layer F.SilkS) (width 0.127))
  (fp_line (start -1 1) (end -1 -1) (layer F.SilkS) (width 0.127))
  (fp_line (start 2 -2) (end -2 -2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2 -2) (end 2 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2 2) (end -2 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2 2) (end -2 -2) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole circle (at 0 0) (size 1.54 1.54) (drill 1) (layers *.Cu *.Mask))
)
