(footprint "L_7.3x7.3_H3.5"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Choke, SMD, 7.3x7.3mm 3.5mm height")
	(tags "Choke SMD")
	(property "Reference" "L3"
		(at 0 -4.45 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "130675b0-7b1d-41a9-9e37-346e7380e2c3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "5.6uH"
		(at 0 4.45 180)
		(layer "F.Fab")
		(uuid "b4abea9f-3dcd-4525-8822-07b3ba493814")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Inductor_SMD:L_7.3x7.3_H3.5"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bba9ea00-de59-4508-9f7e-2e43c0854fb0")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b3b67cde-bd50-4005-a549-4b30d4fcf01e")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0b4b44ed-03b4-438f-912e-b96256cb2363")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "LCSC" "C497868"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a8e9c20e-7403-40fa-92a9-5d2accc917d6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "YJYCOIN"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a4930c14-3bc5-43a1-b14e-e39a7ba5d1f3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "YSPI0630A-5R6M"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a0b64105-2832-4579-88ae-f6ecb226f70a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "075492d3-631d-451a-9c04-802a95cc6391")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_arc
		(start -3.724999 -3.650001)
		(mid -3.703032 -3.703033)
		(end -3.65 -3.725)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d672c124-c59f-4511-b024-87d32f5484ba")
	)
	(fp_arc
		(start -3.650001 3.724999)
		(mid -3.703033 3.703032)
		(end -3.725 3.65)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "509df2ba-41c9-4870-af64-fbef6254c493")
	)
	(fp_arc
		(start 3.650001 -3.724999)
		(mid 3.703033 -3.703032)
		(end 3.725 -3.65)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "471bb827-6a22-4a0e-a49d-bf91e2c54fb6")
	)
	(fp_arc
		(start 3.724999 3.650001)
		(mid 3.703032 3.703033)
		(end 3.65 3.725)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "cb4e8f99-da29-49a1-acdd-32ef9b9fda24")
	)
	(fp_poly
		(pts
			(xy -3.65 -3.65) (xy -3.65 -3) (xy -3.8 -3) (xy -3.8 -3.65) (xy -3.65 -3.8) (xy -3 -3.8) (xy -3 -3.65)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "5f3ceecc-e331-4110-ab43-152be7389d97")
	)
	(fp_poly
		(pts
			(xy -3.65 3.65) (xy -3 3.65) (xy -3 3.8) (xy -3.65 3.8) (xy -3.8 3.65) (xy -3.8 3) (xy -3.65 3)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "e62f0bd6-050a-40bc-8e01-c21e42a0b79f")
	)
	(fp_poly
		(pts
			(xy 3.65 -3.65) (xy 3 -3.65) (xy 3 -3.8) (xy 3.65 -3.8) (xy 3.8 -3.65) (xy 3.8 -3) (xy 3.65 -3)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "f1382227-ec3e-49e5-866f-c49557e6129c")
	)
	(fp_poly
		(pts
			(xy 3.65 3.65) (xy 3.65 3) (xy 3.8 3) (xy 3.8 3.65) (xy 3.65 3.8) (xy 3 3.8) (xy 3 3.65)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "271be5b8-d930-4202-97d9-870292d0061c")
	)
	(fp_line
		(start -4.2 -3.9)
		(end -4.2 3.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "01a7f4ab-e6c7-4171-908b-e468cf9f3ffd")
	)
	(fp_line
		(start -4.2 3.9)
		(end 4.2 3.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "dd1e307e-2f05-42c0-b714-4ef056dc6a11")
	)
	(fp_line
		(start 4.2 -3.9)
		(end -4.2 -3.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c2dc0938-6afc-4adc-b9c4-3a8e75c94520")
	)
	(fp_line
		(start 4.2 3.9)
		(end 4.2 -3.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fa57d88d-2adb-4957-8357-58e9c6e41ea5")
	)
	(fp_line
		(start -3.65 -3.65)
		(end -3.65 -1.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "388e60f0-c60d-43ab-87cf-d1cb0a2356ce")
	)
	(fp_line
		(start -3.65 -3.65)
		(end 3.65 -3.65)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "23457b21-e03a-4ef2-b5cd-98ce5e598f11")
	)
	(fp_line
		(start -3.65 3.65)
		(end -3.65 1.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1c63b56a-7c98-480f-b86d-71166f6be545")
	)
	(fp_line
		(start 3.65 -3.65)
		(end 3.65 -1.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fce3b475-6f70-4ca8-b682-c9314c6d45b2")
	)
	(fp_line
		(start 3.65 3.65)
		(end -3.65 3.65)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "046845ed-3749-462c-975e-b7ac00d83c6f")
	)
	(fp_line
		(start 3.65 3.65)
		(end 3.65 1.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8ab8c48b-2fdd-4984-84b8-3816d63153db")
	)
	(fp_arc
		(start -2.29 -2.29)
		(mid 0 -3.238549)
		(end 2.29 -2.29)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7d07c38d-942c-41e7-98ec-339c1cb49249")
	)
	(fp_arc
		(start 2.29 2.29)
		(mid 0 3.238549)
		(end -2.29 2.29)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7e8dce3e-ca4d-42d9-8ef2-f45fd5c0767a")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "1dc52878-caa2-4915-8f8a-8a8252979b94")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3 0)
		(size 1.8 3.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "01bcd00c-2ddb-41a2-b08c-f4e62a299552")
	)
	(pad "2" smd roundrect
		(at 3 0)
		(size 1.8 3.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "89ad3c41-f36d-49eb-b465-1d287ee5d0a9")
	)
	(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_7.3x7.3_H3.5.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD7_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_TDK_SLF7032.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)