(footprint "JST_XH_B3B-XH-AM_1x03_P2.50mm_Vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "JST XH series connector, B3B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST XH vertical boss")
	(property "Reference" "J4"
		(at 2.5 -3.55 0)
		(layer "F.SilkS")
		(uuid "ee475cbc-8d0e-410e-aac0-f96daf2f7745")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "End-stop 4"
		(at 2.5 4.6 0)
		(layer "F.Fab")
		(uuid "50c55bd2-992e-484e-8860-574505c9bcf2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_JST:JST_XH_B3B-XH-AM_1x03_P2.50mm_Vertical"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ac7a90e1-9283-4635-bf6a-00d6ce4a461c")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "092aa488-16ab-4e8c-8a4e-958d9279b791")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" "Generic connector, single row, 01x03, script generated"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "93752efd-6ac3-49a1-ab92-b01b99979f4f")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "MPN" "B3B-XH-AM(LF)(SN)"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1d9e48e7-c6ef-4643-8b1c-7ceea68850ff")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C161870"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1d197070-3a71-45f6-af62-1b06c4a435b1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "JST"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3c836086-cef1-4354-abfb-44854e8d25f0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -2.85 -2.75)
		(end -2.85 -1.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f4f8dbc4-c3e7-4357-888e-07be2697324a")
	)
	(fp_line
		(start -2.56 -2.46)
		(end -2.56 3.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c45ad563-5d4c-4d02-8f96-7a8cbcab7c27")
	)
	(fp_line
		(start -2.56 3.51)
		(end 7.56 3.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c8936c4a-d50e-4669-96e3-1dc20e580679")
	)
	(fp_line
		(start -2.55 -2.45)
		(end -2.55 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6cdd2e9b-c44b-4ffb-a2c0-dcd8f535797d")
	)
	(fp_line
		(start -2.55 -1.7)
		(end -0.750001 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "57ac10fc-81c7-4f52-a35d-777176b290ad")
	)
	(fp_line
		(start -2.55 -0.2)
		(end -1.8 -0.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "896b51b7-c3f0-474e-8a81-df600b586818")
	)
	(fp_line
		(start -1.8 -0.2)
		(end -1.8 1.14)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "27a3a30d-d179-4e37-a7d6-578e67bc3046")
	)
	(fp_line
		(start -1.6 -2.75)
		(end -2.85 -2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8a012335-d7be-40f4-961e-b25a282a8697")
	)
	(fp_line
		(start -0.750001 -1.7)
		(end -0.75 -2.450001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "53d720d0-f7d1-48bc-bd89-76cdfb2541f3")
	)
	(fp_line
		(start -0.75 -2.450001)
		(end -2.55 -2.45)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "76f5063b-7de9-4bce-99c8-96c265482514")
	)
	(fp_line
		(start 0.75 -2.450001)
		(end 0.750001 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "369e7fa2-07ff-4b61-93d1-c2994ff3e568")
	)
	(fp_line
		(start 0.750001 -1.7)
		(end 4.25 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "083d8f05-3ee0-4006-81ce-182aebfe2eff")
	)
	(fp_line
		(start 2.5 2.75)
		(end -0.74 2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6c30a9fd-daa9-41e7-9865-6e9080dc2fde")
	)
	(fp_line
		(start 4.25 -2.45)
		(end 0.75 -2.450001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "91c67ea5-4d8f-4ab3-8bd8-bfbdba6ad5cc")
	)
	(fp_line
		(start 4.25 -1.7)
		(end 4.25 -2.45)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cdd6ccee-07eb-47ef-b8f4-3ff76595ca55")
	)
	(fp_line
		(start 5.75 -2.450001)
		(end 5.75 -1.700001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c9da4151-3571-496b-81f2-2063388eca96")
	)
	(fp_line
		(start 5.75 -1.700001)
		(end 7.55 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f5ae904a-32f0-4b83-9acf-d0eda262e435")
	)
	(fp_line
		(start 6.8 -0.199999)
		(end 6.8 2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "630f1650-2cf4-4a68-9d21-c78aa4594173")
	)
	(fp_line
		(start 6.8 2.75)
		(end 2.5 2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "05d32641-a4ff-4d29-946c-e9b3858e775c")
	)
	(fp_line
		(start 7.55 -2.45)
		(end 5.75 -2.450001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0d5a3692-0fed-42e0-aa6b-99b490693bf2")
	)
	(fp_line
		(start 7.55 -1.7)
		(end 7.55 -2.45)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a8f332c9-d686-481a-8c78-e8486001f874")
	)
	(fp_line
		(start 7.55 -0.2)
		(end 6.8 -0.199999)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c3f1e336-709b-4dfd-b725-1c4583075838")
	)
	(fp_line
		(start 7.56 -2.46)
		(end -2.56 -2.46)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "24d6fa25-403e-4329-92ac-eb5590953b60")
	)
	(fp_line
		(start 7.56 3.51)
		(end 7.56 -2.46)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a570e1c7-b996-443b-8fc7-c7b90445afb3")
	)
	(fp_line
		(start -2.95 -2.85)
		(end -2.95 3.899999)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1aab436c-4897-4a63-9792-f9b2e904e06f")
	)
	(fp_line
		(start -2.95 3.899999)
		(end 7.949999 3.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "080a2adc-4aa0-4e5e-8ea3-9531a2ffecd4")
	)
	(fp_line
		(start 7.949999 3.9)
		(end 7.95 -2.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fba3d967-1930-4a43-b88b-ff4617822859")
	)
	(fp_line
		(start 7.95 -2.85)
		(end -2.95 -2.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "705c2dad-eb02-42fb-b83a-48f353696c70")
	)
	(fp_line
		(start -2.450001 -2.35)
		(end -2.450001 3.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0cfc3832-a950-4ef5-86de-94390d1a0c3b")
	)
	(fp_line
		(start -2.450001 3.4)
		(end 7.45 3.400001)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6c2ebd05-7404-45ca-8f9e-7aa1172a8dfc")
	)
	(fp_line
		(start -0.625 -2.35)
		(end 0 -1.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ac606257-9eae-48de-a14b-9a3676548d8d")
	)
	(fp_line
		(start 0 -1.35)
		(end 0.625 -2.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c26ea926-5999-472f-a818-14c28ae086be")
	)
	(fp_line
		(start 7.45 -2.349999)
		(end -2.450001 -2.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1e8f0eb3-93f5-4ba5-80af-e6a6fa657713")
	)
	(fp_line
		(start 7.45 3.400001)
		(end 7.45 -2.349999)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "55907357-fbc2-41b8-b767-586b0fe3c7f4")
	)
	(fp_text user "${REFERENCE}"
		(at 2.5 2.7 0)
		(layer "F.Fab")
		(uuid "2719e5e6-eceb-4522-8960-7d487ac19008")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -1.6 2)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(uuid "16f08dca-80ab-49c0-b4ce-1f961f09ab41")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.147059)
		(uuid "648751b0-9bb2-4db5-878e-3e73d43be9bc")
	)
	(pad "2" thru_hole oval
		(at 2.5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2aa3a561-e4ea-47dd-81ea-2f3b94a9156c")
	)
	(pad "3" thru_hole oval
		(at 5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "051a359f-8ec5-458e-bb2e-c25e136da3c3")
	)
	(model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B3B-XH-AM_1x03_P2.50mm_Vertical.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "/home/stefan/kicad/library/3dmodels/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)