(footprint "L_Abracon_ASPI-0630LR"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "smd shielded power inductor https://abracon.com/Magnetics/power/ASPI-0630LR.pdf")
	(tags "inductor abracon smd shielded")
	(property "Reference" "L3"
		(at 0 -4.25 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "3b1ab6b4-e09e-432f-8dc1-e8e529ac529a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "1.2uH"
		(at 0 4.25 180)
		(layer "F.Fab")
		(uuid "512a808f-4031-4ebb-8efb-1145a190f630")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Inductor_SMD:L_Abracon_ASPI-0630LR"
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "45bfd399-9a87-4701-bf84-f9460772c487")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
			(justify mirror)
		)
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "929280aa-7eb9-4aa3-b90b-968e987a390b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
			(justify mirror)
		)
	)
	(property "Description" "10A 1.2uH ±20%"
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "09737535-fcc0-4a95-b8fa-90c7b749a259")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
			(justify mirror)
		)
	)
	(property "LCSC" "C305187"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "04cc4b7d-06e3-42d8-bdc9-8a854c7ea10d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "TAI-TECH"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "4fd94d20-4ed2-4b73-ae55-2068cb9847b4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "TMPA0603S-1R2MN-D"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "65c988f7-bc82-4978-825d-1a6c46d7a621")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3.7 -3.4)
		(end 3.7 -3.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "53bfb81d-dc20-4d60-a19b-2a933a96be82")
	)
	(fp_line
		(start -3.7 -1.9)
		(end -3.7 -3.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9a26e3b1-2e91-42a6-bc3f-97c21c88629a")
	)
	(fp_line
		(start -3.7 1.9)
		(end -3.7 3.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c0f09c14-d39c-4367-bf6c-b875eb7104e4")
	)
	(fp_line
		(start 3.7 -1.9)
		(end 3.7 -3.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "47ebe134-2ba1-45d2-9800-09784e48337e")
	)
	(fp_line
		(start 3.7 1.9)
		(end 3.7 3.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "777e0b59-d95e-4944-a8d2-22087b868e26")
	)
	(fp_line
		(start 3.7 3.4)
		(end -3.7 3.4)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "961c10dd-f750-4187-991d-9f962d36e5e4")
	)
	(fp_line
		(start -4.35 1.45)
		(end -4.35 -1.45)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "bee49835-3b1a-4ed2-8439-3a43ac0d9dd6")
	)
	(fp_line
		(start -3.95 -1.85)
		(end -3.85 -1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fcea8842-b303-432c-9271-e2b30454f884")
	)
	(fp_line
		(start -3.85 -1.85)
		(end -3.85 -3.33)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d00d0c25-011e-44f0-9cb6-2f318b5fef9d")
	)
	(fp_line
		(start -3.85 1.85)
		(end -3.95 1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "596e7474-3cc2-4e80-9f8f-8d9b362beb4e")
	)
	(fp_line
		(start -3.85 3.33)
		(end -3.85 1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "404f0bf0-4736-44a4-853f-c72bcb075a94")
	)
	(fp_line
		(start -3.6 -3.58)
		(end 3.6 -3.58)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1749e493-de3b-4a9b-a094-3a241d388ecf")
	)
	(fp_line
		(start 3.6 3.58)
		(end -3.6 3.58)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "bd8ba27c-37f9-48de-a72d-aac4f5c2f929")
	)
	(fp_line
		(start 3.85 -3.33)
		(end 3.85 -1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "56117c15-7a24-4885-a0d6-c5117d258b19")
	)
	(fp_line
		(start 3.85 -1.85)
		(end 3.95 -1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7fe9dba9-e0e2-4f82-8d8a-6cf338f0f9e8")
	)
	(fp_line
		(start 3.85 1.85)
		(end 3.85 3.33)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "efa83a1e-7808-4d33-9538-a74df4ce5306")
	)
	(fp_line
		(start 3.95 1.85)
		(end 3.85 1.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9fd381d4-8873-4548-9dc7-0e48349945bd")
	)
	(fp_line
		(start 4.35 -1.45)
		(end 4.35 1.45)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "93ab5d0c-c389-49d2-a60a-e1d2674a9ccc")
	)
	(fp_arc
		(start -4.35 -1.45)
		(mid -4.232843 -1.732843)
		(end -3.95 -1.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "74008e98-0876-4e8b-a27b-1a18a2e9d551")
	)
	(fp_arc
		(start -3.95 1.85)
		(mid -4.232843 1.732843)
		(end -4.35 1.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "47c9594c-64d8-479e-81cf-3f905d0af400")
	)
	(fp_arc
		(start -3.85 -3.33)
		(mid -3.776777 -3.506777)
		(end -3.6 -3.58)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e88c96b5-cd6b-4e3c-9a79-5409ee3e8872")
	)
	(fp_arc
		(start -3.6 3.58)
		(mid -3.776777 3.506777)
		(end -3.85 3.33)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6b6ffbfe-7c44-4167-866f-9f6cb7db636f")
	)
	(fp_arc
		(start 3.6 -3.58)
		(mid 3.776777 -3.506777)
		(end 3.85 -3.33)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ec550061-f981-4553-aa5f-9b69b75568c2")
	)
	(fp_arc
		(start 3.85 3.33)
		(mid 3.776777 3.506777)
		(end 3.6 3.58)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "99edbd37-25ed-4ff0-aee7-cb5edee9c02e")
	)
	(fp_arc
		(start 3.95 -1.85)
		(mid 4.232843 -1.732843)
		(end 4.35 -1.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6ec6dbc2-6d40-44b6-a110-3e77a9f92e9f")
	)
	(fp_arc
		(start 4.35 1.45)
		(mid 4.232843 1.732843)
		(end 3.95 1.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "94701da1-f51d-4344-8346-734f57e121de")
	)
	(fp_line
		(start -3.599999 -3.325)
		(end -3.599999 3.325)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "89117620-9385-4a4b-89b5-a6a84b779627")
	)
	(fp_line
		(start -3.599999 3.325)
		(end 3.599999 3.325)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "79074f9a-b13e-4c1a-a67f-48842075b62b")
	)
	(fp_line
		(start 3.599999 -3.325)
		(end -3.599999 -3.325)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f42d2911-0e96-4833-9daa-157a2b755af5")
	)
	(fp_line
		(start 3.599999 3.325)
		(end 3.599999 -3.325)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d3403647-0f51-4dc4-b5d8-c1c58186fdd5")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "a08f5fa2-9f5d-4618-986a-070ed59896ef")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.025 0)
		(size 2.35 3.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "00ca74c5-70a7-4083-85b3-22235f842811")
	)
	(pad "2" smd roundrect
		(at 3.025 0)
		(size 2.35 3.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f68060dd-d777-4a6e-bf32-79299761fd4a")
	)
	(model ":KICAD7_3DMODEL_DIR:Inductor_SMD.3dshapes/Inductor_GCDA0630.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 -90)
		)
	)
)
