(footprint "M.2 Nut M2.5 x 0.9" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Field2" "")
  (property "Sheetfile" "M.2 B and E.kicad_sch")
  (property "Sheetname" "M.2 B and E")
  (property "exclude_from_bom" "")
  (attr smd exclude_from_bom)
  (fp_text reference "H21" (at 0 -7.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 49a19617-3c55-4896-87c1-4d9725028d76)
  )
  (fp_text value "MOUNT_HOLE" (at 0 -6 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 60d711c8-d330-45b3-bc72-a7f5dea03d81)
  )
  (fp_text user "${REFERENCE}" (at 0 -4.5 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 33a16f17-3e2c-4a0a-ae30-a61a932fb507)
  )
  (fp_arc (start -2.533845 0.788749) (mid -2.653741 -0.012456) (end -2.526329 -0.8125)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp e298a816-5e64-42e0-afea-1c0d3ca700b7))
  (fp_arc (start -1.95 -1.8) (mid -1.316084 -2.304435) (end -0.559519 -2.594115)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 689afccf-e116-4f16-8d2d-4086bfd61cfd))
  (fp_arc (start -0.583845 2.588749) (mid -1.337657 2.291979) (end -1.96681 1.781615)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 620f2005-c673-4087-9ab6-a924c23fbcc5))
  (fp_arc (start 0.583845 -2.588749) (mid 1.337657 -2.291979) (end 1.96681 -1.781615)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp f93cfe40-6614-4b93-b2bd-16324119e4dd))
  (fp_arc (start 1.95 1.8) (mid 1.316085 2.304437) (end 0.559519 2.594115)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp b08cad57-c768-4505-bbca-af4d3bb5f650))
  (fp_arc (start 2.533845 -0.788749) (mid 2.65374 0.012456) (end 2.526329 0.8125)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 2e9ad89b-819d-4ed1-a19b-768a9f516905))
  (pad "1" thru_hole circle (at 0 0) (size 4.55 4.55) (drill 4.25) (layers "*.Cu" "B.Mask")
    (zone_connect 2) (tstamp 00f82ad0-bdad-4f54-a195-12063e3947df))
  (pad "1" smd circle (at 0 0) (size 6.2 6.2) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp 159acbe6-edc2-406c-a577-5384ddef5138))
  (model ":KICAD7_3DMODEL_DIR:Hardware.3dshapes/M.2 SMD Nut 0.9mm.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
