(footprint "Raspberry Pi 5 Plug-In"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "A1"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "05a3120c-084e-4588-8362-3cc370920994")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Pluggable_Assembly"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "67103e07-bb68-47c5-97c9-5e6521594db5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Module:Raspberry Pi 5 Plug-In"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bf2c3381-f544-4ec3-8321-e4df6cf42903")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "eb7dfb87-3c72-4c1a-9c8e-a8f7be3947fe")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f54f9c0c-a207-428a-8f7d-a9c81beb0765")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr exclude_from_bom)
	(fp_line
		(start -35.4 24.5)
		(end 15.4 24.5)
		(stroke
			(width 0.05)
			(type dash)
		)
		(layer "F.Fab")
		(uuid "5094459f-31a8-4f0c-8d33-334ebc0252ce")
	)
	(fp_line
		(start -10 27)
		(end -10 22)
		(stroke
			(width 0.05)
			(type dash)
		)
		(layer "F.Fab")
		(uuid "c1fcfdcd-cd10-4984-93c4-79fb65112444")
	)
	(fp_line
		(start 16.5 -18.5)
		(end 21.5 -18.5)
		(stroke
			(width 0.05)
			(type dash)
		)
		(layer "F.Fab")
		(uuid "2909a64f-6873-4166-a09a-2c9a22a9693f")
	)
	(fp_line
		(start 19 -21)
		(end 19 -16)
		(stroke
			(width 0.05)
			(type dash)
		)
		(layer "F.Fab")
		(uuid "18027636-a42b-4165-aae5-f98a0b83e6ff")
	)
	(fp_line
		(start 24 -28)
		(end 24 -9.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "703558cb-98af-4a30-b8fe-e7f2eacd1138")
	)
	(fp_line
		(start 24 -9.5)
		(end 28 -9.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "91bafd74-1ede-41ff-a8cb-59c549c4312e")
	)
	(fp_line
		(start 28 -9.5)
		(end 28 28)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "f87d6641-690b-40df-b14c-a92747ef2f75")
	)
	(fp_rect
		(start -42.5 -28)
		(end 42.5 28)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "fc810bc2-ebff-4a7f-a36c-d54c3898e733")
	)
	(fp_circle
		(center -39 -24.5)
		(end -37.65 -24.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "f919301f-899b-490b-b85f-868f8f3aaa30")
	)
	(fp_circle
		(center -39 24.5)
		(end -37.65 24.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "eb5dc802-e8c3-4c69-84cf-0fd66324e77f")
	)
	(fp_circle
		(center 19 -24.5)
		(end 20.35 -24.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "dff00fda-3449-474e-af10-e3c7044331fc")
	)
	(fp_circle
		(center 19 24.5)
		(end 20.35 24.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "68fc21cb-a54d-4ba9-99f8-e7ca62b81ba3")
	)
	(fp_text user "M2.5 / 10.5-11mm spacer"
		(at -42 -26 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "051e1cab-2ea5-4f59-b7fc-7598717d7ac1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left bottom)
		)
	)
	(fp_text user "Ethernet Jack"
		(at 25.893417 -10.310083 90)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "5b3ad8b4-112e-486c-958f-d1e41e335734")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left bottom)
		)
	)
	(fp_text user "GPIO header"
		(at -35.904203 26.107703 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "91ebd562-f6e7-470a-9cc2-319d89a595fc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left bottom)
		)
	)
	(fp_text user "POE header"
		(at 17 -18 -90)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "944dbde2-7333-4c08-8d55-0c9571d0013b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left bottom)
		)
	)
	(fp_text user "1"
		(at -35.4 24.2 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "98f96bc0-56aa-4e69-acba-abbe571c9909")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.1)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c5874eeb-6f8c-4685-bc7d-13cb84342659")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(model "/home/stefan/kicad/library/3dmodels/Module.3dshapes/RaspberryPi5.step"
		(offset
			(xyz 0 0 11.1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)