(footprint "JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "JST XH series connector, B2B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST XH vertical boss")
	(property "Reference" "J14"
		(at 1.25 -3.550001 180)
		(layer "F.SilkS")
		(uuid "c6845548-c10e-4f39-a33e-c5d9bccfac35")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "UP"
		(at 2.25 4.6 180)
		(layer "F.Fab")
		(uuid "1fece7bb-bf5b-446b-aee0-57ed699c5159")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_JST:JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "acbbae99-a024-496b-88ce-bd3da80aefd4")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c547d0e6-b3e1-412f-915b-5a3b8b17d51a")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" "Generic connector, single row, 01x02, script generated"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1e5cc7df-274f-4360-85c8-62a2e5af1bce")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "MFG" "JST"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "514a78e7-e6ca-49d3-8767-c0d04516f9d5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4862a7be-c575-4b1c-9948-969533fa5243")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d330b856-eb86-4de9-8b1c-0f78f634abec")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -2.85 -2.75)
		(end -2.85 -1.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ba107a28-d032-4c80-9c7e-53b3126aa4fa")
	)
	(fp_line
		(start -2.56 -2.46)
		(end -2.56 3.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f8ce65ea-e98e-47fb-bc94-ac9612c9e98c")
	)
	(fp_line
		(start -2.56 3.51)
		(end 5.06 3.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6d20221b-0442-4b38-8940-ba039a559999")
	)
	(fp_line
		(start -2.55 -2.45)
		(end -2.55 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "23d63a8e-5f18-40e7-9532-8c7c92029fcb")
	)
	(fp_line
		(start -2.55 -1.7)
		(end -0.750001 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1ad3ad37-7cff-499e-b0cd-b12f0d3ee242")
	)
	(fp_line
		(start -2.55 -0.2)
		(end -1.8 -0.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "78beced6-a5aa-4524-98f9-74d94b5b0a85")
	)
	(fp_line
		(start -1.8 -0.2)
		(end -1.8 1.14)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ec724969-b386-4170-b82e-5d3e0dbbd5fd")
	)
	(fp_line
		(start -1.6 -2.75)
		(end -2.85 -2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "af04e61c-297b-43d6-8533-2f629634b142")
	)
	(fp_line
		(start -0.750001 -1.7)
		(end -0.75 -2.450001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e2a73330-25ee-4430-8265-a21609c1ed6a")
	)
	(fp_line
		(start -0.75 -2.450001)
		(end -2.55 -2.45)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b1d53797-dbcc-4789-8b44-d8a8f27fa98d")
	)
	(fp_line
		(start 0.75 -2.450001)
		(end 0.750001 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "733e9bb3-cd3f-48e2-80a3-f59039391b13")
	)
	(fp_line
		(start 0.750001 -1.7)
		(end 1.749999 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "96390e81-3072-48a8-ab99-2cd9d9232383")
	)
	(fp_line
		(start 1.25 2.75)
		(end -0.74 2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "725b878d-9ab7-40a6-93ac-711896ce9aa1")
	)
	(fp_line
		(start 1.749999 -2.45)
		(end 0.75 -2.450001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0a4041e6-7191-48db-a99b-c8bfaf2979bd")
	)
	(fp_line
		(start 1.749999 -1.7)
		(end 1.749999 -2.45)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b49ececc-a1ae-4d4d-a9d7-7ef2d09b4458")
	)
	(fp_line
		(start 3.25 -2.450001)
		(end 3.250001 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3ae9737d-fb4a-495c-b5f3-d8c228ad1c20")
	)
	(fp_line
		(start 3.250001 -1.7)
		(end 5.05 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "57907ca6-85ae-41b1-a8bb-bd81dd713543")
	)
	(fp_line
		(start 4.3 -0.2)
		(end 4.3 2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a5a48a98-1002-4875-8b47-0b8766b628dc")
	)
	(fp_line
		(start 4.3 2.75)
		(end 1.25 2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9b5d224d-84fe-48d4-b76a-5be9c87d3fa8")
	)
	(fp_line
		(start 5.05 -2.45)
		(end 3.25 -2.450001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "21ddb5eb-c368-4a46-86c8-53d63b3b0f1a")
	)
	(fp_line
		(start 5.05 -1.7)
		(end 5.05 -2.45)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ab651119-ad03-411d-b592-533a2c432452")
	)
	(fp_line
		(start 5.05 -0.2)
		(end 4.3 -0.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "92bf160a-b3cb-45df-bae5-e81314c9287e")
	)
	(fp_line
		(start 5.06 -2.46)
		(end -2.56 -2.46)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9f0d3c47-79ac-42a2-90ea-6135e9246532")
	)
	(fp_line
		(start 5.06 3.51)
		(end 5.06 -2.46)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d9fe9442-3428-48d1-8ea9-a2cf3bd397d8")
	)
	(fp_line
		(start -2.95 -2.85)
		(end -2.95 3.899999)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b43af90b-9273-4cde-b06d-42a0fb9acbcf")
	)
	(fp_line
		(start -2.95 3.899999)
		(end 5.45 3.899999)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "0b917bcb-22ac-40aa-8fc2-f140cd16ec7c")
	)
	(fp_line
		(start 5.45 -2.85)
		(end -2.95 -2.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "aeed9dfe-6ff7-46bb-981a-6fa479f56b92")
	)
	(fp_line
		(start 5.45 3.899999)
		(end 5.45 -2.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f3a66a0e-d785-44a0-a314-75e002395ee6")
	)
	(fp_line
		(start -2.450001 -2.35)
		(end -2.450001 3.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4007212c-afbe-498d-9a74-73f0143088bc")
	)
	(fp_line
		(start -2.450001 3.4)
		(end 4.950001 3.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5b5339bb-becd-4131-b636-e42f0c91f263")
	)
	(fp_line
		(start -0.625 -2.35)
		(end 0 -1.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "17ae779b-3a9c-4d7c-b2c4-e239bae259db")
	)
	(fp_line
		(start 0 -1.35)
		(end 0.625 -2.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2c43884c-0560-42de-a610-42002e5dd4d2")
	)
	(fp_line
		(start 4.950001 -2.35)
		(end -2.450001 -2.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f526d5fa-ee7e-4b16-8d3a-5740daab237a")
	)
	(fp_line
		(start 4.950001 3.4)
		(end 4.950001 -2.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "82cdb51c-290f-439b-a7fd-cab57e55cf1c")
	)
	(fp_text user "${REFERENCE}"
		(at 1.25 2.7 180)
		(layer "F.Fab")
		(uuid "867c7aa0-c10c-44af-a9df-9824692ecda0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -1.6 2)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(uuid "56856305-6f33-4ef8-82c4-a4099f18f8fb")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.7 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.147059)
		(uuid "feaf68e3-6bd4-4067-83ec-2e15e1c0484d")
	)
	(pad "2" thru_hole oval
		(at 2.5 0)
		(size 1.7 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3c1e4c34-94b9-4f3c-a14a-015d119708e2")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)