(footprint "6P_2x1.25_P1.5"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "J3"
		(at 0 -4.95 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "625001ec-16d4-4cd0-b1eb-2e175fdde6ca")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SWD"
		(at 2.375 0 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "75bffcbd-9212-417f-8feb-2ca70bdd04f1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6268d0a2-2486-4303-8505-2e9761255228")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a482082f-e218-4aa5-86d0-fdca49c29d07")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3ec425fa-84fc-45cb-a3bf-e772e951824c")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr through_hole exclude_from_pos_files exclude_from_bom)
	(fp_poly
		(pts
			(xy -1.15 -3.75) (xy -1.4 -3.55) (xy -1.4 -3.95)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "d5e9a0fb-4f60-46c2-9f5a-7907c4228b78")
	)
	(fp_line
		(start -1.15 4.2)
		(end -1.15 -4.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b2217d0f-4309-4445-9ba6-9485f7983ebd")
	)
	(fp_line
		(start -0.825 -4.525)
		(end 0.825 -4.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1ed39ce7-4bc2-4252-8ef9-28cbe5b048e7")
	)
	(fp_line
		(start 0.825 4.525)
		(end -0.825 4.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5d18009c-b02b-4561-add8-cf32d95c5a13")
	)
	(fp_line
		(start 1.15 -4.2)
		(end 1.15 4.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3d39a86e-1cf3-49a5-a71b-55f1a3410076")
	)
	(fp_arc
		(start -1.15 -4.2)
		(mid -1.05481 -4.42981)
		(end -0.825 -4.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d908f5bd-b49e-42c2-a0f9-6bd1e6f0db1f")
	)
	(fp_arc
		(start -0.825 4.525)
		(mid -1.05481 4.42981)
		(end -1.15 4.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5ca44bff-f9ec-4b65-b630-f02103a7efc7")
	)
	(fp_arc
		(start 0.825 -4.525)
		(mid 1.05481 -4.42981)
		(end 1.15 -4.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5312ecc0-df25-44bc-92b3-13360e55cebc")
	)
	(fp_arc
		(start 1.15 4.2)
		(mid 1.05481 4.42981)
		(end 0.825 4.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "423625ec-c785-4633-94f0-cedc3610bb95")
	)
	(fp_text user "${REF}"
		(at -1.9 0 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "dca89be9-55be-4fe8-88ee-e92cc44329da")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" connect roundrect
		(at 0 -3.75)
		(size 2 1.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.143)
		(uuid "d013dd43-3dbe-4e40-9269-a0e03b3e87b5")
	)
	(pad "2" connect roundrect
		(at 0 -2.25)
		(size 2 1.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.143)
		(uuid "a73a1b5f-8cf2-43a7-bfb7-76c581924d9e")
	)
	(pad "3" connect roundrect
		(at 0 -0.75)
		(size 2 1.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.143)
		(uuid "c2fd6b28-e081-476b-a4ac-464cf29216b4")
	)
	(pad "4" connect roundrect
		(at 0 0.75)
		(size 2 1.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.143)
		(uuid "33c596c8-232a-4153-9e90-c7d254ebc427")
	)
	(pad "5" connect roundrect
		(at 0 2.25)
		(size 2 1.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.143)
		(uuid "c0d8931d-c069-4aa4-a61a-a1b4d3f0d7e8")
	)
	(pad "6" connect roundrect
		(at 0 3.75)
		(size 2 1.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.143)
		(uuid "0110d3d3-d46e-4ccb-87c7-9ad40e7f403e")
	)
)