(footprint "DFN-6-1EP_1.2x1.2mm_P0.4mm_EP0.3x0.94mm_PullBack"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "DFN, 6 Pin (http://www.onsemi.com/pub/Collateral/NCP133-D.PDF), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "DFN NoLead")
	(property "Reference" "U16"
		(at 0 -1.550001 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "b8e43196-1e0e-408c-9dd7-7faa44dd4a8c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "NCP176"
		(at 0 1.550001 180)
		(layer "F.Fab")
		(uuid "48656ff6-c985-483b-ba86-a85fe272efb8")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.0625)
			)
		)
	)
	(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_1.2x1.2mm_P0.4mm_EP0.3x0.94mm_PullBack"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "96ac79e6-97fb-4e02-972b-f65405d86614")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "23da4ba8-1d67-40d5-82d4-0e66845abe63")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "21918ef6-c866-41df-a612-92577c9fa402")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "LCSC" "C233363"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "abc6ba7e-6272-4ef7-a219-2afa202dc1fd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "onsemi"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "2748d6ff-9cd2-4eaa-a3ba-728d584e5f1a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "NCP176AMX330TCG"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "41b7776c-4252-49fc-8433-d7e6f2cd209e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Preferred" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "dda9c8b5-c7bd-453d-b175-df028ebf2581")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3b17cf58-cdfb-41ed-b7a4-7916656035e4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.6 0.71)
		(end 0.6 0.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "33eddf9f-8ba1-4468-baa6-3bdc0bc1e84a")
	)
	(fp_line
		(start 0 -0.71)
		(end 0.6 -0.71)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "77fe7c17-9239-4735-92af-e02c0aa66f84")
	)
	(fp_line
		(start -0.85 -0.6)
		(end -0.85 0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "609fed7e-5835-4515-af33-5db75672eccd")
	)
	(fp_line
		(start 0.6 -0.85)
		(end -0.6 -0.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "892a6181-ad43-48a7-bfca-8588c17b348b")
	)
	(fp_line
		(start 0.6 0.85)
		(end -0.6 0.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0b74c95e-e08a-41b1-81cc-7a40f22a37a2")
	)
	(fp_line
		(start 0.85 -0.6)
		(end 0.85 0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4a650711-10d8-4ea9-b970-0cbd280d8611")
	)
	(fp_arc
		(start -0.85 -0.6)
		(mid -0.776777 -0.776777)
		(end -0.6 -0.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "055160fb-6c1c-492c-b017-126cde3f6c0f")
	)
	(fp_arc
		(start -0.6 0.85)
		(mid -0.776777 0.776777)
		(end -0.85 0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d9c0ed66-01a0-4a5d-94dd-461d9d5f4670")
	)
	(fp_arc
		(start 0.6 -0.85)
		(mid 0.776777 -0.776777)
		(end 0.85 -0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "53ae4261-d0ef-4ce9-b839-a6f1c7adb30d")
	)
	(fp_arc
		(start 0.85 0.6)
		(mid 0.776777 0.776777)
		(end 0.6 0.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7e47ed8f-6b71-4383-a047-e3a0d2411333")
	)
	(fp_line
		(start -0.6 -0.6)
		(end 0.6 -0.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d07873d1-8eed-4d90-bfb8-6a9efc16567f")
	)
	(fp_line
		(start -0.6 -0.3)
		(end -0.3 -0.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e5a8e3c0-fb08-4f1e-a8ce-67f589b58fc0")
	)
	(fp_line
		(start -0.6 0.6)
		(end -0.6 -0.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1615c91f-4c0e-45d2-82cc-266a423aa728")
	)
	(fp_line
		(start 0.6 -0.6)
		(end 0.6 0.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6d397a7e-ac9b-42b9-9329-95eff4679b55")
	)
	(fp_line
		(start 0.6 0.6)
		(end -0.6 0.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "03106e02-f019-47ea-a5db-40d50230dd13")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "c3da80f0-6ebd-4c45-a07b-044d9b96807b")
		(effects
			(font
				(size 0.3 0.3)
				(thickness 0.04)
			)
		)
	)
	(pad "" smd oval
		(at -0.525 -0.4)
		(size 0.3 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "3748d663-2236-46af-9651-dc60cd928e3d")
	)
	(pad "" smd oval
		(at -0.525 0)
		(size 0.3 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "d9a29d1c-c5c1-4220-a163-60dc30edf337")
	)
	(pad "" smd oval
		(at -0.525 0.4)
		(size 0.3 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f6714451-dd09-4601-b4e3-611813458039")
	)
	(pad "" smd roundrect
		(at 0 -0.3)
		(size 0.3 0.45)
		(layers "F.Paste")
		(roundrect_rratio 0.5)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "36d0397a-b65c-4106-aaf3-64d5e2c9af76")
	)
	(pad "" smd roundrect
		(at 0 0.3)
		(size 0.3 0.45)
		(layers "F.Paste")
		(roundrect_rratio 0.5)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8f78359e-60b3-4593-9b8f-c8a1b80c41bf")
	)
	(pad "" smd oval
		(at 0.525 -0.4)
		(size 0.3 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "6dec98ee-88c1-4870-a256-26f40c6abb17")
	)
	(pad "" smd oval
		(at 0.525 0)
		(size 0.3 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ef5cc4a1-ea0d-42b4-bc9e-a07f542e9441")
	)
	(pad "" smd oval
		(at 0.525 0.4)
		(size 0.3 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0e627052-eb5d-4fc8-ad46-536fd76b9b56")
	)
	(pad "1" smd roundrect
		(at -0.525 -0.4)
		(size 0.37 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2083333333)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "724a44a5-6168-47bf-9eb4-d9b4088b9455")
	)
	(pad "2" smd roundrect
		(at -0.525 0)
		(size 0.37 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2083333333)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "15cb4dba-2fe4-4e53-ae6f-89d53860a958")
	)
	(pad "3" smd roundrect
		(at -0.525 0.4)
		(size 0.37 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2083333333)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4498cfaa-d7a4-403c-acbf-dbef09f3e7c8")
	)
	(pad "4" smd roundrect
		(at 0.525 0.4)
		(size 0.37 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2083333333)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1970113e-91e1-4dc2-9f5f-1e0354a7e2cf")
	)
	(pad "5" smd roundrect
		(at 0.525 0)
		(size 0.37 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2083333333)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9fb704ab-e7dc-4739-a9ce-e784770301ca")
	)
	(pad "6" smd roundrect
		(at 0.525 -0.4)
		(size 0.37 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2083333333)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "612d2cce-c4ce-4b0f-a657-b4016cf7d38c")
	)
	(pad "7" smd roundrect
		(at 0 0)
		(size 0.4 1.18)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.125)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a0d52c8f-d817-4708-ab00-e23246a368a8")
	)
	(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-6-1EP_1.2x1.2mm_P0.4mm_EP0.3x0.94mm_PullBack.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-6-1EP_1.2x1.2mm_P0.4mm_EP0.3x0.94mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)