(footprint "Texas_DSBGA-8_0.9x1.9mm_Layout2x4_P0.5mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Texas Instruments, DSBGA, 0.9x1.9mm, 8 bump 2x4 (perimeter) array, NSMD pad definition (http://www.ti.com/lit/ds/symlink/txb0102.pdf, http://www.ti.com/lit/an/snva009ag/snva009ag.pdf)")
	(tags "Texas Instruments DSBGA BGA YZP R-XBGA-N8")
	(property "Reference" "U8"
		(at 0 -2.000001 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "8319c5d5-4429-4625-9fa3-1550d4a1980d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SN74LVC2G66YZP"
		(at 0 2.000001 180)
		(layer "F.Fab")
		(uuid "1261f9ab-7634-48cb-b29e-2ad7e50ef09b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Package_BGA:Texas_DSBGA-8_0.9x1.9mm_Layout2x4_P0.5mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9af007aa-6cf8-4929-8c9e-7cbb10f558f6")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "530543cc-77ab-42f3-8f41-6d39de38ed84")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7224aba0-63d1-411b-8974-b9cb081df786")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "LCSC" "C2865655"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "8324eb5d-6d91-4761-a6d6-fc95cc779d79")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "TI"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "0ea838b0-bd33-4bf4-a757-69655511ce2d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "SN74LVC2G66YZPR"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "873e2acd-23cf-4601-9e0e-ff4480102414")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7e20123c-c835-4838-85fa-5355b1f3b338")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.05)
	(attr smd)
	(fp_line
		(start -0.55 -0.7)
		(end -0.55 1.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f0a284d3-1320-42d2-973e-4b11a23b97c5")
	)
	(fp_line
		(start -0.55 1.05)
		(end 0.55 1.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ee8869eb-94ad-4ba4-9b7b-c345ef35c436")
	)
	(fp_line
		(start 0.55 -1.05)
		(end -0.199999 -1.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "64393aad-b24f-4650-9c89-718f8eb7e8a2")
	)
	(fp_line
		(start 0.55 -1.05)
		(end 0.55 1.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6b89a4f8-dec1-467a-adf3-e2a075cfc70c")
	)
	(fp_line
		(start -0.725 0.975001)
		(end -0.725 -0.975001)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a344c35c-771e-4aca-b99e-05fd9d241a5c")
	)
	(fp_line
		(start -0.475 -1.225)
		(end 0.475 -1.225)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3fc9a99c-344e-4a8c-a479-98996ce55106")
	)
	(fp_line
		(start 0.475 1.225)
		(end -0.475 1.225)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "fd2d20fc-8e1e-4c86-8b1c-f6072ca6dafb")
	)
	(fp_line
		(start 0.725 -0.975001)
		(end 0.725 0.975001)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7f9fbbad-3a58-4155-a02b-7e2e483bdf37")
	)
	(fp_arc
		(start -0.725 -0.975001)
		(mid -0.651777 -1.151777)
		(end -0.475 -1.225)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4923d0b3-e620-4443-baeb-b0031d6d6ab8")
	)
	(fp_arc
		(start -0.475 1.225)
		(mid -0.651777 1.151777)
		(end -0.725 0.975001)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "58724e5a-d46e-49da-80c3-291e24ecbdbf")
	)
	(fp_arc
		(start 0.475 -1.225)
		(mid 0.651776 -1.151777)
		(end 0.725 -0.975001)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "fc1fbcfb-913b-4c09-aefb-4ee7cb998bed")
	)
	(fp_arc
		(start 0.725 0.975001)
		(mid 0.651776 1.151777)
		(end 0.475 1.225)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8a53685f-ab10-40e8-a585-491cb009b15b")
	)
	(fp_line
		(start -0.47 -0.97)
		(end -0.47 0.97)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e808df03-ed12-4a0b-96ee-07b4336b3267")
	)
	(fp_line
		(start -0.47 -0.8)
		(end -0.3 -0.970001)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "39db4320-a05a-48fa-ac9d-6c37de713975")
	)
	(fp_line
		(start -0.47 0.97)
		(end 0.47 0.97)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4b292343-5d96-4283-9a15-b1bdae331754")
	)
	(fp_line
		(start 0.47 -0.97)
		(end -0.47 -0.97)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "631b592b-02a5-49a0-90be-5677a5b9bff6")
	)
	(fp_line
		(start 0.47 0.97)
		(end 0.47 -0.97)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "11490feb-ab4c-4907-b338-06df5b64fabe")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 -90)
		(layer "F.Fab")
		(uuid "618bf26e-5750-4e9f-b582-a0dd7c535a75")
		(effects
			(font
				(size 0.4 0.4)
				(thickness 0.05)
			)
		)
	)
	(pad "" smd roundrect
		(at -0.25 -0.75)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "56da5cec-9f50-4a64-b469-038243ae0fb8")
	)
	(pad "" smd roundrect
		(at -0.25 -0.25)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "6a888845-aef4-4dce-aede-1dd214f4fa79")
	)
	(pad "" smd roundrect
		(at -0.25 0.25)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "fa02a8d6-0f91-4657-9b96-d34ef8d5c69e")
	)
	(pad "" smd roundrect
		(at -0.25 0.75)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "98c3075f-ce39-43a5-8204-a80bb3cd0704")
	)
	(pad "" smd roundrect
		(at 0.25 -0.75)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c621f9d7-c803-43ec-9838-9b5e6c57f67c")
	)
	(pad "" smd roundrect
		(at 0.25 -0.25)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c23b84d5-d14d-4f61-b810-37b92e81ad07")
	)
	(pad "" smd roundrect
		(at 0.25 0.25)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e284bcd5-4340-45ad-972e-73cc0aa293e8")
	)
	(pad "" smd roundrect
		(at 0.25 0.75)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "630047d4-7cc8-4e39-a5b7-6425e30c661b")
	)
	(pad "A1" smd circle
		(at -0.25 -0.75)
		(size 0.265 0.265)
		(layers "F.Cu" "F.Mask")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "287c8e6f-03de-4dbd-a15f-516ab783b23d")
	)
	(pad "A2" smd circle
		(at 0.25 -0.75)
		(size 0.265 0.265)
		(layers "F.Cu" "F.Mask")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "17b189ac-d8e2-4784-a9a4-295a12e1df12")
	)
	(pad "B1" smd circle
		(at -0.25 -0.25)
		(size 0.265 0.265)
		(layers "F.Cu" "F.Mask")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b4d6ff4a-9fbd-40ca-a6e1-afd66ba03f9b")
	)
	(pad "B2" smd circle
		(at 0.25 -0.25)
		(size 0.265 0.265)
		(layers "F.Cu" "F.Mask")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "cf773109-ef48-4dfa-a04f-d48e6ff66dce")
	)
	(pad "C1" smd circle
		(at -0.25 0.25)
		(size 0.265 0.265)
		(layers "F.Cu" "F.Mask")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0e876df8-aa48-4b7f-8dec-53e5848ed8b3")
	)
	(pad "C2" smd circle
		(at 0.25 0.25)
		(size 0.265 0.265)
		(layers "F.Cu" "F.Mask")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2da19f89-3799-4611-ac21-9aec6aafb88c")
	)
	(pad "D1" smd circle
		(at -0.25 0.75)
		(size 0.265 0.265)
		(layers "F.Cu" "F.Mask")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "6826b9b3-dc57-4f3a-8be4-888e2a996621")
	)
	(pad "D2" smd circle
		(at 0.25 0.75)
		(size 0.265 0.265)
		(layers "F.Cu" "F.Mask")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "87bf93dc-33cb-4503-84a2-258dcb4d41fb")
	)
	(model "${KICAD6_3DMODEL_DIR}/Package_BGA.3dshapes/Texas_DSBGA-8_0.9x1.9mm_Layout2x4_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)