(footprint "MR60PB-M"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -5.15 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "8d17cddf-22b7-43de-85b7-af5550eafc9b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "MR60PB-M"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "4f02c2bd-8b18-49cb-b421-364c2a6a96d7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ab4adc08-6054-48aa-bb8e-a9703b473f76")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "001a2bfb-824f-4f80-a6f9-e0faf98adb7e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "60e216ab-146b-4db7-ba17-2a6634f786db")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -5.5 4.85)
		(end 5.5 4.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ffc10ae8-2b8c-4ccc-9a23-d47d356a29c5")
	)
	(fp_line
		(start 5.5 -4.85)
		(end -5.5 -4.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4dd8a1e1-1aba-4442-9e3a-1f0b031f2283")
	)
	(fp_arc
		(start -5.5 4.85)
		(mid -10.35 0)
		(end -5.5 -4.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bb5ecde3-7397-4fad-8804-29eea2e62d25")
	)
	(fp_arc
		(start 5.5 -4.85)
		(mid 10.35 0)
		(end 5.5 4.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "43be5a6b-5909-463e-837e-b350c6ebeec1")
	)
	(fp_line
		(start -5.5 4.6)
		(end 5.5 4.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "44e29c90-adfc-4891-91ea-cbed84b7f1a5")
	)
	(fp_line
		(start 5.5 -4.6)
		(end -5.5 -4.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "2645eeea-46b0-46e8-9a48-7d6777f30643")
	)
	(fp_arc
		(start -5.5 4.6)
		(mid -10.1 0)
		(end -5.5 -4.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "7d3ac456-141c-4512-889f-6a7c4d869d6d")
	)
	(fp_arc
		(start 5.5 -4.6)
		(mid 10.1 0)
		(end 5.5 4.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "9cf6f76a-3940-4dbb-8789-e4146e33a753")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "e6a6b1b2-d574-4fa7-a179-9a6d97c8e48e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" connect roundrect
		(at -5.55 0)
		(size 4.9 4.9)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.1020408163)
		(uuid "acef6661-e3e3-40c6-ad14-2f546deeafad")
	)
	(pad "1" thru_hole circle
		(at -5.5 0)
		(size 3.7 3.7)
		(drill 3.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fbc0e636-c132-49ff-9373-06c8657fa45d")
	)
	(pad "2" connect roundrect
		(at -0.05 0)
		(size 4.9 4.9)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.2)
		(uuid "4ba70533-c4b6-4099-baad-ed9149ff15f2")
	)
	(pad "2" thru_hole circle
		(at 0 0)
		(size 3.7 3.7)
		(drill 3.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4b50a124-1949-45b9-a5d1-00452ae0defb")
	)
	(pad "3" connect roundrect
		(at 5.45 0)
		(size 4.9 4.9)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.2)
		(uuid "6be6b4aa-de5b-450d-8c9f-f151682809b5")
	)
	(pad "3" thru_hole circle
		(at 5.5 0)
		(size 3.7 3.7)
		(drill 3.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c4d36252-6828-4129-93c2-99dd8c451d73")
	)
	(model "${KICAD6_3DMODEL_DIR}/Connector_AMASS.3dshapes/User Library-MR60PB-M.STEP"
		(offset
			(xyz 0 0 2.2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
