(module 1P_Castellated_HC (layer F.Cu) (tedit 5BEB1FFE)
  (fp_text reference J4 (at 0 6.3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Conn_01x01_Female (at -0.05 7.95) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.05)))
  )
  (pad 1 thru_hole oval (at 0 1) (size 5.4 7.4) (drill oval 4 6) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.3 0.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.3 1.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 2.3 0.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 2.3 1.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.3 2) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 2.3 2) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.2 2.7) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 2.2 2.7) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 1.9 3.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -1.9 3.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -1.4 3.8) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 1.4 3.8) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -0.7 4.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0.7 4.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0 4.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu *.Mask))
)
