(footprint "UDFN-9_1.0x3.8mm_P0.5mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "9-pin UDFN package, 1.0x3.8mm, (Ref: https://katalog.we-online.de/pbs/datasheet/824014881.pdf)")
	(tags "UDFN SMD")
	(property "Reference" "D6"
		(at -0.05 -2.75 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "fc0ed1f3-1f18-4d9d-9077-8b679be2b1f0")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "DT1240A-08LP3810"
		(at 1 0 90)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "87bfbf83-2535-468f-baa4-24c607dbfe0a")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.0625)
			)
		)
	)
	(property "Footprint" "Package_DFN_QFN:UDFN-9_1.0x3.8mm_P0.5mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "66741a4b-4b04-4a48-8b94-4c871d077fe2")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DT1240A-08LP3810.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b36d7bcf-19ac-4f77-b439-9bf9d8fdf806")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "05b72c91-a923-4b0b-b798-c215512dd56a")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "LCSC" "C5175174"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "9b9e1a29-accf-4e7b-b791-52778b59774b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "Diodes"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "ab1c74af-74c3-4de3-907e-2bbc71155f59")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "DT1240A-08LP3810Q-7"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "a63c8192-0643-4879-a54e-592e36d684ce")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -0.75 -1.45)
		(end -0.6 -1.05)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "601eb15a-c152-4f8c-b7a4-c0a86b10858a")
	)
	(fp_rect
		(start -0.75 -0.575)
		(end -0.6 -0.225)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "6f2908ef-0edb-49d1-9d5a-bb8f77d9336f")
	)
	(fp_rect
		(start -0.75 0.225)
		(end -0.6 0.575)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "60380682-0a35-4dab-a195-4fdf03df52c6")
	)
	(fp_rect
		(start -0.75 1.05)
		(end -0.6 1.45)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "7a0c98f5-ee47-4789-a3fb-72ea5403df7d")
	)
	(fp_rect
		(start 0.6 -1.05)
		(end 0.75 -0.65)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "51f246f1-0398-4a51-afcf-33b8732309d4")
	)
	(fp_rect
		(start 0.6 -0.175)
		(end 0.75 0.175)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "8979144d-b2c1-4f50-bf71-4b471fa236ac")
	)
	(fp_rect
		(start 0.6 0.65)
		(end 0.75 1.05)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "52bed06e-db5f-4f90-b510-d727ed39c75e")
	)
	(fp_arc
		(start -0.675 -2)
		(mid -0.653033 -2.053033)
		(end -0.6 -2.075)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9dc22fa1-760a-401a-a7cd-827a2907583e")
	)
	(fp_arc
		(start -0.6 2.075)
		(mid -0.653033 2.053033)
		(end -0.675 2)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dd4619cc-23a2-4104-89c8-fc12ce7c1d39")
	)
	(fp_arc
		(start 0.6 -2.075)
		(mid 0.653033 -2.053033)
		(end 0.675 -2)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4db643e6-9561-41a0-a114-20c1c3ad5ef0")
	)
	(fp_arc
		(start 0.675 2)
		(mid 0.653033 2.053033)
		(end 0.6 2.075)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "da6f85ca-e13f-4cd5-8032-6fcf71ec7c42")
	)
	(fp_poly
		(pts
			(xy -0.75 -1.7) (xy -0.9 -1.85) (xy -0.9 -1.55)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "041a497b-8ee9-488e-be8c-986dd47c7e52")
	)
	(fp_poly
		(pts
			(xy 0.6 -1.525) (xy 0.6 -2) (xy -0.6 -2) (xy -0.6 -1.925) (xy -0.75 -1.925) (xy -0.75 -2) (xy -0.6 -2.15)
			(xy 0.6 -2.15) (xy 0.75 -2) (xy 0.75 -1.525)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "6482ad9b-36f0-460c-b73a-2effd80b2d02")
	)
	(fp_poly
		(pts
			(xy 0.6 1.525) (xy 0.6 2) (xy -0.6 2) (xy -0.6 1.925) (xy -0.75 1.925) (xy -0.75 2) (xy -0.6 2.15)
			(xy 0.6 2.15) (xy 0.75 2) (xy 0.75 1.525)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "a7d6d839-c1ae-4904-8798-eb92ea3d62eb")
	)
	(fp_line
		(start -0.8 -1.85)
		(end -0.8 1.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "313c2723-5c08-461e-8874-3f42eb14086b")
	)
	(fp_line
		(start -0.5 2.15)
		(end 0.5 2.15)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e0faf3cc-d306-4d31-80c3-d4a70d972a42")
	)
	(fp_line
		(start 0.5 -2.15)
		(end -0.5 -2.15)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f8735812-617d-4d11-bd19-79894bbda5d8")
	)
	(fp_line
		(start 0.8 1.85)
		(end 0.8 -1.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b33d683e-fd88-498b-99ce-5a442a3ce2b4")
	)
	(fp_arc
		(start -0.8 -1.85)
		(mid -0.712132 -2.062132)
		(end -0.5 -2.15)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "75f9e6a6-50f1-47c8-be55-5f7c9d46a5fd")
	)
	(fp_arc
		(start -0.5 2.15)
		(mid -0.712132 2.062132)
		(end -0.8 1.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "026155a5-bd53-4bff-89b9-f7fd9eabf303")
	)
	(fp_arc
		(start 0.5 -2.15)
		(mid 0.712132 -2.062132)
		(end 0.8 -1.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1c6225be-6ddf-46e0-b3f7-335cd74b0b30")
	)
	(fp_arc
		(start 0.8 1.85)
		(mid 0.712132 2.062132)
		(end 0.5 2.15)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1a5bc0c9-6666-433d-a654-d5ad37b0bc06")
	)
	(fp_rect
		(start -0.5 -1.9)
		(end 0.5 1.9)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "182e67a4-3d9a-49a3-8469-6e06b4c6617c")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "ca3e575e-1e67-4ecb-9fbf-df83a341eb49")
		(effects
			(font
				(size 0.3 0.3)
				(thickness 0.05)
			)
		)
	)
	(pad "" smd oval
		(at -0.4 -1.7)
		(size 0.35 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "05933678-71b0-44f7-9e56-c68ffdc96a40")
	)
	(pad "" smd oval
		(at -0.4 -0.8)
		(size 0.35 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c6870f1d-c95e-415d-89d2-83771ce5c19c")
	)
	(pad "" smd oval
		(at -0.4 0)
		(size 0.35 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1790e912-2470-4298-a70e-3be7bd19ede3")
	)
	(pad "" smd oval
		(at -0.4 0.8)
		(size 0.35 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "d8d540cc-ed5a-4218-9b43-66353c5d4142")
	)
	(pad "" smd oval
		(at -0.4 1.7)
		(size 0.35 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4df6184b-d628-4c94-b23b-c2cb4932fc8c")
	)
	(pad "" smd oval
		(at 0.4 -1.3)
		(size 0.35 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5f880fc9-a377-42ac-b7c8-46f9c0fa0642")
	)
	(pad "" smd oval
		(at 0.4 -0.4)
		(size 0.35 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "09b0cb36-37c5-4b58-a99f-7d4733e2ddf9")
	)
	(pad "" smd oval
		(at 0.4 0.4)
		(size 0.35 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "73983db8-09c4-4515-8d28-be4c7a361b7c")
	)
	(pad "" smd oval
		(at 0.4 1.3)
		(size 0.35 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f6ee1b72-44b5-4b05-8c90-d90aa598f6b4")
	)
	(pad "1" smd roundrect
		(at -0.4 -1.7)
		(size 0.5 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4307af98-ed54-4576-b390-663c0ee3f4a9")
	)
	(pad "2" smd roundrect
		(at -0.4 -0.8)
		(size 0.5 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "aacd55a7-f64d-4328-85fd-0b9cadda84c5")
	)
	(pad "3" smd roundrect
		(at -0.4 0)
		(size 0.5 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "691e2ab3-f8f9-49e7-bf46-e1fbba28eca8")
	)
	(pad "4" smd roundrect
		(at -0.4 0.8)
		(size 0.5 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "89de2769-6299-46fc-bdd4-af6cf538f35b")
	)
	(pad "5" smd roundrect
		(at -0.4 1.7)
		(size 0.5 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "70de0d90-c1af-441c-855e-6fe5f0d0ffa1")
	)
	(pad "6" smd roundrect
		(at 0.4 1.3)
		(size 0.5 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ff481316-00aa-4d19-a569-b66f52c83009")
	)
	(pad "7" smd roundrect
		(at 0.4 0.4)
		(size 0.5 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f27b9d24-ae09-48a4-8ecb-064844601ee1")
	)
	(pad "8" smd roundrect
		(at 0.4 -0.4)
		(size 0.5 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c691e0d8-584c-4514-a8e5-e734795a987a")
	)
	(pad "9" smd roundrect
		(at 0.4 -1.3)
		(size 0.5 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7cfaac43-f4d4-4f90-afc4-53a336365716")
	)
	(model ":KICAD7_3DMODEL_DIR:Package_DFN_QFN.3dshapes/UDFN-9 1.0x3.8.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)