(module 5P_4x1.5 (layer F.Cu) (tedit 56ABAD87)
  (attr virtual)
  (fp_text reference J4 (at 0 -5.5) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value I2C (at -2.75 0 90) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user 1 (at -2.5 -4.5) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (pad 1 connect rect (at 0 -4) (size 4 1.5) (layers F.Cu F.Mask)
    (zone_connect 0))
  (pad 2 connect oval (at 0 -2) (size 4 1.5) (layers F.Cu F.Mask)
    (zone_connect 2))
  (pad 3 connect oval (at 0 0) (size 4 1.5) (layers F.Cu F.Mask)
    (zone_connect 0))
  (pad 4 connect oval (at 0 2) (size 4 1.5) (layers F.Cu F.Mask)
    (zone_connect 0))
  (pad 5 connect oval (at 0 4) (size 4 1.5) (layers F.Cu F.Mask)
    (zone_connect 0))
)
