(footprint "Crystal_SMD_3225-4Pin_3.2x2.5mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
	(tags "SMD SMT crystal")
	(property "Reference" "Y1"
		(at 0 -2.450001 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "5f39be95-1e69-4bd3-8eb6-1c5d3f96f6a5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "12MHz"
		(at 0 2.450001 180)
		(layer "F.Fab")
		(uuid "2f56409c-026f-491a-b5a4-8a2486033946")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "82a72064-0a1b-4be6-b315-a641b6bc3834")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
			(justify mirror)
		)
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "b8de3b10-6514-4a3c-a457-2bd9f5c052cd")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
			(justify mirror)
		)
	)
	(property "Description" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "167e3553-8ce1-41d4-8799-0c857ed2335e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
			(justify mirror)
		)
	)
	(property "LCSC" "C9002"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "4fd478e5-52d6-414f-8705-179d9a6cca5c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "YXC"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "14e68d84-2bf5-4679-b076-4d92976a0784")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "X322512MSB4SI"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "0718d1ea-bcef-4789-8c33-852bfb408ee5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_arc
		(start -1.85 1.575)
		(mid -1.903033 1.553033)
		(end -1.925 1.5)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ff502784-fc46-4274-a48f-b8c2b9f6b2e3")
	)
	(fp_poly
		(pts
			(xy -1.85 -1.4) (xy -1.85 1.5) (xy 1.75 1.5) (xy 1.75 1.65) (xy -1.85 1.65) (xy -2 1.5) (xy -2 -1.4)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "7f1ef02c-5894-471f-9e1d-e305efdfae70")
	)
	(fp_line
		(start -1.95 1.3)
		(end -1.95 -1.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f54bdc57-6f67-49a3-9fdf-4f7aa5974fcd")
	)
	(fp_line
		(start -1.65 -1.6)
		(end 1.65 -1.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e74e381f-6b10-4e11-b4c0-6819fa1c0e97")
	)
	(fp_line
		(start 1.65 1.6)
		(end -1.65 1.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4fe697a6-c3c7-4eca-8b35-a97a9520c2df")
	)
	(fp_line
		(start 1.95 -1.3)
		(end 1.95 1.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "277ab97b-f918-411e-aa32-6d86cd7151e1")
	)
	(fp_arc
		(start -1.95 -1.3)
		(mid -1.862132 -1.512132)
		(end -1.65 -1.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4433e626-ca01-4b09-88c1-98440386fb59")
	)
	(fp_arc
		(start -1.65 1.6)
		(mid -1.862132 1.512132)
		(end -1.95 1.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a90da40e-2ae0-48d6-9595-ddce9c97b178")
	)
	(fp_arc
		(start 1.65 -1.6)
		(mid 1.862132 -1.512132)
		(end 1.95 -1.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "21d5ed30-04cb-4f26-904a-627802c4bf7e")
	)
	(fp_arc
		(start 1.95 1.3)
		(mid 1.862132 1.512132)
		(end 1.65 1.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bee2039a-f9ea-4793-afbe-19c97025064b")
	)
	(fp_line
		(start -1.6 -1.25)
		(end 1.6 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "14ea30b2-75b2-4076-bfb0-56ea28a4775b")
	)
	(fp_line
		(start -1.6 1.25)
		(end -1.6 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1c022aab-5f26-45c2-a9f5-9f7bf213568d")
	)
	(fp_line
		(start -0.600001 1.25)
		(end -1.6 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "36d238d7-8910-412e-a9f4-942475b795ee")
	)
	(fp_line
		(start 1.6 -1.25)
		(end 1.6 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8a1e5214-335c-4350-837d-b565eefcaba6")
	)
	(fp_line
		(start 1.6 1.25)
		(end -1.6 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "70dbd212-a100-4e3d-8556-5278d7b8a031")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "b075cc83-e42f-4d34-953d-377dc6733731")
		(effects
			(font
				(size 0.7 0.7)
				(thickness 0.105)
			)
		)
	)
	(pad "" smd roundrect
		(at -1.1 -0.85)
		(size 1.1 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.2777777778)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "58b38a82-5acb-4602-beaa-afd1b9b04a18")
	)
	(pad "" smd roundrect
		(at -1.1 0.85)
		(size 1.1 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.2777777778)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "31bf4393-225f-4e5b-b799-e783c2686bc7")
	)
	(pad "" smd roundrect
		(at 1.1 -0.85)
		(size 1.1 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.2777777778)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b6491021-8d13-4656-9507-da7b1fcf4789")
	)
	(pad "" smd roundrect
		(at 1.1 0.85)
		(size 1.1 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.2777777778)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "dc425b0e-cd7a-4b2d-bc7b-723eb78fe22f")
	)
	(pad "1" smd roundrect
		(at -1.1 0.85)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.15)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "10e04bea-e5de-49f6-8bca-7f717d9cdca3")
	)
	(pad "2" smd roundrect
		(at 1.1 0.85)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.15)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right bottom_left)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "624d628f-7fb1-4d04-b0a8-06736f43b247")
	)
	(pad "3" smd roundrect
		(at 1.1 -0.85)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.15)
		(chamfer_ratio 0.05)
		(chamfer top_left bottom_left bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a3589278-51c8-41b8-b7c5-b1cbc753656f")
	)
	(pad "4" smd roundrect
		(at -1.1 -0.85)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.15)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_left bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c85cb441-da6d-40aa-83ba-95170480376a")
	)
	(model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
