(footprint "1412_C"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1.325 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "757dbb4d-6b98-45f0-8706-cb1e4c60540d")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "1412_C"
		(at 0 0.95 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "84345d63-d56f-42ef-8ead-3976643439ff")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
		)
	)
	(property "Footprint" ""
		(at 0 1.05 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "01272672-78f8-4683-82b2-3659761f7c27")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 1.05 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "90c22bb5-a0d7-4f8c-aa86-d3bd23f0d98d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 1.05 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "73c912c1-7c34-4fbb-af87-448499073b15")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_poly
		(pts
			(xy -0.15 -0.625) (xy 0.15 -0.625) (xy 0.25 -0.775) (xy -0.25 -0.775)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "6579e2ef-8769-4ebd-aae6-26f5ea74a927")
	)
	(fp_poly
		(pts
			(xy 0.15 0.625) (xy -0.15 0.625) (xy -0.25 0.775) (xy 0.25 0.775)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "358d7e0f-f130-4c63-894c-405df5863f64")
	)
	(fp_line
		(start -0.9 0.575)
		(end -0.9 -0.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6e8282c5-fea6-4b75-ad13-443b8dc526d7")
	)
	(fp_line
		(start -0.7 -0.775)
		(end 0.7 -0.775)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7182b40a-ca1b-48cc-ba09-db1ffd408b58")
	)
	(fp_line
		(start 0.7 0.775)
		(end -0.7 0.775)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a791bd07-57ab-4a97-bfa5-059eccc35326")
	)
	(fp_line
		(start 0.9 -0.575)
		(end 0.9 0.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9296a018-cb76-4586-b7f2-b1ec520e2683")
	)
	(fp_arc
		(start -0.9 -0.575)
		(mid -0.841421 -0.716421)
		(end -0.7 -0.775)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "22ba899d-1b80-47fb-93e0-18203d26e262")
	)
	(fp_arc
		(start -0.7 0.775)
		(mid -0.841421 0.716421)
		(end -0.9 0.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "075a1366-21d2-4bcc-94c4-7cb07b0938d1")
	)
	(fp_arc
		(start 0.7 -0.775)
		(mid 0.841421 -0.716421)
		(end 0.9 -0.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9a0c3137-e3d2-4df5-9550-69b060b97364")
	)
	(fp_arc
		(start 0.9 0.575)
		(mid 0.841421 0.716421)
		(end 0.7 0.775)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3d3e6fbe-46a9-40c8-b874-d8f939e9cf93")
	)
	(fp_rect
		(start -0.7 -0.6)
		(end 0.7 0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "11aef28f-8412-4214-92e5-302f47107401")
	)
	(fp_text user "${REFERENCE}"
		(at 0 1.3 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "5835fa64-bcfb-40e6-a4eb-aa9ccd99f6c2")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.4875 0)
		(size 0.525 1.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(thermal_bridge_angle 45)
		(uuid "6a77370d-8459-4a3b-8706-07c587f9538b")
	)
	(pad "2" smd roundrect
		(at 0.4875 0)
		(size 0.525 1.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(chamfer_ratio 0.05)
		(chamfer top_left bottom_left)
		(thermal_bridge_angle 45)
		(uuid "b8be16af-26e7-4bfa-b950-c9a5a050441d")
	)
)
