(footprint "Crystal_SMD_3215-2Pin_3.2x1.5mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SMD Crystal FC-135 https://support.epson.biz/td/api/doc_check.php?dl=brief_FC-135R_en.pdf")
	(tags "SMD SMT Crystal")
	(property "Reference" "Y3"
		(at 0 -2 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "48cb84cc-8a8a-4527-9c7a-88950877674e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "32768"
		(at 0 2 0)
		(layer "F.Fab")
		(uuid "bb4de9d1-4c78-4cd1-aa0d-0c9098f2541b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Crystal:Crystal_SMD_3215-2Pin_3.2x1.5mm"
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "e2d24c32-a8f3-423d-954f-e807eaba12af")
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify mirror)
		)
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "29eb3af7-a44d-4b8f-a59b-f0e50a0ed39b")
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify mirror)
		)
	)
	(property "Description" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "f59b90d3-87f8-4269-9145-f3b91b1d65fc")
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify mirror)
		)
	)
	(property "LCSC" "C95361"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "c172a846-7cb9-4c33-a6a7-9d8c808eac10")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "Seiko"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2a99ad2b-680f-4259-b214-2ffe2b682bbf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "Q13FC1350004900"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7c6c8f81-c76d-41de-afe5-170ba042ddd9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0.675 -0.875)
		(end -0.675 -0.875)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3c821e4a-00ac-4f82-b56c-a872839fb1d5")
	)
	(fp_line
		(start 0.675 0.875)
		(end -0.675 0.875)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "27e90baf-160e-4e5c-8f1a-17c30831af79")
	)
	(fp_line
		(start -2 1.15)
		(end -2 -1.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8a5ec1da-07eb-4bd5-9685-7af676df0195")
	)
	(fp_line
		(start 2 -1.15)
		(end -2 -1.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "0afd00c0-f296-4dba-b89f-61ebee320bad")
	)
	(fp_line
		(start 2 1.15)
		(end -2 1.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8b530ece-7a16-4dd6-a2c7-c5b24eadd4b8")
	)
	(fp_line
		(start 2 1.15)
		(end 2 -1.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4aa574ca-633d-42d2-ada7-49dbc74f64fb")
	)
	(fp_line
		(start -1.6 0.75)
		(end -1.6 -0.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ff0687ce-1c01-4cc9-bd2c-0c8bd60d7fd9")
	)
	(fp_line
		(start 1.6 -0.75)
		(end -1.6 -0.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8e586fbb-418a-4cb6-a012-5e4ef1289063")
	)
	(fp_line
		(start 1.6 0.75)
		(end -1.6 0.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "28e17f0e-e0bf-49fd-b9bb-3f6de528b628")
	)
	(fp_line
		(start 1.6 0.75)
		(end 1.6 -0.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d7b031d2-8f0b-4ad3-a7cf-38281427c1b4")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2 0)
		(layer "F.Fab")
		(uuid "4d5d45f1-b981-4a83-b929-283bb36cf626")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at 1.25 0)
		(size 1 1.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "93792bb1-bd24-4648-baa9-6826dc4a1d16")
	)
	(pad "2" smd rect
		(at -1.25 0)
		(size 1 1.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "34996cf4-a4aa-4ccc-96d1-828691bfb527")
	)
	(model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3215-2Pin_3.2x1.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD7_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_MicroCrystal_CC7V-T1A-2Pin_3.2x1.5mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)