(footprint "MOUNT_HOLE_M2"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(locked yes)
	(layer "F.Cu")
	(tags "MOUNT HOLE FASTENER SCREW")
	(property "Reference" "H7"
		(at 0 -1 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "38c4edb6-6f55-4a46-87bd-7878c294f1e8")
		(effects
			(font
				(size 0.001 0.001)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "M2"
		(at 0 1 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "fa677060-23e0-4463-b47e-8d842528e47a")
		(effects
			(font
				(size 0.001 0.001)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "MountingHole:MOUNT_HOLE_M2"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "03648e22-bdc9-4f5f-9947-8163d9852c8a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "0ee6b798-fbb9-4273-a452-66c809239615")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "a015cb0f-2286-4b02-bfb8-8c7125ffeed2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Enable" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "9a07e807-30ec-499b-8f19-e0b29308bfa4")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "exclude_from_bom" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d3b6b819-7440-4750-b588-9dfcde1394e8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.0001)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_circle
		(center 0 0)
		(end 1.925 0)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill none)
		(layer "B.SilkS")
		(uuid "f7db79c7-4db2-4dde-b2c3-137dd74f9b1a")
	)
	(fp_circle
		(center 0 0)
		(end 2.25 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "B.CrtYd")
		(uuid "10d84138-4048-422a-acd9-0ffc97aa7033")
	)
	(fp_circle
		(center 0 0)
		(end 2.25 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "784afb62-58ae-4886-968c-b5417283fc92")
	)
	(fp_circle
		(center 0 0)
		(end 4 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "B.Fab")
		(uuid "8e998f07-a11b-4981-9480-1bc513155424")
	)
	(fp_text user "M2 INSERT + PLASTIC WALL 1,75mm"
		(at 0 2.7 0)
		(layer "B.Fab")
		(uuid "e5a83732-a419-4004-b948-14ac97d56bbe")
		(effects
			(font
				(size 0.2 0.2)
				(thickness 0.05)
			)
			(justify mirror)
		)
	)
	(fp_text user "M2"
		(at 2.2 -1.6 0)
		(layer "F.Fab")
		(uuid "f3bd04e0-a19e-4f12-8b34-13803dd9151a")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.127)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.7 2.7)
		(drill 2.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.2)
			(max_length 0.15)
			(best_width_ratio 1)
			(max_width 0.3)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "bcc2d053-170b-43b8-9c0d-fcae8f695b1a")
	)
	(pad "1" connect circle
		(at 0 0)
		(size 4 4)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.2)
			(max_length 0.15)
			(best_width_ratio 1)
			(max_width 0.3)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8b6297fa-f1a3-4b85-bb38-dcc0c8737362")
	)
)
