(footprint "1P_D0.8"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "4820e8eb-6893-4033-9557-07133ccc8335")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "1P_D0.8"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "f1e6d07a-e6ff-403d-b381-93b23e97ca7e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "1P_D0.8"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d218bf68-17d3-4587-a98d-9e72893947bc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ba9e2f84-48c6-4a7a-9b39-c6cb8af4e7ef")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1f1f5c02-96cc-4f2e-b7cd-ae8a1b8cecc6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd exclude_from_pos_files exclude_from_bom)
	(fp_circle
		(center 0 0)
		(end 0.55 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "a8dd8ca2-3eb0-42dd-a6d4-63683cbe5aaf")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "e2ed83c9-e61b-4c09-b95a-e4e0be549fbf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" connect circle
		(at 0 0)
		(size 0.8 0.8)
		(layers "F.Cu" "F.Mask")
		(uuid "ada23472-f28f-4abc-815c-cc40b12da98d")
	)
)
