(footprint "G-Switch_SK-22F03-Gxxx_DPDT_Angled" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "LCSC" "C2848866")
  (property "MFG" "G-Switch")
  (property "MPN" "SK-22F03-G060")
  (property "Sheetfile" "ShuntModule.kicad_sch")
  (property "Sheetname" "")
  (attr smd)
  (fp_text reference "SW1" (at 0 -8.2 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 88dc3605-4191-4a1e-98e7-569cb2007c46)
  )
  (fp_text value "TERMINATE" (at 0 -0.5 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    (tstamp e1b70873-51b7-4b68-ad0b-269f467712a2)
  )
  (fp_text user "G075" (at -4.1 7.4 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp 04d25511-8450-4000-827a-8ac1df940d33)
  )
  (fp_text user "G070" (at -4.1 6.9 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp 40b7b880-eec4-42d3-8ee6-7d1656ce6781)
  )
  (fp_text user "G080" (at -4.1 7.9 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp 42dfb776-0904-459c-acda-3fa994a3aece)
  )
  (fp_text user "G100" (at -4.1 9.9 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp 743f8ab9-2c5f-4dc8-ac32-8576a2f01daf)
  )
  (fp_text user "G090" (at -4.1 8.9 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp 7b85027d-ab95-46d3-b5d0-e44c7d8c526e)
  )
  (fp_text user "G040" (at -4.1 3.9 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp 80989cd8-678b-4b41-88d0-8425a1184075)
  )
  (fp_text user "G020" (at -4.1 1.9 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp 86eeffc1-93d3-400e-9ec8-04a711ac5485)
  )
  (fp_text user "G050" (at -4.1 4.9 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp 98ebc1da-7ae9-4616-8a3b-17677eb10104)
  )
  (fp_text user "G060" (at -4.1 5.9 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp aad2466c-37f4-4caa-880c-25c93af827e9)
  )
  (fp_text user "G095" (at -4.1 9.4 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp be0754a2-b64b-421d-bd36-f2e45da0afce)
  )
  (fp_text user "G065" (at -4.1 6.4 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp c09eab82-7564-4e2c-8ac8-572d8fc9dc36)
  )
  (fp_text user "${REFERENCE}" (at 0 -6.7 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c42e0d82-b925-4ddf-985c-87cc211179ee)
  )
  (fp_text user "G055" (at -4.1 5.4 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp d6d6f87a-8458-45d6-abdb-fe1f89edb2b5)
  )
  (fp_text user "G085" (at -4.1 8.4 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp e42010ec-0f30-4758-a5ea-ceee81bb559c)
  )
  (fp_text user "G030" (at -4.1 2.9 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)) (justify left bottom))
    (tstamp f207c1c7-6019-4854-8ac3-2ddb1c8f1d50)
  )
  (fp_arc (start -8.575 -7.5) (mid -8.553033 -7.553033) (end -8.5 -7.575)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 425e4859-5243-4204-85ff-0a6608a8e2ba))
  (fp_arc (start -8.575 -7.5) (mid -8.553033 -7.553033) (end -8.5 -7.575)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp fa9000e4-5cb7-47ac-9f5c-1f55a175db92))
  (fp_arc (start -8.5 0.075) (mid -8.553033 0.053033) (end -8.575 0)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 213bb81e-3aa5-4666-9917-08564e0433d6))
  (fp_arc (start 8.5 -7.575) (mid 8.553033 -7.553033) (end 8.575 -7.5)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp f1e60587-c299-4b16-b539-dcf518856619))
  (fp_arc (start 8.575 0) (mid 8.553033 0.053033) (end 8.5 0.075)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 1e66ec29-ef75-4ed5-8ea4-07f3776a7a58))
  (fp_poly
    (pts
      (xy -8.5 -7.5)
      (xy -7.5 -7.5)
      (xy -7.5 -7.65)
      (xy -8.5 -7.65)
      (xy -8.65 -7.5)
      (xy -8.65 -6.5)
      (xy -8.5 -6.5)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 1c9f5f05-f862-4fb2-9dad-92dc856288f4))
  (fp_poly
    (pts
      (xy -8.5 -7.5)
      (xy -7.5 -7.5)
      (xy -7.5 -7.65)
      (xy -8.5 -7.65)
      (xy -8.65 -7.5)
      (xy -8.65 -6.5)
      (xy -8.5 -6.5)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp f8d1926a-64cd-4048-9293-3ccf260b7725))
  (fp_poly
    (pts
      (xy -8.5 0)
      (xy -8.5 -1)
      (xy -8.65 -1)
      (xy -8.65 0)
      (xy -8.5 0.15)
      (xy -7.5 0.15)
      (xy -7.5 0)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 7a4a633b-0abe-4132-88c8-e0b33e44480c))
  (fp_poly
    (pts
      (xy 8.5 -7.5)
      (xy 8.5 -6.5)
      (xy 8.65 -6.5)
      (xy 8.65 -7.5)
      (xy 8.5 -7.65)
      (xy 7.5 -7.65)
      (xy 7.5 -7.5)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp b1fa4f8a-ff40-453f-8845-0e379d9c5ddc))
  (fp_poly
    (pts
      (xy 8.5 0)
      (xy 7.5 0)
      (xy 7.5 0.15)
      (xy 8.5 0.15)
      (xy 8.65 0)
      (xy 8.65 -1)
      (xy 8.5 -1)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 5655455a-da92-4957-ac8d-8c7bbdbcd100))
  (fp_line (start -8.9 -4.75) (end -8.9 -2.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ec8c0ebb-56d3-4a61-b0c5-301456bb90ce))
  (fp_line (start -8.757565 -2.343948) (end -8.75 0)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b474eede-7c5f-4437-80e1-71ea07a8a38d))
  (fp_line (start -8.75 -7.5) (end -8.757565 -5.156052)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 18f08a84-6d8e-438c-bad9-3c5550670aa1))
  (fp_line (start -8.5 0.25) (end 8.5 0.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 894798e7-4fa2-438b-9f79-e87ad745036c))
  (fp_line (start 8.5 -7.75) (end -8.5 -7.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1ac88920-0463-436b-975c-b165e3accb11))
  (fp_line (start 8.75 0) (end 8.757565 -2.343948)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0f29d795-534d-42dd-8623-11c8349d09c1))
  (fp_line (start 8.757565 -5.156052) (end 8.75 -7.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c2f0ca3b-c6ad-4e3d-9443-00516a8132ca))
  (fp_line (start 8.9 -2.75) (end 8.9 -4.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0342d7cb-25ab-461d-8489-9f3d545fc52b))
  (fp_arc (start -8.9 -4.75) (mid -8.863358 -4.965154) (end -8.757565 -5.156052)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8e23094e-8a09-4e2e-898d-caf44fea8a26))
  (fp_arc (start -8.757565 -2.343948) (mid -8.863359 -2.534845) (end -8.9 -2.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6c8cacbd-be3c-429f-8d9f-74197f6afabb))
  (fp_arc (start -8.75 -7.5) (mid -8.676777 -7.676777) (end -8.5 -7.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a7ecb969-a153-462f-80d4-8b9521e11644))
  (fp_arc (start -8.5 0.25) (mid -8.676777 0.176777) (end -8.75 0)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp eb4f173c-3360-4f78-b52c-0ace11fcf3d6))
  (fp_arc (start 8.5 -7.75) (mid 8.676777 -7.676777) (end 8.75 -7.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 51674508-5206-4e7b-9384-192e04e48af3))
  (fp_arc (start 8.75 0) (mid 8.676777 0.176777) (end 8.5 0.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 430cf8fd-c01c-4645-a909-a7bb0bf3e125))
  (fp_arc (start 8.757565 -5.156052) (mid 8.863359 -4.965155) (end 8.9 -4.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ba49ad78-ed96-4f65-ae1b-dee5e187c97e))
  (fp_arc (start 8.9 -2.75) (mid 8.863358 -2.534845) (end 8.757565 -2.343948)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 47468c66-1bcd-4ef0-996a-b4727f9beafa))
  (fp_line (start -4.2 0) (end -4.2 10)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 879d9b26-84c3-4816-9836-9c070f28c54b))
  (fp_line (start -4.2 2) (end 1.2 2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp f0012744-ee45-44e7-9c25-387eb77c8a48))
  (fp_line (start -4.2 3) (end 1.2 3)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp dd689fa6-7db6-49d0-86b1-556cdfc8a834))
  (fp_line (start -4.2 4) (end 1.2 4)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp be62a931-2dd0-412c-a966-3a5b9515e959))
  (fp_line (start -4.2 5) (end 1.2 5)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp f0b88683-8e6c-41ba-abad-6433cfe4054d))
  (fp_line (start -4.2 5.5) (end 1.2 5.5)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp c9a1ee46-5db1-42a5-acd4-05d9c9c73817))
  (fp_line (start -4.2 6) (end 1.2 6)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 12f85514-20a5-40c0-b27a-11b25e985114))
  (fp_line (start -4.2 6.5) (end 1.2 6.5)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 23370305-f902-495e-a50f-706ed4b7ba89))
  (fp_line (start -4.2 7) (end 1.2 7)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp b1dc1ef5-3ea2-4a19-b342-e6e745347968))
  (fp_line (start -4.2 7.5) (end 1.2 7.5)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 4418164b-155d-4b33-ba48-1b1358e4c9ff))
  (fp_line (start -4.2 8) (end 1.2 8)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 6592f321-1e13-4461-b061-d4bf34e4cfba))
  (fp_line (start -4.2 8.5) (end 1.2 8.5)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 9b104bf5-aace-4434-8551-5e71cca0e3fc))
  (fp_line (start -4.2 9) (end 1.2 9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp e6ee9299-c733-4084-a8a7-0f9fac151fff))
  (fp_line (start -4.2 9.5) (end 1.2 9.5)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp d8b7973a-1a76-4aa8-b9b7-e288280e76e0))
  (fp_line (start -4.2 10) (end 1.2 10)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 459910fd-bda6-4c15-bfc7-013258411103))
  (fp_line (start 1.2 10) (end 1.2 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 448a6155-60f9-4ddc-a668-2f70174590b4))
  (fp_line (start 1.2 10) (end 4.2 10)
    (stroke (width 0.1) (type dash)) (layer "F.Fab") (tstamp c19d400d-3679-4a55-87e8-eb24adbf2fcf))
  (fp_line (start 4.2 10) (end 4.2 0)
    (stroke (width 0.1) (type dash)) (layer "F.Fab") (tstamp 4889d381-60fe-4450-9022-ee02d8a08ed5))
  (fp_rect (start -8.5 0) (end 8.5 -7.5)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 65e7bc77-b116-4a36-94a6-7f07dd967b1b))
  (pad "1" thru_hole circle (at -4 -5.05) (size 1.55 1.55) (drill 1.25) (layers "*.Cu" "*.Mask") (tstamp 67b55a6b-9b15-4bf0-948f-01674af217a3))
  (pad "1" smd roundrect (at -4 -5.05) (size 1.85 1.85) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25) (tstamp 5b10ef0d-8bc0-4b1c-9048-7be04031b47e))
  (pad "2" thru_hole circle (at 0 -5.05) (size 1.55 1.55) (drill 1.25) (layers "*.Cu" "*.Mask") (tstamp 0a72c147-82ad-4607-8184-1ef580f2c557))
  (pad "2" smd roundrect (at 0 -5.05) (size 1.85 1.85) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25) (tstamp fef3e8e9-6fa4-4821-83d2-5ac05269c932))
  (pad "3" thru_hole circle (at 4 -5.05) (size 1.55 1.55) (drill 1.25) (layers "*.Cu" "*.Mask") (tstamp c297eee4-85c7-4268-b5ea-73239b0cf23c))
  (pad "3" smd roundrect (at 4 -5.05) (size 1.85 1.85) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25) (tstamp a7fca4b1-c575-4d01-94c4-0c0ecabe0791))
  (pad "4" thru_hole circle (at -4 -2.45) (size 1.55 1.55) (drill 1.25) (layers "*.Cu" "*.Mask") (tstamp 03b5710c-eb5f-44c3-ab23-5b20b5767d33))
  (pad "4" smd roundrect (at -4 -2.45) (size 1.85 1.85) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25) (tstamp f87629d3-1207-4143-94b1-15bcf02d94ed))
  (pad "5" thru_hole circle (at 0 -2.45) (size 1.55 1.55) (drill 1.25) (layers "*.Cu" "*.Mask") (tstamp 6270a466-3194-4a29-909e-0c639bec883d))
  (pad "5" smd roundrect (at 0 -2.45) (size 1.85 1.85) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25) (tstamp 1a6c1e3e-96f6-4a78-b8ff-542245c93bad))
  (pad "6" thru_hole circle (at 4 -2.45) (size 1.55 1.55) (drill 1.25) (layers "*.Cu" "*.Mask") (tstamp 731bcfc5-d911-40cb-b952-f3b21fbe1c89))
  (pad "6" smd roundrect (at 4 -2.45) (size 1.85 1.85) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25) (tstamp 064deadf-f298-4d26-accb-9175cb0eecff))
  (pad "MP" thru_hole oval (at -8.25 -3.75) (size 0.95 2.95) (drill oval 0.65 2.65) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp be373223-4cf1-4eb7-8f3f-99ee6d263f85))
  (pad "MP" smd roundrect (at -8.25 -3.75) (size 1.25 3.25) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 4f5744a7-b82e-4bc7-900f-015fb7f17a4c))
  (pad "MP" thru_hole oval (at 8.25 -3.75) (size 0.95 2.95) (drill oval 0.65 2.65) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 39336651-eae4-4141-806c-1ee0b7b134c5))
  (pad "MP" smd roundrect (at 8.25 -3.75) (size 1.25 3.25) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp ebffc7be-75b2-4951-945a-d81236642c78))
  (model ":KICAD7_3DMODEL_DIR:Button_Switch_THT.3dshapes/XB-SK-22F03.stp"
    (offset (xyz -8.5 0 -3))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
