(footprint "2P_7.3x7.3_P7.8" (version 20210108) (generator pcbnew) (layer "F.Cu")
  (tedit 6006BC7B)
  (property "MPN" "NO PART")
  (property "Sheet file" "BrushedMotorController18V15A.kicad_sch")
  (property "Sheet name" "")
  (attr exclude_from_pos_files)
  (fp_text reference "M1" (at -8.25 0 90 unlocked) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 64333cba-e9cd-4d6a-9113-977d7533843e)
  )
  (fp_text value "MOTOR" (at -6.5 0 90 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 29e57e5d-f32a-45a6-9e76-a323b738db7a)
  )
  (fp_text user "${REF}" (at -5 0 90 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d1098221-a269-472e-b75e-dd50a41caaf2)
  )
  (pad "1" connect rect (at -3.9 0) (size 7.3 7.3) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp be849b9a-2740-47d0-acc1-f41b1d4c494f))
  (pad "2" connect rect (at 3.9 0) (size 7.3 7.3) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp 6ed9b1e7-9395-4886-8402-6daa2bfe1dea))
)
