(module MOUNT_HOLE_4-40 (layer F.Cu) (tedit 577019B7)
  (tags "MOUNT HOLE FASTENER SCREW")
  (solder_mask_margin 0.0001)
  (attr virtual)
  (fp_text reference H5 (at 0 -1) (layer F.SilkS) hide
    (effects (font (size 0 0) (thickness 0.15)))
  )
  (fp_text value MOUNT_HOLE (at 0 1) (layer F.SilkS) hide
    (effects (font (size 0 0) (thickness 0.15)))
  )
  (fp_text user "4-40 INSERT + PLASTIC WALL 1,75mm" (at 0 4.5) (layer B.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.02)) (justify mirror))
  )
  (fp_circle (center 0 0) (end 5.0139 0) (layer B.Fab) (width 0.05))
  (fp_text user 4-40 (at 0 -3.9) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_circle (center 0 0) (end 3.2639 0) (layer B.SilkS) (width 0.127))
  (pad 1 thru_hole circle (at 0 0) (size 3.802 3.802) (drill 3.302) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad 1 connect circle (at 0 0) (size 6.5278 6.5278) (layers F.Cu F.Mask)
    (zone_connect 2))
)
