(footprint "WideInputPowerModule"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -7.3 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "03ad6c03-b100-46ba-9e45-ae2707d0c06f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "WideInputPowerModule"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "91a1f93b-4153-4eeb-84ea-016d91d10f29")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "WideInputPowerModule"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f2b04fbb-a050-434f-9330-90d25f9e11d1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1623f154-3ad7-4d94-92cc-ae2a63e2613e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e238fe87-aef0-4513-bf05-5a44b847a48c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -13.65 -1.85)
		(end -13.5 2.6)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "0407bc86-69e9-45cb-9078-63c024ff0032")
	)
	(fp_rect
		(start -8.1 -6.65)
		(end 8.1 -6.5)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "a39ab55f-146b-4549-92d2-0e0aa52b9be2")
	)
	(fp_rect
		(start -8.1 6.5)
		(end 8.1 6.65)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "41b0dc17-9a43-424d-bda3-7c458f8a52f0")
	)
	(fp_rect
		(start 13.5 -2.6)
		(end 13.65 2.6)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "24ab27fc-da5d-4e49-b51c-e62730607d5f")
	)
	(fp_line
		(start -13.75 -6.1)
		(end -13.75 6.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "451d913b-cbd4-4dd1-ba00-7199b01e1346")
	)
	(fp_line
		(start -13.1 -6.75)
		(end 13.1 -6.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0d600142-bc89-428f-99a2-44e2ab76393b")
	)
	(fp_line
		(start 13.1 6.75)
		(end -13.1 6.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "98740769-20a1-4a33-8e93-074140e9d4fd")
	)
	(fp_line
		(start 13.75 6.1)
		(end 13.75 -6.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "930da291-c017-44d4-b74e-4690a5b294e7")
	)
	(fp_arc
		(start -13.75 -6.1)
		(mid -13.559619 -6.559619)
		(end -13.1 -6.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0da97ae1-c9e4-4607-b9b1-cbc5fd881391")
	)
	(fp_arc
		(start -13.1 6.75)
		(mid -13.559619 6.559619)
		(end -13.75 6.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "28303a9d-a77d-41b5-bd25-1b6d9d620d17")
	)
	(fp_arc
		(start 13.1 -6.75)
		(mid 13.559619 -6.559619)
		(end 13.75 -6.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3e9f2895-9e4f-4fef-b0ce-ba5ee050b704")
	)
	(fp_arc
		(start 13.75 6.1)
		(mid 13.559619 6.559619)
		(end 13.1 6.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b35cfb21-6dd0-4275-bfdb-d4e8653c9178")
	)
	(fp_line
		(start -13.5 6.1)
		(end -13.5 -6.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "97994175-3a36-4332-b050-20d860fbd564")
	)
	(fp_line
		(start -13.1 -6.5)
		(end 13.1 -6.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "c424111e-9eaf-4aa4-87a7-be19dd008865")
	)
	(fp_line
		(start 13.1 6.5)
		(end -13.1 6.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "b41fd6c6-36fe-4a4e-9ade-75aeacdea5b1")
	)
	(fp_line
		(start 13.5 -6.1)
		(end 13.5 6.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "7774d81a-8223-4e9a-8c9f-421db0e06079")
	)
	(fp_arc
		(start -13.5 -6.1)
		(mid -13.382843 -6.382843)
		(end -13.1 -6.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "8a4743e9-9e64-420d-9c29-ef8c9035e87a")
	)
	(fp_arc
		(start -13.1 6.5)
		(mid -13.382843 6.382843)
		(end -13.5 6.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "d44845b7-ff7f-451f-9d9d-231b4e438685")
	)
	(fp_arc
		(start 13.1 -6.5)
		(mid 13.382843 -6.382843)
		(end 13.5 -6.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "dff2e872-9c31-4119-b0e6-8366c86d47a4")
	)
	(fp_arc
		(start 13.5 6.1)
		(mid 13.382843 6.382843)
		(end 13.1 6.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "edb6500a-9482-4244-bc80-918703bc4ff4")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "2784dad3-0a67-4541-95cc-613dc0bedbae")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" smd roundrect
		(at -12.5 -4.275)
		(size 1.6 1.45)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "4912ee44-8742-4013-abbe-fec06b12d643")
	)
	(pad "" smd roundrect
		(at -12.5 -2.625)
		(size 1.6 1.45)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "e1a50592-b268-4083-a52b-48bfba2d2176")
	)
	(pad "" smd roundrect
		(at -12.5 3.475)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "b8a127e1-5bc7-4978-baec-cc856daa9c36")
	)
	(pad "" smd roundrect
		(at -12.5 5.425)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "f80c97f0-ba83-4cf9-a4a7-246ce27d85f5")
	)
	(pad "" smd roundrect
		(at -10.7 -4.275)
		(size 1.6 1.45)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "18773ab0-3549-4889-9043-fc2bbcd4ec8e")
	)
	(pad "" smd roundrect
		(at -10.7 -2.625)
		(size 1.6 1.45)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "92a4a5f8-31a2-47e9-b715-9b5ead3260db")
	)
	(pad "" smd roundrect
		(at -10.7 3.475)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "a182e1ce-95b6-4070-95d3-51a833607a82")
	)
	(pad "" smd roundrect
		(at -10.7 5.425)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "7e689862-8b72-4b98-a9f6-99fd5eafe65d")
	)
	(pad "" smd roundrect
		(at -8.9 -4.275)
		(size 1.6 1.45)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "d4ea1707-dbca-48e7-8474-e1b7436e4e74")
	)
	(pad "" smd roundrect
		(at -8.9 -2.625)
		(size 1.6 1.45)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "f16e1943-d43f-441e-96c6-927a7e2e6577")
	)
	(pad "" smd roundrect
		(at -8.9 3.475)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "2a69c46f-25d9-4c5c-bbc1-7d560b3db353")
	)
	(pad "" smd roundrect
		(at -8.9 5.425)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "7b0e2928-1023-4381-ba3f-c68fc214ff79")
	)
	(pad "" smd roundrect
		(at 8.9 -5.45)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "524dc602-9042-483b-aa5b-a81a8684f51f")
	)
	(pad "" smd roundrect
		(at 8.9 -3.5)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "353a4229-3083-496a-84d7-c6efebc5ba2d")
	)
	(pad "" smd roundrect
		(at 8.9 3.5)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "f59165fa-3aeb-4272-814d-f53d8ecda653")
	)
	(pad "" smd roundrect
		(at 8.9 5.45)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "bc7068be-58c4-409a-bfc8-a7f0a962b475")
	)
	(pad "" smd roundrect
		(at 10.7 -5.45)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "5c744f7c-c1ff-42a1-9969-9e14bc0addb6")
	)
	(pad "" smd roundrect
		(at 10.7 -3.5)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "cbfd8c83-4e74-444b-baa0-3fefa17077da")
	)
	(pad "" smd roundrect
		(at 10.7 3.5)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "a01baff5-f71d-4920-96d1-3a4f8a856715")
	)
	(pad "" smd roundrect
		(at 10.7 5.45)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "ba89fcb7-add7-4458-9d68-5f860576a7e9")
	)
	(pad "" smd roundrect
		(at 12.5 -5.45)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "cd6c5f8c-7916-4083-8afb-7f22853ff13c")
	)
	(pad "" smd roundrect
		(at 12.5 -3.5)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "a59a1c96-12bc-4276-839e-084e42369926")
	)
	(pad "" smd roundrect
		(at 12.5 3.5)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "5b7ead84-5a98-4684-b4b1-9188886167e2")
	)
	(pad "" smd roundrect
		(at 12.5 5.45)
		(size 1.6 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.21875)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "7df04b3c-ccb8-4d41-aab9-65b85f398896")
	)
	(pad "1" smd roundrect
		(at -10.7 4.45)
		(size 5.2 3.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.09459459459)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "d132a122-ae67-489c-91b3-38ccf721e34e")
	)
	(pad "2" smd roundrect
		(at 10.7 4.45)
		(size 5.2 3.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.09459459459)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "f69efce0-69a2-401e-89ae-23379dd13636")
	)
	(pad "3" smd roundrect
		(at 10.7 -4.45)
		(size 5.2 3.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.09459459459)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "802ac225-71b4-4559-8846-593f7b6d9fe9")
	)
	(pad "4" smd roundrect
		(at -10.7 -3.45)
		(size 5.2 3.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.109375)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "0af2ab47-58e3-46b4-900f-8b89842bc544")
	)
	(pad "5" smd roundrect
		(at -12.65 -1.1)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "7ae7f479-3def-4c08-afec-73b4edef4f2e")
	)
	(pad "6" smd roundrect
		(at -11.15 -1.1)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "5a6c86cb-e754-4958-857b-9ec89c619188")
	)
	(pad "7" smd roundrect
		(at -12 -5.8)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "e30ad6dd-1d65-4a5b-96c8-2b3f61ee9094")
	)
	(pad "8" smd roundrect
		(at -10.6 -5.8)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "acc94209-08ce-4389-a8f2-397e4461761c")
	)
	(pad "9" smd roundrect
		(at -9.2 -5.8)
		(size 1 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(uuid "acf77286-fef9-43cc-abc1-02512d0bfe0e")
	)
	(model "${KICAD6_3DMODEL_DIR}/Module.3dshapes/WideInputPowerModule.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
