(footprint "JST_SH_SM08B-SRSS-TB_1x08-1MP_P1.00mm_Horizontal"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "JST SH series connector, SM08B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST SH top entry")
	(property "Reference" "J1"
		(at 0 -3.98 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "117d5fce-72ab-40b5-a179-a100756fcc6f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "HALL/TEMP"
		(at 0 3.98 0)
		(layer "F.Fab")
		(uuid "a18f1c37-9046-4197-b270-1dea05a5fc8b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "JST_SH_SM08B-SRSS-TB_1x08-1MP_P1.00mm_Horizontal"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3bf73081-a76c-415d-97f7-4565d40a0a2e")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5e9df83e-1a79-4ea3-9404-9555ca84dcee")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" "Generic connectable mounting pin connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "da39294e-5dea-48f2-8269-f054b36cd142")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "LCSC" "C160407"
		(at 0.65 -8.75 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "57d374c3-49f5-489f-b7ce-0895699a09e1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "JST"
		(at 0.65 -8.75 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d10c2254-f63e-402a-a3e9-8eee1088def4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "SM08B-SRSS-TB(LF)(SN)"
		(at 0 -8.7 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d1549b96-2a9a-42e1-8c36-9b77108bd358")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Preferred" ""
		(at 0.65 -8.75 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8f796a9b-b11d-4ae3-afc9-8b5cb95db34f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0fa629e3-2b17-4ac0-ac8d-92a68ad4c150")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -5.11 -1.785)
		(end -4.06 -1.785)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d50245d8-fbfa-41ae-bcab-3ab2cfb4582b")
	)
	(fp_line
		(start -5.11 0.715)
		(end -5.11 -1.785)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "57c98c6b-20ea-4985-aa21-360d450027cd")
	)
	(fp_line
		(start -4.06 -1.785)
		(end -4.06 -2.775)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "521295fa-2b41-4033-a549-1767cf0dc663")
	)
	(fp_line
		(start -3.94 2.685)
		(end 3.94 2.685)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b1a234f6-a9ca-4eef-ad7b-2e2d1f7dbe8d")
	)
	(fp_line
		(start 5.11 -1.785)
		(end 4.06 -1.785)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "57cdad5f-40e2-404e-b553-04c60f50e13d")
	)
	(fp_line
		(start 5.11 0.715)
		(end 5.11 -1.785)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "84d2bed5-e006-4e1f-aa6c-dc67727a288e")
	)
	(fp_line
		(start -5.55 1.225)
		(end -5.55 2.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c19bddaf-477e-43ba-b343-cd42fc7e5aad")
	)
	(fp_line
		(start -5.25 -1.675)
		(end -5.247014 0.836943)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "39c49be4-b6e3-4353-b086-5c5e97767727")
	)
	(fp_line
		(start -5.15 2.925)
		(end 5.15 2.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b9634f6c-b4ab-4ea9-bf0f-602dd90bcd34")
	)
	(fp_line
		(start -5 -1.925)
		(end -3.95 -1.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5b16a945-394d-44d1-b091-ad06ca641002")
	)
	(fp_line
		(start -3.95 -1.925)
		(end -3.95 -2.625)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "54121bcc-9259-4bd4-ad9e-410889f8ce67")
	)
	(fp_line
		(start 3.65 -2.925)
		(end -3.65 -2.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "aed50ee4-3489-457d-9cc7-809420ddbcc2")
	)
	(fp_line
		(start 3.95 -1.925)
		(end 3.95 -2.625)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "eca00aa2-534d-4454-aa9e-e39649c1dee2")
	)
	(fp_line
		(start 5 -1.925)
		(end 3.95 -1.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "50e09d3c-9c55-46a2-b43a-280926c5bee6")
	)
	(fp_line
		(start 5.25 -1.675)
		(end 5.247014 0.836943)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "35fd6d6b-ae71-416e-8125-2e09f86c6af5")
	)
	(fp_line
		(start 5.55 1.225)
		(end 5.55 2.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c1c3f8bb-3c63-422f-8325-4951de12e848")
	)
	(fp_arc
		(start -5.55 1.225)
		(mid -5.465282 0.978835)
		(end -5.247014 0.836943)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "949c82bf-ee13-4171-9c3c-1cd0d50bc551")
	)
	(fp_arc
		(start -5.25 -1.675)
		(mid -5.176777 -1.851777)
		(end -5 -1.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2a6ff41c-32fb-4169-beb8-a13d13e18aa8")
	)
	(fp_arc
		(start -5.15 2.925)
		(mid -5.432843 2.807843)
		(end -5.55 2.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e06d7c0c-a502-45ee-ba83-0c0f4d9d12f1")
	)
	(fp_arc
		(start -3.95 -2.625)
		(mid -3.862132 -2.837132)
		(end -3.65 -2.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e8207b6d-db8b-4531-9c9b-15cae9cca043")
	)
	(fp_arc
		(start 3.65 -2.925)
		(mid 3.862132 -2.837132)
		(end 3.95 -2.625)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0291c870-cf1d-4df1-aedc-d7d5bdf877de")
	)
	(fp_arc
		(start 5 -1.925)
		(mid 5.176777 -1.851777)
		(end 5.25 -1.675)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5c12f948-4d73-4147-946d-6470aebfdfbe")
	)
	(fp_arc
		(start 5.247014 0.836943)
		(mid 5.465282 0.978835)
		(end 5.55 1.225)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "07466dfc-6be5-487f-9f7e-e2dd6bdfb097")
	)
	(fp_arc
		(start 5.55 2.525)
		(mid 5.432843 2.807843)
		(end 5.15 2.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6b17d291-b7d3-47fc-b940-1780b80edf77")
	)
	(fp_line
		(start -5 -1.675)
		(end -5 2.575)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "556486fa-cd1e-494d-96f3-14569fc0d9fc")
	)
	(fp_line
		(start -5 -1.675)
		(end 5 -1.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a6172615-d164-4693-9496-f189cc593c7f")
	)
	(fp_line
		(start -5 2.575)
		(end 5 2.575)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "322dc46a-8c9e-4aea-8b8c-47f76c42fddc")
	)
	(fp_line
		(start -4 -1.675)
		(end -3.5 -0.967893)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3ec9c70b-611d-4881-b499-51000185e6fe")
	)
	(fp_line
		(start -3.5 -0.967893)
		(end -3 -1.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f7961203-1245-4d1c-861a-4b8627509014")
	)
	(fp_line
		(start 5 -1.675)
		(end 5 2.575)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c7887a02-dea5-42c5-944e-9280b18317b3")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "7d620d9f-33c8-462c-8a8a-36f0c327599d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.5 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "cb82bec9-d0da-4893-afba-e088752c0dbe")
	)
	(pad "2" smd roundrect
		(at -2.5 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "bd88ea64-c3d3-4cab-8164-5d5360a29c03")
	)
	(pad "3" smd roundrect
		(at -1.5 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "47db8a3e-a165-4951-bf1c-6b205fa5134a")
	)
	(pad "4" smd roundrect
		(at -0.5 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "05e9c8f5-ed0b-4035-8890-5525261724ed")
	)
	(pad "5" smd roundrect
		(at 0.5 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "fa66db7d-7683-4417-9c4e-53eea4046b20")
	)
	(pad "6" smd roundrect
		(at 1.5 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2ef47aa6-3d63-4f51-b539-29ecdf62ff0d")
	)
	(pad "7" smd roundrect
		(at 2.5 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "67721c33-49ec-4fe5-985e-5870843180c5")
	)
	(pad "8" smd roundrect
		(at 3.5 -2)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8cfcfad4-7b02-46ee-aeb9-2d05ef0a0350")
	)
	(pad "MP" smd roundrect
		(at -4.8 1.875)
		(size 1.2 1.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2083333333)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "93f3cd13-f670-40bd-a5e5-ea57acaff5db")
	)
	(pad "MP" smd roundrect
		(at 4.8 1.875)
		(size 1.2 1.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2083333333)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7faf1593-86a1-41d8-968b-78b753c9fc95")
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM08B-SRSS-TB_1x08-1MP_P1.00mm_Horizontal.step"
		(hide yes)
		(offset
			(xyz 0 1.325 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM08B-SRSS-TB.STEP"
		(offset
			(xyz 0 -0.45 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
