(footprint "M.2 Nut M2.5 x 6.5" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Field2" "")
  (property "Sheetfile" "MXM and M.2-M.kicad_sch")
  (property "Sheetname" "MXM and M.2-M")
  (property "exclude_from_bom" "")
  (attr smd exclude_from_bom)
  (fp_text reference "H19" (at 0 -7.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b9644c45-ace3-4362-8190-f98aa5a90091)
  )
  (fp_text value "MOUNT_HOLE" (at 0 -6 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b9aed2ea-2799-4150-92be-b60da49c6b83)
  )
  (fp_text user "${REFERENCE}" (at 0 -4.5 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fcbcdfe3-5d7f-478b-9d03-88759f0c4b13)
  )
  (fp_arc (start -2.533845 0.788749) (mid -2.653741 -0.012456) (end -2.526329 -0.8125)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp de92a92f-d18d-4716-b812-ca3bf60ddb67))
  (fp_arc (start -1.95 -1.8) (mid -1.316084 -2.304435) (end -0.559519 -2.594115)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp b1131297-ceb2-42ea-a0d1-87c0986eef7d))
  (fp_arc (start -0.583845 2.588749) (mid -1.337657 2.291979) (end -1.96681 1.781615)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 22507847-b33f-4b08-819a-d3996029c640))
  (fp_arc (start 0.583845 -2.588749) (mid 1.337657 -2.291979) (end 1.96681 -1.781615)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 1ab3a2a6-a0df-4427-8824-de83903cb3d3))
  (fp_arc (start 1.95 1.8) (mid 1.316085 2.304438) (end 0.559519 2.594115)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp c7d6c45d-697b-4eaf-a043-b3ec853141b5))
  (fp_arc (start 2.533845 -0.788749) (mid 2.65374 0.012456) (end 2.526329 0.8125)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 12db5d59-4c50-467d-a25d-2ded6b3bd701))
  (pad "1" thru_hole circle (at 0 0) (size 4.55 4.55) (drill 4.25) (layers "*.Cu" "B.Mask")
    (zone_connect 2) (tstamp a06b3c55-f5b2-45d8-9a26-3bc0c02e5e5a))
  (pad "1" smd circle (at 0 0) (size 6.2 6.2) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp 2e3c108b-095a-4417-9702-fb07702b98ad))
  (model ":KICAD7_3DMODEL_DIR:Hardware.3dshapes/M.2 SMD Nut 6.5mm.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
