(footprint "L_Murata_DFE201610P"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Inductor, Murata, DFE201610P, 2.0x1.6x1.0mm, https://www.murata.com/~/media/webrenewal/products/inductor/chip/tokoproducts/wirewoundmetalalloychiptype/m_dfe201610p.ashx")
	(tags "Inductor power chip flatwire")
	(property "Reference" "L1"
		(at 0 -1.8 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "d65972fd-ab50-4905-b5d0-86fd63b39a75")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "1uH"
		(at 0 1.8 0)
		(layer "F.Fab")
		(uuid "c5cb99a2-dde6-4965-aaf0-06b27816f1da")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Inductor_SMD:L_Murata_DFE201610P"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "aeb0b40e-89a7-46cd-8546-4dd80ea6cf13")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2ad96378-e8a2-4482-a9a5-ef0ae0402362")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "eb1b3314-db28-4898-9ffe-f846e6ac98a2")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "MFG" "Murata"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e9969b31-dddd-4eca-89f3-477d376b4597")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "DFE201612PD-1R0M=P2"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "04c9e72c-5cff-4801-b0b4-a882bab04bca")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C2043195"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8cbf846b-f54a-4886-b065-7e1db0b14f4e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.26 -1.06)
		(end 1.26 -1.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "812c30f5-7cd2-46a9-8c9c-23dcb44900ed")
	)
	(fp_line
		(start -1.26 1.06)
		(end 1.26 1.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "97faf7d8-1d59-40b3-b89d-1b30cc7e3a67")
	)
	(fp_line
		(start -1.25 -1.050001)
		(end -1.25 1.050001)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1a31a27c-20d4-4526-861e-13bccde06750")
	)
	(fp_line
		(start -1.25 1.050001)
		(end 1.25 1.050001)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b59118fc-e85c-463f-8aff-88c0ce40d3bb")
	)
	(fp_line
		(start 1.25 -1.050001)
		(end -1.25 -1.050001)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fa247c76-4920-4fe6-a4a4-9e1d5888e585")
	)
	(fp_line
		(start 1.25 1.050001)
		(end 1.25 -1.050001)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b50266d6-9f2b-43a1-8dd0-38586b9b1378")
	)
	(fp_line
		(start -1 -0.8)
		(end -1 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5b7e69f2-8ad7-47ab-871b-890310800a05")
	)
	(fp_line
		(start -1 0.8)
		(end 1 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "687495c3-3db0-419e-bb3e-14256b3f9860")
	)
	(fp_line
		(start 1 -0.8)
		(end -1 -0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3f224f96-3f5a-4b8f-99bd-c880375fb370")
	)
	(fp_line
		(start 1 0.8)
		(end 1 -0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "68e37f57-f3f9-4620-96d4-81aa3911d05d")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "4d4933dd-fe8b-4fdb-bb68-35f21889bb85")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(pad "1" smd rect
		(at -0.724999 0)
		(size 0.55 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "dd6b34b6-d168-4fac-8121-c6edbfa39324")
	)
	(pad "2" smd rect
		(at 0.724999 0)
		(size 0.55 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "7ec03650-0f8a-45a4-b4f7-6a25445c9ff1")
	)
	(model "${KICAD7_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Cenker_CKCS201610.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)