(module Prog_5P_Edge_Castellations (layer F.Cu) (tedit 5527AC48)
  (solder_mask_margin -0.1)
  (attr virtual)
  (fp_text reference REF** (at -3 0 90) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value Prog_5P_Edge_Castellations (at -2 0 90) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user CASTELLATIONS (at -1 0 90) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user GND (at 1.5 2) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user SIO (at 1.5 1) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user CLK (at 1.5 0) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user RST (at 1.5 -1) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user VCC (at 1.5 -2) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start 0 -2.5) (end 0 2.5) (layer F.Fab) (width 0.05))
  (pad 1 thru_hole rect (at 0 -2) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad 2 thru_hole circle (at 0 -1) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad 3 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad 4 thru_hole circle (at 0 1) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad 5 thru_hole circle (at 0 2) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask))
)
