(footprint "SMD Nut M2.5 x 6.5 SMTSO2565"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "H6"
		(at 0 -7.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "9d15cb5e-fb0e-4965-8bf7-65e9b66cb902")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "M2.5"
		(at 0 -6 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5f61b5f5-8e87-4126-b8cc-4c94808a1cce")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Hardware:SMD Nut M2.5 x 6.5 SMTSO2565"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8c750dde-ae41-4a2f-ae88-e563ff98a74e")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "01b34f33-a12b-4d1b-9a0b-1a0b1a1e6cf3")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a772f2fa-9fed-4fa9-9882-7eba378fac1b")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "LCSC" "C2916327"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6b30c18e-2162-46e8-bf73-a1887c1541f8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "Sinhoo"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "dc686011-79d1-4656-8730-9c4490cef4df")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "SMTSO2565CTJ"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bee913e5-2da7-4d77-9f99-77311cb3bdf8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Enable" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f037d2a2-2147-4678-83e8-06fe7830b5e4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_arc
		(start -2.533845 0.788749)
		(mid -2.653741 -0.012456)
		(end -2.526329 -0.8125)
		(stroke
			(width 0.9)
			(type default)
		)
		(layer "F.Paste")
		(uuid "898f56eb-c0a0-4abc-8a25-76ca014c1dd6")
	)
	(fp_arc
		(start -1.95 -1.8)
		(mid -1.316084 -2.304435)
		(end -0.559519 -2.594115)
		(stroke
			(width 0.9)
			(type default)
		)
		(layer "F.Paste")
		(uuid "201956ce-ca90-45b4-835f-799d30275276")
	)
	(fp_arc
		(start -0.583845 2.588749)
		(mid -1.337657 2.291979)
		(end -1.96681 1.781615)
		(stroke
			(width 0.9)
			(type default)
		)
		(layer "F.Paste")
		(uuid "59502c9a-735a-415a-995a-2e61fcb6f5ca")
	)
	(fp_arc
		(start 0.583845 -2.588749)
		(mid 1.337657 -2.291979)
		(end 1.96681 -1.781615)
		(stroke
			(width 0.9)
			(type default)
		)
		(layer "F.Paste")
		(uuid "8f06378d-c2ec-4940-b62c-660c29068d59")
	)
	(fp_arc
		(start 1.95 1.8)
		(mid 1.316085 2.304437)
		(end 0.559519 2.594115)
		(stroke
			(width 0.9)
			(type default)
		)
		(layer "F.Paste")
		(uuid "dba4acc1-f47e-41be-812d-c1917a9d93e3")
	)
	(fp_arc
		(start 2.533845 -0.788749)
		(mid 2.65374 0.012456)
		(end 2.526329 0.8125)
		(stroke
			(width 0.9)
			(type default)
		)
		(layer "F.Paste")
		(uuid "6a8452d8-70aa-4eb6-8534-5e5d4bec570e")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -4.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f0e1ad14-a81e-4d85-9377-4ffb8a991659")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 4.52 4.52)
		(drill 4.22)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
		(uuid "6b16db09-c2ef-4f68-9059-c244485ea02b")
	)
	(pad "1" smd circle
		(at 0 0)
		(size 6.2 6.2)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(uuid "34aab146-5d08-49a0-aad7-53296b7c7a13")
	)
	(model ":KICAD7_3DMODEL_DIR:Hardware.3dshapes/Nut [SMTSO] [M2.5 x 6.5].step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)