(footprint "2P_7.25x7.25_P7.75" (version 20210108) (generator pcbnew) (layer "F.Cu")
  (tedit 6006BBA9)
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at -8.25 0 90 unlocked) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp e532beb8-b8f4-4e57-a25b-dee4151ccb15)
  )
  (fp_text value "2P_7.25x7.25_P7.75" (at -6.5 0 90 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 697b426b-6744-4a91-89c9-402af8d139fe)
  )
  (fp_text user "${REF}" (at -5 0 90 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 35443dcc-db76-4939-8abf-a6aaa9d05548)
  )
  (pad "1" connect rect (at -3.875 0) (size 7.25 7.25) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp 89c54630-3dff-4b5a-9151-78e8efd0a1cc))
  (pad "2" connect rect (at 3.875 0) (size 7.25 7.25) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp 655a3f10-f337-4d9c-bd51-bbe3a3b2a1ee))
)
