(module Bridge_Rectifier_30x4.6 (layer F.Cu) (tedit 5944BE45)
  (solder_mask_margin -0.05)
  (fp_text reference REF** (at 0 0.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Bridge_Rectifier_30x4.6 (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -15 0) (end -15 4.6) (layer F.Fab) (width 0.05))
  (fp_line (start -15 4.6) (end 15 4.6) (layer F.Fab) (width 0.05))
  (fp_line (start 15 4.6) (end 15 0) (layer F.Fab) (width 0.05))
  (fp_line (start 15 0) (end -15 0) (layer F.Fab) (width 0.05))
  (fp_line (start -15 3.6) (end 15 3.6) (layer F.Fab) (width 0.05))
  (fp_line (start -1.6 3.6) (end -1.6 0) (layer F.Fab) (width 0.05))
  (fp_line (start 1.6 3.6) (end 1.6 0) (layer F.Fab) (width 0.05))
  (pad + thru_hole circle (at -12.5 3) (size 1.7 1.7) (drill 1.4) (layers *.Cu F.Mask))
  (pad A+ thru_hole circle (at -2.5 3) (size 1.7 1.7) (drill 1.4) (layers *.Cu F.Mask))
  (pad A- thru_hole circle (at 5 3) (size 1.7 1.7) (drill 1.4) (layers *.Cu F.Mask))
  (pad - thru_hole circle (at 12.5 3) (size 1.7 1.7) (drill 1.4) (layers *.Cu F.Mask))
  (pad + connect roundrect (at -12.5 3) (size 2 2.7) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad A+ connect roundrect (at -2.5 3) (size 2 2.7) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad A- connect roundrect (at 5 3) (size 2 2.7) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad - connect roundrect (at 12.5 3) (size 2 2.7) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad + connect roundrect (at -12.5 3) (size 2.7 0.8) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad A+ connect roundrect (at -2.5 3) (size 2.7 0.8) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad A- connect roundrect (at 5 3) (size 2.7 0.8) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad - connect roundrect (at 12.5 3) (size 2.7 0.8) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (model Diode_THT.3dshapes/Bridge_Rectifier_30x4.6.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
