(footprint "Omron_D2F"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "SW5"
		(at 0 -3.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "dffd96b8-e75d-43d6-b0f1-e87e23f006f8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Middle-click"
		(at 0 2 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "d5d063ed-4e4e-4d34-a273-ff40c1c87036")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Button_Switch_THT:Omron_D2F"
		(at -0.05 -13.4 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "70631641-2c4c-4b1d-bd14-a54ee45e48d8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at -0.05 -13.4 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4dd86022-32e2-4dce-9fe9-23ddcaa4eb53")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Switch, single pole double throw"
		(at -0.05 -13.4 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "88a429b8-a44f-4b14-a7de-9cc7e5f5aece")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C5157566"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "28f519fd-6fe8-4b04-b286-25089d282f8b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "Omron Electronics"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d0fe8f93-889f-4768-9b3c-09a020200298")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "D2FC-F-7N(20M)"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0813e3d6-9d3b-493d-852b-9b8199af19be")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -6.4 -2.9)
		(end -6.4 -1.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3f6ace53-56b6-43df-b805-9dc954d7ddac")
	)
	(fp_line
		(start -6.4 -2.9)
		(end -5.4 -2.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "57f84154-edf0-4bd1-a1e8-f520afa6d4c8")
	)
	(fp_line
		(start -6.4 2.9)
		(end -6.4 1.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8b9ccd3f-80b1-44b1-9941-9ecaa1628948")
	)
	(fp_line
		(start -6.4 2.9)
		(end -5.4 2.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c98df619-a45e-4f24-a394-0924f1ab1b23")
	)
	(fp_line
		(start 6.4 -2.9)
		(end 5.4 -2.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f0820ceb-0586-4d4a-96e0-248aefe293cf")
	)
	(fp_line
		(start 6.4 -2.9)
		(end 6.4 -1.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5c8739ad-62bf-4dfd-9a31-e43efdd2a018")
	)
	(fp_line
		(start 6.4 2.9)
		(end 5.4 2.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "bf3077d8-43c7-4789-a20a-74816196e858")
	)
	(fp_line
		(start 6.4 2.9)
		(end 6.4 1.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "dc9e808d-0ddb-4450-ab2a-839e0a4ec5ac")
	)
	(fp_line
		(start -6.9 -2.9)
		(end -6.9 2.9)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d2a3e2b2-b408-4e9c-a8c8-af58a6e6f8aa")
	)
	(fp_line
		(start -6.4 3.4)
		(end 6.4 3.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "fdb80328-1f89-4b12-8e33-1d480aa67579")
	)
	(fp_line
		(start 6.4 -3.4)
		(end -6.4 -3.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e44f5b33-f82f-4378-b051-4512a486e2a7")
	)
	(fp_line
		(start 6.9 2.9)
		(end 6.9 -2.9)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ba8f87cb-3255-408d-867d-289c9e3131ef")
	)
	(fp_arc
		(start -6.9 -2.9)
		(mid -6.753553 -3.253553)
		(end -6.4 -3.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "fddcdf28-7701-479a-9ffd-48472246fa45")
	)
	(fp_arc
		(start -6.4 3.4)
		(mid -6.753553 3.253553)
		(end -6.9 2.9)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "429d2601-fcde-4110-b214-65526eece99b")
	)
	(fp_arc
		(start 6.4 -3.4)
		(mid 6.753553 -3.253553)
		(end 6.9 -2.9)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "89c8e641-193b-4b71-bed8-bc4da8e84fa0")
	)
	(fp_arc
		(start 6.9 2.9)
		(mid 6.753553 3.253553)
		(end 6.4 3.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4213e8ce-1a6c-4ff7-8924-33e8e3295aa6")
	)
	(fp_line
		(start -1.95 -1.45)
		(end -1.95 1.45)
		(stroke
			(width 0.1)
			(type dash)
		)
		(layer "F.Fab")
		(uuid "18ef9e9d-06b2-47b7-897d-a45935d07be9")
	)
	(fp_rect
		(start -6.4 -2.9)
		(end 6.4 2.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "d978e5c6-3ade-4dc8-b7c4-72fc4192761c")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "6fda8034-8a3b-4eea-a6e8-51891dc2dd1e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 5.08 0)
		(size 1.5 1.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "28328f27-d69e-4cb9-b766-34a095610ff7")
	)
	(pad "1" smd circle
		(at 5.08 0)
		(size 2.2 2.2)
		(layers "B.Cu" "B.Paste" "B.Mask")
		(uuid "8fad8ea4-ec39-4ed3-a643-907c4f4ad0f2")
	)
	(pad "2" thru_hole circle
		(at -5.08 0)
		(size 1.5 1.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0202f822-1d5d-45d0-a68c-1fb36a9db952")
	)
	(pad "2" smd circle
		(at -5.08 0)
		(size 2.2 2.2)
		(layers "B.Cu" "B.Paste" "B.Mask")
		(uuid "83c507ff-1cab-46cc-974a-88f5188251b1")
	)
	(pad "3" thru_hole circle
		(at 0 0)
		(size 1.5 1.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "74809bc4-129d-40b8-ba10-f72b9eab5449")
	)
	(pad "3" smd circle
		(at 0 0)
		(size 2.2 2.2)
		(layers "B.Cu" "B.Paste" "B.Mask")
		(uuid "262ad6fb-edf2-4b85-9948-72d555e2d462")
	)
	(model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/Omron D2FC-F-7N.step"
		(offset
			(xyz 6.4 -2.9 0.525)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 -90)
		)
	)
)
