(footprint "2P_7.3x7.3_P8.3" (version 20210108) (generator pcbnew) (layer "F.Cu")
  (tedit 6006D90C)
  (property "MPN" "NO PART")
  (property "Sheet file" "BrushedMotorController18V15A.kicad_sch")
  (property "Sheet name" "")
  (attr exclude_from_pos_files)
  (fp_text reference "M1" (at -8.6 0 90 unlocked) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 94c994e4-3704-4e9e-b097-8ec9a3670d1f)
  )
  (fp_text value "MOTOR" (at -6.5 0 90 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4519ba4e-3b32-4158-956d-186a10dec6f2)
  )
  (fp_text user "${REF}" (at -5 0 90 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6df94124-5e21-45ad-b9f5-dc4fddf41669)
  )
  (pad "1" connect rect (at -4.15 0) (size 7.3 7.3) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp 7d34d2f2-0124-48c5-b133-22ba366f4c9a))
  (pad "2" connect rect (at 4.15 0) (size 7.3 7.3) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp e39d622e-9d09-452a-ab15-015a025f0d59))
)
