(footprint "TSOT-23-8"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "TSOT, 8 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant BA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "TSOT TO_SOT_SMD")
	(property "Reference" "B1B_U2"
		(at 0 -2.2 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "6c726f7d-d618-4392-b58a-3167fee7526b")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "INA241A3QDDFRQ1"
		(at 0.525 0 -90)
		(layer "F.Fab")
		(uuid "0d3c424f-61b5-49ac-9f63-830a90250b53")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.0625)
			)
		)
	)
	(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-8"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "159cebe8-880c-4bff-b3a5-d10341cf558c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina241a-q1.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9966b2b1-c59e-4c18-ac22-7f91cece7ad4")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f32bfda4-6650-42fc-a22f-9b45ec71499f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C6051859"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "c1264fc8-5d0e-4eac-a02a-a551b7a8374d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "TI"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "2a8709f2-cab3-4f49-80be-46629a75bf9e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "INA241A3QDDFRQ1"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "042ea65e-04ab-46b2-95db-b701b27ce8f8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Preferred" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "53b949c9-1bc6-42cb-8a1d-1811413f0b74")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9551312d-7183-4bc7-a1e8-98080748b6df")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -0.8 -1.65)
		(end 0.8 -1.5)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "66c0595e-4b36-47e9-8c09-fc989b025e54")
	)
	(fp_rect
		(start -0.8 1.5)
		(end 0.8 1.65)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "2c4d229a-7921-41e7-ae4e-89189fdb13f5")
	)
	(fp_poly
		(pts
			(xy -1.75 -0.975) (xy -1.95 -1.15) (xy -1.95 -0.8)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "d3f9eb17-1c37-4e81-9802-40a4a3ea7919")
	)
	(fp_line
		(start -1.799999 1.1)
		(end -1.799999 -1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ec20efba-f2ae-4028-b691-db1300326a6a")
	)
	(fp_line
		(start -1.55 -1.35)
		(end -1.05 -1.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5159c110-3e15-4553-95df-8558df607f07")
	)
	(fp_line
		(start -1.55 1.35)
		(end -1.05 1.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4a72181a-6971-4043-94f2-135a4fcd7447")
	)
	(fp_line
		(start -1.05 -1.35)
		(end -1.05 -1.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "81f231a1-600a-4539-af89-fd6d54022406")
	)
	(fp_line
		(start -1.05 1.35)
		(end -1.05 1.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c459fc05-4048-44c2-b2e2-c29a2facec7e")
	)
	(fp_line
		(start -0.8 1.7)
		(end 0.8 1.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9d798adc-ae0c-40a6-9e89-f6b60078243f")
	)
	(fp_line
		(start 0.8 -1.7)
		(end -0.8 -1.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "57cabd30-333c-46b1-afa6-ae69c7e25112")
	)
	(fp_line
		(start 1.05 -1.35)
		(end 1.05 -1.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b52f9024-845b-48ff-8200-3dc366d69faf")
	)
	(fp_line
		(start 1.05 1.35)
		(end 1.05 1.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b67e8fc4-e894-471a-9638-b81e52a72ebf")
	)
	(fp_line
		(start 1.55 -1.35)
		(end 1.05 -1.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e9d0d1bf-ac2f-41ec-b740-000176a2f99d")
	)
	(fp_line
		(start 1.55 1.35)
		(end 1.05 1.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a819a3ec-588e-45d5-8cf4-e905cd41200f")
	)
	(fp_line
		(start 1.799999 -1.1)
		(end 1.799999 1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8830e094-450a-4487-91b1-8ea0f1a8e2d8")
	)
	(fp_arc
		(start -1.799999 -1.1)
		(mid -1.726777 -1.276777)
		(end -1.55 -1.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ca0fdd34-c3fb-4f8b-8d50-502a73987078")
	)
	(fp_arc
		(start -1.55 1.35)
		(mid -1.726776 1.276776)
		(end -1.799999 1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3510f333-37d2-4338-a854-c4a591e41768")
	)
	(fp_arc
		(start -1.05 -1.45)
		(mid -0.976778 -1.626778)
		(end -0.8 -1.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "84347aab-c123-41a8-bc4d-575992b198f7")
	)
	(fp_arc
		(start -0.8 1.7)
		(mid -0.976777 1.626777)
		(end -1.05 1.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2bc33b9d-167a-4ebc-8d2a-ddff58633eb2")
	)
	(fp_arc
		(start 0.8 -1.7)
		(mid 0.976777 -1.626777)
		(end 1.05 -1.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6b4b6446-fee3-4d5d-9deb-321d59bef975")
	)
	(fp_arc
		(start 1.05 1.45)
		(mid 0.976777 1.626777)
		(end 0.8 1.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bbac3094-e2f7-4669-8282-9adf160cf7f0")
	)
	(fp_arc
		(start 1.55 -1.35)
		(mid 1.726777 -1.276777)
		(end 1.799999 -1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3aeb10b0-70ff-4fa5-a179-9cc9423a225b")
	)
	(fp_arc
		(start 1.799999 1.1)
		(mid 1.726776 1.276776)
		(end 1.55 1.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "50b9684f-56e7-4b9d-b171-5c275c809da3")
	)
	(fp_line
		(start -0.8 -1.45)
		(end 0.8 -1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ab30e7f8-3f9e-4bae-89e6-1712f9b6eece")
	)
	(fp_line
		(start -0.8 -1.050001)
		(end -0.4 -1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "067cfff7-6359-4862-b9c8-3e4f99aa7869")
	)
	(fp_line
		(start -0.8 1.45)
		(end -0.8 -1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "176293e6-7eba-471f-9094-ba69f9ebc396")
	)
	(fp_line
		(start 0.8 -1.45)
		(end 0.8 1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7e4a7e00-1bb8-42f9-8ca4-ba18fc32a8fb")
	)
	(fp_line
		(start 0.8 1.45)
		(end -0.8 1.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "bda3ca4d-66c9-4206-aa77-39aa3ff69321")
	)
	(fp_text user "${REFERENCE}"
		(at -0.475 0 -90)
		(layer "F.Fab")
		(uuid "bf02e429-1af6-4a0d-aa72-c14cc5197496")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.06)
			)
		)
	)
	(pad "" smd oval
		(at -1.25 -0.975)
		(size 0.7 0.35)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b86a67e3-ef3f-4f84-b43e-1914fd11ec38")
	)
	(pad "" smd oval
		(at -1.25 -0.325)
		(size 0.7 0.35)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "87669f5c-0196-4e25-a4d0-9e2e16a237da")
	)
	(pad "" smd oval
		(at -1.25 0.325)
		(size 0.7 0.35)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "53a62459-997c-4373-b28f-51283627beec")
	)
	(pad "" smd oval
		(at -1.25 0.975)
		(size 0.7 0.35)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4264c6c0-c4cc-4ff4-a44b-2c3b7d67e854")
	)
	(pad "" smd oval
		(at 1.25 -0.975)
		(size 0.7 0.35)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8b96597b-ccbd-49e2-8298-e56ae0639410")
	)
	(pad "" smd oval
		(at 1.25 -0.325)
		(size 0.7 0.35)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "08046363-8e63-4c83-b5b9-67bf53649c1e")
	)
	(pad "" smd oval
		(at 1.25 0.325)
		(size 0.7 0.35)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "557ff15e-fd5e-44f8-815e-2f7e616201bd")
	)
	(pad "" smd oval
		(at 1.25 0.975)
		(size 0.7 0.35)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f443a494-57fe-4d05-bdb9-953d1e0a233d")
	)
	(pad "1" smd roundrect
		(at -1.25 -0.975)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2222222222)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "59b28224-5cd7-4c97-ae16-db22ecb33e43")
	)
	(pad "2" smd roundrect
		(at -1.25 -0.325)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2222222222)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "16664853-8b08-4ca3-8411-55ff2c79cc72")
	)
	(pad "3" smd roundrect
		(at -1.25 0.325)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2222222222)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b80e2d50-4814-4609-881f-fbd0288efe9c")
	)
	(pad "4" smd roundrect
		(at -1.25 0.975)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2222222222)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "eac76281-8fef-4148-9852-d72975bfdaf7")
	)
	(pad "5" smd roundrect
		(at 1.25 0.975)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2222222222)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "df633f92-efc1-4e35-9734-02bdcdb1edc1")
	)
	(pad "6" smd roundrect
		(at 1.25 0.325)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2222222222)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "01a1047a-4f3e-47ab-8fb3-fc907ef2223e")
	)
	(pad "7" smd roundrect
		(at 1.25 -0.325)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2222222222)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "6b30be1a-14ec-47fd-93c9-64003318e2ca")
	)
	(pad "8" smd roundrect
		(at 1.25 -0.975)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2222222222)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8f43aec6-c953-4159-b6f2-330abc1cce97")
	)
	(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-8.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
