(footprint "U.FL_Molex_MCRF_73412-0110_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Molex Microcoaxial RF Connectors (MCRF), mates Hirose U.FL, (http://www.molex.com/pdm_docs/sd/734120110_sd.pdf)")
  (tags "mcrf hirose ufl u.fl microcoaxial")
  (property "Field2" "")
  (property "Sheetfile" "Flight Controller.kicad_sch")
  (property "Sheetname" "Flight Controller")
  (attr smd)
  (fp_text reference "ANT1" (at 0 2.75 180) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp cbcca571-0db7-4612-9cdf-965b290b28da)
  )
  (fp_text value "Antenna_PCB_type" (at -2.35 -1.85 180) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 5ac3f9b8-c774-4da8-a035-3cfb621d5cc7)
  )
  (fp_text user "${REFERENCE}" (at -2.2 1.85 180) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 267d3ab0-1a27-4adb-b158-c510c4f0aae3)
  )
  (fp_line (start -1.5 -1.5) (end -0.7 -1.5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b515b3f2-8639-4db9-8f8a-8ca7056a1e8d))
  (fp_line (start -1.5 -1.3) (end -1.5 -1.5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 12ed22ee-7628-4eee-8b75-66be32095af4))
  (fp_line (start -1.3 1.5) (end -1.5 1.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e240f99c-f3a2-4331-adf3-69101d8b1630))
  (fp_line (start -0.7 1.5) (end -1.3 1.5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0f705af0-7f0f-4fe2-93f8-c37e0c63785f))
  (fp_line (start -0.7 1.5) (end -0.7 2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2d481944-1be3-4973-951b-720c1997f2ea))
  (fp_line (start 0.7 -1.5) (end 1.5 -1.5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 289f4258-dee3-4ffa-b3e5-7978f136704a))
  (fp_line (start 0.7 1.5) (end 0.7 2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8e9e800f-5cc1-4a22-8b67-908b8ebfe940))
  (fp_line (start 1.5 -1.5) (end 1.5 -1.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6cff136a-02d6-41f1-a14b-e7c00a8fa26b))
  (fp_line (start 1.5 1.3) (end 1.5 1.5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ea952d22-9e74-49db-a92c-a17cadd9d1de))
  (fp_line (start 1.5 1.5) (end 0.7 1.5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a70b4815-9a51-477e-a0c8-5fa66b047190))
  (fp_line (start -2.25 1.1) (end -2.25 -1.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ed822867-94b3-4da5-a6f4-c871bab3fb36))
  (fp_line (start -1.75 -1.35) (end -2 -1.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp dc1f4d6f-1f5c-4da3-8e35-b62f25cb8403))
  (fp_line (start -1.75 1.35) (end -2 1.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 73dcacfd-1a8b-444a-bfc4-697641ed634b))
  (fp_line (start -0.75 -2) (end -0.75 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c98ea5ef-ea14-408a-835d-7ccebd8a448e))
  (fp_line (start -0.75 -1.8) (end -1.3 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3746b25c-f7c7-4cbb-a478-12f04f1ec7d2))
  (fp_line (start -0.75 1.8) (end -1.3 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 11ddc261-ff6c-4829-8ff8-9d5f558903c7))
  (fp_line (start -0.75 2) (end -0.75 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 22a1628a-edac-4c64-81a3-cabb4a4247e2))
  (fp_line (start -0.5 -2.25) (end 0.5 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 933926f2-746a-4acb-ba4f-c5b3fc6955e6))
  (fp_line (start 0.5 2.25) (end -0.5 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2033258d-8c9d-42f1-b3b8-282ece3624b6))
  (fp_line (start 0.75 -2) (end 0.75 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 29975a2d-df43-4153-bf67-0f2b2551920b))
  (fp_line (start 0.75 -1.8) (end 1.3 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b608413b-f9fc-4c53-b0f0-949a9cc2f859))
  (fp_line (start 0.75 1.8) (end 1.3 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 39eb019f-1764-44fe-96eb-42b982b47032))
  (fp_line (start 0.75 2) (end 0.75 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4aac6394-f590-4b10-b669-336e0cd1022e))
  (fp_line (start 1.75 -1.35) (end 2 -1.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0076cc1d-aa5e-4fd2-b599-eaf02935f4dc))
  (fp_line (start 1.75 1.35) (end 2 1.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 87c5ed03-87a7-4a60-9caa-4c91ba1ed144))
  (fp_line (start 2.25 -1.1) (end 2.25 1.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f99f0a49-02f1-4d0b-b2ac-61abc05477a7))
  (fp_arc (start -2.25 -1.1) (mid -2.176777 -1.276777) (end -2 -1.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f60b0b80-0b05-4bde-a19d-894e981aeb79))
  (fp_arc (start -2 1.35) (mid -2.176777 1.276777) (end -2.25 1.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9e65864c-1a98-481b-b312-a43211518e9d))
  (fp_arc (start -1.75 -1.35) (mid -1.618198 -1.668198) (end -1.3 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e645ab03-c7de-4783-9a8f-59b229e23fb9))
  (fp_arc (start -1.3 1.8) (mid -1.618198 1.668198) (end -1.75 1.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 975bee71-38b8-4b46-a87c-e53e0de81904))
  (fp_arc (start -0.75 -2) (mid -0.676777 -2.176777) (end -0.5 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9ede1edd-c84b-49ec-a28f-6f715306374f))
  (fp_arc (start -0.5 2.25) (mid -0.676777 2.176777) (end -0.75 2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1078d789-832f-49c7-a2f0-600ea38e79dc))
  (fp_arc (start 0.5 -2.25) (mid 0.676777 -2.176777) (end 0.75 -2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b1be6f02-d4b0-4624-982a-173c85a688ef))
  (fp_arc (start 0.75 2) (mid 0.676777 2.176777) (end 0.5 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4351685d-7834-404f-898b-11082dc99f27))
  (fp_arc (start 1.3 -1.8) (mid 1.618198 -1.668198) (end 1.75 -1.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp eb25e296-39e5-41b7-9737-cd2524bc439e))
  (fp_arc (start 1.75 1.35) (mid 1.618198 1.668198) (end 1.3 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c0a47608-6a68-4741-8c54-92fcf2de5202))
  (fp_arc (start 2 -1.35) (mid 2.176777 -1.276777) (end 2.25 -1.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9863b8f2-6d49-411e-839a-eb8e8b5d2b3a))
  (fp_arc (start 2.25 1.1) (mid 2.176777 1.276777) (end 2 1.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f97bfc15-2580-4cac-9567-cf390b982934))
  (fp_line (start -1.3 -1.3) (end -1.3 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a12369a4-1d52-4fd8-90d2-ad8e2385fc88))
  (fp_line (start -1.3 -1.3) (end 1.3 -1.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7009de8c-3ebf-49b8-bc76-2a1bd9878367))
  (fp_line (start -1.3 1) (end -1 1.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ef2156d9-b08d-401e-a8ab-1a83b5a96b11))
  (fp_line (start -1 1.3) (end 1.3 1.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 358de4b4-df1c-455d-9fc8-56e876f908b9))
  (fp_line (start -0.3 1.3) (end 0 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c76bc814-7900-46ee-9bdc-a971179526bb))
  (fp_line (start 0 1) (end 0.3 1.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 20874053-85bb-41c5-a4da-bc1e07184d96))
  (fp_line (start 1.3 -1.3) (end 1.3 1.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a6157d45-377e-4960-97c6-ab5da4aff098))
  (fp_circle (center 0 0) (end 0 0.05)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 4228b33e-3aec-409d-b07e-eee870c9cadd))
  (fp_circle (center 0 0) (end 0 0.125)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp b005de2c-906a-4329-8f29-c5182a22a6d2))
  (fp_circle (center 0 0) (end 0 0.2)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 1fe45746-ba10-4e85-a92f-a7bce963308d))
  (fp_circle (center 0 0) (end 0.9 0)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 028e2a29-a8c4-4cff-9f91-d77c09911aec))
  (pad "1" smd rect (at 0 1.5) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 2259dfe8-f0e1-498f-9d4a-346bfe9f9f8e))
  (pad "2" smd rect (at -1.475 0) (size 1.05 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 162045a8-abf6-4f16-8181-6ffd5f67cc53))
  (pad "2" smd rect (at 0 -1.5) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 70ee2299-7c68-47b1-8ad9-d8d6844c0d07))
  (pad "2" smd rect (at 1.475 0) (size 1.05 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ee45b89f-c8bf-40b1-8e03-cf184f4c0959))
  (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/U.FL_Molex_MCRF_73412-0110_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ":KICAD7_3DMODEL_DIR:Connector_Coaxial.3dshapes/734120110.stp"
    (offset (xyz 0 0 1.25))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 180))
  )
)
