(footprint "JST_XH_B5B-XH-AM_1x05_P2.50mm_Vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "JST XH series connector, B5B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST XH vertical boss")
	(property "Reference" "J1"
		(at 5 -3.55 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "e46a0aa7-e668-4487-9bc1-5bf91eb196a3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Display"
		(at 5 4.6 180)
		(layer "F.Fab")
		(uuid "9514058d-7057-4046-9a64-2b62da51b06a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_JST:JST_XH_B5B-XH-AM_1x05_P2.50mm_Vertical"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "88e3cc2c-0a9a-421e-855d-d4b93491b954")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "921c0720-d4fb-4698-8fda-dd519c9d2bd9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "1x5P 5P XH 1 2.5mm 5 Plugin,P=2.5mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1d4f9568-3175-4c68-bfb7-c05c4198b24e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Enable" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6912e976-6284-458f-b858-cf9b01a30750")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "USD_per_1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "59ba3173-a874-409b-927a-34abcb0246ca")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "USD_per_1000" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9cade87f-2f97-493d-821e-2b9239fb6368")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C2318"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8bd6138b-8674-47ac-8294-b323fb139765")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "BOOMELE(Boom Precision Elec)"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bec75ced-d2ee-4db5-a6c6-b5d5c44af42b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "XH-5A"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "114f77b8-eee7-497a-9ea3-752100462de1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLCPCB_PreferredPart" "N"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "061211a9-5716-4627-bb0d-5401ac78b676")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLCPCB_StandardOnly" "N"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "475c1f96-f7e9-44be-bfdc-0ef2dfcc7bdf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -2.85 -2.75)
		(end -2.85 -1.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4603a017-61d0-409c-ab1c-8d71e159d1d9")
	)
	(fp_line
		(start -2.56 -2.46)
		(end -2.56 3.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8d6b1ba8-12de-4daf-94fe-76d76488fa45")
	)
	(fp_line
		(start -2.56 3.51)
		(end 12.56 3.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4d37a2da-1061-4ce9-9aa3-7099eadb206a")
	)
	(fp_line
		(start -2.55 -2.45)
		(end -2.55 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "04126570-915a-42ce-8598-6f97791e1253")
	)
	(fp_line
		(start -2.55 -1.7)
		(end -0.750001 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "13684470-35a2-40f1-95ab-0abba8e5bad9")
	)
	(fp_line
		(start -2.55 -0.2)
		(end -1.8 -0.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "27ed411f-0f2c-426b-b9c6-34f215fbbe4a")
	)
	(fp_line
		(start -1.8 -0.2)
		(end -1.8 1.14)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "bf4b9ff6-9433-42e5-ba6e-57be29cfb2be")
	)
	(fp_line
		(start -1.6 -2.75)
		(end -2.85 -2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1864066c-65ea-4de5-81ff-556c9508bd75")
	)
	(fp_line
		(start -0.750001 -1.7)
		(end -0.75 -2.450001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f9e45ffa-c67a-4604-a804-e63d2bb8fc1f")
	)
	(fp_line
		(start -0.75 -2.450001)
		(end -2.55 -2.45)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d05e8f8e-cc58-4db6-962f-62c42c8a4ecf")
	)
	(fp_line
		(start 0.75 -2.450001)
		(end 0.750001 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e57a66a6-9205-40be-b68f-16ca703a9a9e")
	)
	(fp_line
		(start 0.750001 -1.7)
		(end 9.25 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "01d1a036-a1ef-425f-a9a4-3db4b770cae2")
	)
	(fp_line
		(start 5 2.75)
		(end -0.74 2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b8b06a52-f8d5-45b5-9c32-0603b292d180")
	)
	(fp_line
		(start 9.25 -2.45)
		(end 0.75 -2.450001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1c41bed3-ff0b-494d-aff5-8ef3bf4dc6fc")
	)
	(fp_line
		(start 9.25 -1.7)
		(end 9.25 -2.45)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "caafa5ea-1155-40f8-abe8-23c213e10afe")
	)
	(fp_line
		(start 10.749999 -1.7)
		(end 12.550001 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "17d016c4-3829-428a-9777-a9ee5e6643b3")
	)
	(fp_line
		(start 10.75 -2.450001)
		(end 10.749999 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "942b1676-d16e-454a-8897-698ea7062fee")
	)
	(fp_line
		(start 11.8 -0.199999)
		(end 11.8 2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1bd116db-b8de-47ef-ac38-c7a69a647b05")
	)
	(fp_line
		(start 11.8 2.75)
		(end 5 2.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a5a80b6d-685f-46a8-9e86-7d20db39097e")
	)
	(fp_line
		(start 12.55 -2.450001)
		(end 10.75 -2.450001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8bef71b1-ad64-4dda-a0c3-38c25f4428c0")
	)
	(fp_line
		(start 12.55 -0.199999)
		(end 11.8 -0.199999)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "628c6598-6339-4931-858d-7fe7a20acc18")
	)
	(fp_line
		(start 12.550001 -1.7)
		(end 12.55 -2.450001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e2e8c791-9c87-4ab4-91c1-55e15bf17964")
	)
	(fp_line
		(start 12.56 -2.46)
		(end -2.56 -2.46)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f0cdb783-8c1c-44e9-98ec-e7c9cfe63752")
	)
	(fp_line
		(start 12.56 3.51)
		(end 12.56 -2.46)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9f2408f1-478a-41dd-8c80-f87231c62f8f")
	)
	(fp_line
		(start -2.95 -2.85)
		(end -2.95 3.899999)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c22c8f25-74a2-4268-9e34-627561fdd10a")
	)
	(fp_line
		(start -2.95 3.899999)
		(end 12.95 3.9)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ab09e50c-87f7-4662-8f06-b4a4ea672870")
	)
	(fp_line
		(start 12.95 -2.85)
		(end -2.95 -2.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "53401c21-c41a-4e03-b4ca-909debc62829")
	)
	(fp_line
		(start 12.95 3.9)
		(end 12.95 -2.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1881e69d-d297-48fb-999d-ab2b195971c3")
	)
	(fp_line
		(start -2.450001 -2.35)
		(end -2.450001 3.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7318d2dd-ebb5-4978-a243-245083b052f3")
	)
	(fp_line
		(start -2.450001 3.4)
		(end 12.449999 3.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3ef72090-07b8-4fb3-b156-f84e9a5fb971")
	)
	(fp_line
		(start -0.625 -2.35)
		(end 0 -1.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "27bc5ac7-b793-4b90-a8c7-e55f6c80b5a2")
	)
	(fp_line
		(start 0 -1.35)
		(end 0.625 -2.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "80337967-f766-4f3e-8477-622a506a6353")
	)
	(fp_line
		(start 12.449999 -2.35)
		(end -2.450001 -2.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "845f2c39-0ed7-4bac-acbe-3950a65167ac")
	)
	(fp_line
		(start 12.449999 3.4)
		(end 12.449999 -2.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e04dad61-d35e-45b5-9d64-be56bdf72e33")
	)
	(fp_text user "${REFERENCE}"
		(at 5 2.7 180)
		(layer "F.Fab")
		(uuid "8380ccc9-f1c5-4302-9d57-dace3cbbf1f4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -1.6 2)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(uuid "c66f24cc-ac79-4a56-821b-4f45a7ba47c7")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.147059)
		(uuid "00fab432-56ac-46a4-b8e4-d14e5ae5924a")
	)
	(pad "2" thru_hole oval
		(at 2.5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "78948dc9-0bc9-4d36-b245-3ba771e6603d")
	)
	(pad "3" thru_hole oval
		(at 5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "df0450bc-9cee-4c41-a87e-5d5978b6c651")
	)
	(pad "4" thru_hole oval
		(at 7.5 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8b7baf7a-f5d6-40f3-816b-c2096e68a24e")
	)
	(pad "5" thru_hole oval
		(at 10 0)
		(size 1.7 1.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a55b80f3-56d5-4173-a83d-4496e72ae325")
	)
	(model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B05B-XH-A_1x05_P2.50mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
