(footprint "JST_SH_BM15B-SRSS-TB_1x15-1MP_P1.00mm_Vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(locked yes)
	(layer "F.Cu")
	(descr "JST SH series connector, BM15B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST SH side entry")
	(property "Reference" "J26"
		(at 0 -2.65 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "1affcad3-c392-4cb5-bf22-ad44618158f7")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "GPIO"
		(at 0 2.35 0)
		(layer "F.Fab")
		(uuid "d77a1ae1-3809-405c-bc0a-379ed993809d")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
		)
	)
	(property "Footprint" "Connector_JST:JST_SH_BM15B-SRSS-TB_1x15-1MP_P1.00mm_Vertical"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7e4347f4-55eb-4001-9f01-0f90ed17e05e")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e9be2bcc-b9b2-4fbe-9b43-c25e544d7d1b")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4b937177-6836-4517-8890-5e266cdd00ba")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "LCSC" "C7472245"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "b880f746-d774-4a1d-ad08-5d4eb2d3130f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "JST"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "5a7cc356-fbeb-42b5-9963-d44dfba3a261")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "BM15B-SRSS-TB"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "9714aae0-cbd0-4593-96e3-17a9969f1e62")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -8.61 -0.04)
		(end -8.61 1.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "15170889-43f6-4a94-8c70-e34c2b9ea1ad")
	)
	(fp_line
		(start -8.61 1.11)
		(end -7.56 1.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "471498b0-34cd-4542-8b57-4015172384d6")
	)
	(fp_line
		(start -7.56 1.11)
		(end -7.56 2.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cd37b5e3-38f4-40d8-8be1-63efffdccda2")
	)
	(fp_line
		(start -7.44 -2.01)
		(end 7.44 -2.01)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "bf3c49d1-2c2a-4d75-b1b5-27c37c5937d3")
	)
	(fp_line
		(start 8.61 -0.04)
		(end 8.61 1.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3e019927-dd59-4639-bc3a-5f6baab9fb79")
	)
	(fp_line
		(start 8.61 1.11)
		(end 7.56 1.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e5bff594-9cc1-4001-bd54-4dec625bfa40")
	)
	(fp_line
		(start -9.05 -1.85)
		(end -9.05 -0.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cd51387e-7189-40a2-a808-fe2183025160")
	)
	(fp_line
		(start -8.75 1)
		(end -8.747014 -0.136943)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "edc1f1db-b257-429c-9bb7-6f71bf4b2381")
	)
	(fp_line
		(start -8.65 -2.25)
		(end 8.65 -2.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "09de6342-b3e6-4c5c-84f5-e2b1963121bd")
	)
	(fp_line
		(start -8.5 1.25)
		(end -7.45 1.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "90b0b01c-7e7a-4a5c-9a55-5f94c924cd0b")
	)
	(fp_line
		(start -7.45 1.25)
		(end -7.45 1.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "078ae9dc-a18f-41d7-bd6d-ca1c7e7d3076")
	)
	(fp_line
		(start -7.15 2.25)
		(end 7.15 2.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "433062fd-4acc-42e2-9f30-7cd8164bcd0e")
	)
	(fp_line
		(start 7.45 1.25)
		(end 7.45 1.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0a05b0e5-58cc-492f-a6fa-721b492502bc")
	)
	(fp_line
		(start 8.5 1.25)
		(end 7.45 1.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0e7c798e-c3b1-4c05-a989-55e44d8e1147")
	)
	(fp_line
		(start 8.75 1)
		(end 8.747014 -0.136943)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cadfbe34-2d0f-4c08-ac44-7c412c6a1dbc")
	)
	(fp_line
		(start 9.05 -1.85)
		(end 9.05 -0.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "38182545-0fd7-4858-90a1-cf66021b1c63")
	)
	(fp_arc
		(start -9.05 -1.85)
		(mid -8.932843 -2.132843)
		(end -8.65 -2.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e2d97732-d66b-4ad1-93d5-1377bb31b984")
	)
	(fp_arc
		(start -8.747014 -0.136943)
		(mid -8.965282 -0.278835)
		(end -9.05 -0.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3f7d8c7a-ac07-41d3-89dd-973252580ee4")
	)
	(fp_arc
		(start -8.5 1.25)
		(mid -8.676777 1.176777)
		(end -8.75 1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "000bbc11-008d-48ef-ae86-f49d2545c770")
	)
	(fp_arc
		(start -7.15 2.25)
		(mid -7.362132 2.162132)
		(end -7.45 1.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2f5bed8b-a98e-4466-82f0-2226200cfc6e")
	)
	(fp_arc
		(start 7.45 1.95)
		(mid 7.362132 2.162132)
		(end 7.15 2.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "fd567cc2-d7cf-4d48-84bb-3503cb7cda29")
	)
	(fp_arc
		(start 8.65 -2.25)
		(mid 8.932843 -2.132843)
		(end 9.05 -1.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "446c3a77-d0d1-4380-80dc-728165589d64")
	)
	(fp_arc
		(start 8.75 1)
		(mid 8.676777 1.176777)
		(end 8.5 1.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8a6f7763-64c4-4126-b4dc-7aad485ca1d1")
	)
	(fp_arc
		(start 9.05 -0.525)
		(mid 8.965282 -0.278835)
		(end 8.747014 -0.136943)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "991051d8-7f88-4ae0-b3cf-aa2a7d50b359")
	)
	(fp_line
		(start -8.5 -1.9)
		(end 8.5 -1.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7d429a07-f621-45a5-88f1-af30a63002fa")
	)
	(fp_line
		(start -8.5 1)
		(end -8.5 -1.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8fb93952-5f17-4fd4-860a-bc5390b59994")
	)
	(fp_line
		(start -8.5 1)
		(end 8.5 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1759b5db-fb16-4226-ae8b-d75a25362e95")
	)
	(fp_line
		(start -7.5 1)
		(end -7 0.292893)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0d27e0c4-d649-4ef4-8078-c064cc58e020")
	)
	(fp_line
		(start -7.15 -1.55)
		(end -7.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b2a7d1db-d359-4721-bbb0-2f3e8b90e8e8")
	)
	(fp_line
		(start -7.15 -0.95)
		(end -6.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8e63645c-58e3-44bc-b572-59f1fcfb9d51")
	)
	(fp_line
		(start -7 0.292893)
		(end -6.5 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d3d35480-9886-4d1c-b1c4-d5ea3ff9cebe")
	)
	(fp_line
		(start -6.85 -1.55)
		(end -7.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a54c9a30-e6d3-4f43-ba3d-d40ed0ef4fde")
	)
	(fp_line
		(start -6.85 -0.95)
		(end -6.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d483e00c-256d-4476-9d03-4dc3051f9bbc")
	)
	(fp_line
		(start -6.15 -1.55)
		(end -6.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b546f25c-d66c-4ecf-a483-dabfbfff08f6")
	)
	(fp_line
		(start -6.15 -0.95)
		(end -5.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "60595aa5-57ea-4189-bafe-8db0b12e7ae1")
	)
	(fp_line
		(start -5.85 -1.55)
		(end -6.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "070ddd27-204e-4abf-8ca2-a715fe3949be")
	)
	(fp_line
		(start -5.85 -0.95)
		(end -5.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "66046380-7bf7-4971-97f4-619cc3764f77")
	)
	(fp_line
		(start -5.15 -1.55)
		(end -5.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3f4eca45-254a-4154-9ad5-dc0c29d2705e")
	)
	(fp_line
		(start -5.15 -0.95)
		(end -4.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a12446d3-abc1-40bf-9b00-1b941626280a")
	)
	(fp_line
		(start -4.85 -1.55)
		(end -5.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4329a381-98f5-4158-8c3c-3d7c798ce65c")
	)
	(fp_line
		(start -4.85 -0.95)
		(end -4.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1d389718-0c3b-4198-b638-f09b8f0f6de5")
	)
	(fp_line
		(start -4.15 -1.55)
		(end -4.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "75dcc3e1-839b-4e10-aafc-1238290f7289")
	)
	(fp_line
		(start -4.15 -0.95)
		(end -3.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "282e74b5-d869-498c-b22f-278ef69d73be")
	)
	(fp_line
		(start -3.85 -1.55)
		(end -4.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c6288491-9252-4a82-8396-5868c77d494d")
	)
	(fp_line
		(start -3.85 -0.95)
		(end -3.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c7313dd7-f2fe-4dca-8db6-02780b1d3ec2")
	)
	(fp_line
		(start -3.15 -1.55)
		(end -3.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "081c8580-8fae-409e-96b4-03b351442bb0")
	)
	(fp_line
		(start -3.15 -0.95)
		(end -2.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f44dc7df-1a8c-41d3-aaea-a1d975d7fafc")
	)
	(fp_line
		(start -2.85 -1.55)
		(end -3.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0853bc9b-6f6b-49d8-9f1d-d15aec5f4b54")
	)
	(fp_line
		(start -2.85 -0.95)
		(end -2.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c4c200c1-06aa-4e5b-be4c-1bd49680e6d2")
	)
	(fp_line
		(start -2.15 -1.55)
		(end -2.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c8923880-31e7-4774-8027-b0681fe465be")
	)
	(fp_line
		(start -2.15 -0.95)
		(end -1.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f0c32c8e-4bcb-459e-8b13-575da92c932b")
	)
	(fp_line
		(start -1.85 -1.55)
		(end -2.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "954be203-beeb-4462-972a-60961e7d4f8a")
	)
	(fp_line
		(start -1.85 -0.95)
		(end -1.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d4745905-37aa-4595-b3ff-432b45577f76")
	)
	(fp_line
		(start -1.15 -1.55)
		(end -1.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f1d3a1ef-055a-4738-8f70-e40764250bc2")
	)
	(fp_line
		(start -1.15 -0.95)
		(end -0.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b2b9e4c1-2025-4ed7-b1ef-f72320778a1c")
	)
	(fp_line
		(start -0.85 -1.55)
		(end -1.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "23e6dc47-ea05-4ce8-93d2-2a74bf8da310")
	)
	(fp_line
		(start -0.85 -0.95)
		(end -0.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5407d2ab-cedc-47d4-9ab7-fd3e19f6f0d7")
	)
	(fp_line
		(start -0.15 -1.55)
		(end -0.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "92c9ccaa-a8ee-4af8-ba26-8be816fa710c")
	)
	(fp_line
		(start -0.15 -0.95)
		(end 0.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cf498ea3-ebc5-485d-9a06-3b374bd96898")
	)
	(fp_line
		(start 0.15 -1.55)
		(end -0.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "75c28e0d-2741-4db1-9d98-2a25deccc493")
	)
	(fp_line
		(start 0.15 -0.95)
		(end 0.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5f33f6bd-744f-4f2e-be96-9f5b166e16ac")
	)
	(fp_line
		(start 0.85 -1.55)
		(end 0.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2284d824-c6dd-4d42-ab6c-91e5dc300785")
	)
	(fp_line
		(start 0.85 -0.95)
		(end 1.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "533b0a69-1658-44b6-9336-faa6be431bad")
	)
	(fp_line
		(start 1.15 -1.55)
		(end 0.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5bc0fb21-2ac5-424e-ba2c-9a2d6ab389a0")
	)
	(fp_line
		(start 1.15 -0.95)
		(end 1.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ac0b9894-fb25-4af0-8893-573e10b10aa4")
	)
	(fp_line
		(start 1.85 -1.55)
		(end 1.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3bc8c890-9515-407d-a6ee-29e7b519717c")
	)
	(fp_line
		(start 1.85 -0.95)
		(end 2.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f3afabf4-bd92-4016-aa9b-753bba2c15cd")
	)
	(fp_line
		(start 2.15 -1.55)
		(end 1.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "136a4878-b70c-4718-aa2f-f9290911871e")
	)
	(fp_line
		(start 2.15 -0.95)
		(end 2.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8a104680-38f1-48d1-a207-718adfa27a30")
	)
	(fp_line
		(start 2.85 -1.55)
		(end 2.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b2c45f67-bf42-4b43-9b44-513e53832b5d")
	)
	(fp_line
		(start 2.85 -0.95)
		(end 3.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "498f8882-5219-41b9-868c-ecb8fb7aeb90")
	)
	(fp_line
		(start 3.15 -1.55)
		(end 2.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6c9617fa-146b-433e-b404-a57bd1a45487")
	)
	(fp_line
		(start 3.15 -0.95)
		(end 3.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "234eb808-e113-4614-908f-648e002ae75f")
	)
	(fp_line
		(start 3.85 -1.55)
		(end 3.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fc17149b-850c-4e67-bd88-38f057526de7")
	)
	(fp_line
		(start 3.85 -0.95)
		(end 4.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "73bae1e4-6d47-437b-9a41-5be90f020730")
	)
	(fp_line
		(start 4.15 -1.55)
		(end 3.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c9137868-7237-4c4c-b819-494683ddcf2e")
	)
	(fp_line
		(start 4.15 -0.95)
		(end 4.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e1c97b80-b0a9-4a0e-a868-f56888e7a718")
	)
	(fp_line
		(start 4.85 -1.55)
		(end 4.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c0d14820-d8ea-4fbe-965b-efe741732e10")
	)
	(fp_line
		(start 4.85 -0.95)
		(end 5.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "52ab7204-d920-4029-85f4-71df842f5220")
	)
	(fp_line
		(start 5.15 -1.55)
		(end 4.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c297d2b8-ed7a-40cc-90f2-9b6bf1d77fd1")
	)
	(fp_line
		(start 5.15 -0.95)
		(end 5.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fc45c721-a094-4ad4-b8f1-7bd3b84e88b1")
	)
	(fp_line
		(start 5.85 -1.55)
		(end 5.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6c414e47-4677-4b0f-870b-406b01febd7d")
	)
	(fp_line
		(start 5.85 -0.95)
		(end 6.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ab640184-1a77-41eb-8d96-9540edbca411")
	)
	(fp_line
		(start 6.15 -1.55)
		(end 5.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "eccd7268-aa9b-44c2-9ad0-df207e167ff8")
	)
	(fp_line
		(start 6.15 -0.95)
		(end 6.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2e8acff4-82e3-4ba6-adcf-b73639d42344")
	)
	(fp_line
		(start 6.85 -1.55)
		(end 6.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a0c74d44-3c56-4275-bed6-5f5cb9b5ca6d")
	)
	(fp_line
		(start 6.85 -0.95)
		(end 7.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "71870ab9-17ab-4362-8daa-0ce55fcf3fd6")
	)
	(fp_line
		(start 7.15 -1.55)
		(end 6.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "64ed71b3-d524-4e4f-bdb2-318ec026727e")
	)
	(fp_line
		(start 7.15 -0.95)
		(end 7.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9dd4a018-af9b-4aae-860d-e6e62c64d654")
	)
	(fp_line
		(start 8.5 1)
		(end 8.5 -1.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "39bf1775-5e25-4aa2-ae4f-c3edb9c4d1b3")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -0.65 0)
		(layer "F.Fab")
		(uuid "ef411d64-fd93-4742-89c5-15cbe0b90c8e")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
		)
	)
	(pad "1" smd roundrect
		(at -7 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f7ec2a32-3b04-46e3-ad3f-64f6f8b24cf1")
	)
	(pad "2" smd roundrect
		(at -6 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f701cac6-236c-41dc-8297-31ff85fb68b5")
	)
	(pad "3" smd roundrect
		(at -5 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "36680383-4534-4143-987c-8e826e51fc74")
	)
	(pad "4" smd roundrect
		(at -4 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "cb6364f8-97b9-4330-a314-9ada08baa491")
	)
	(pad "5" smd roundrect
		(at -3 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "101796fc-8ef4-45cc-bd77-7f8f637840c1")
	)
	(pad "6" smd roundrect
		(at -2 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f6629934-459c-4b7f-b4df-aabe858ad6e8")
	)
	(pad "7" smd roundrect
		(at -1 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8bf9412f-042c-46b2-8706-c2c2bba2e382")
	)
	(pad "8" smd roundrect
		(at 0 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2d63ff02-6440-46c9-96a4-32c7257464e3")
	)
	(pad "9" smd roundrect
		(at 1 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7cf2cc75-0887-4307-907d-7d852049c596")
	)
	(pad "10" smd roundrect
		(at 2 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7a1f2bf7-6b1d-4cca-9d00-afffe6938630")
	)
	(pad "11" smd roundrect
		(at 3 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9440f5ca-47d1-4b73-8d54-46ed18f54066")
	)
	(pad "12" smd roundrect
		(at 4 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "cbbc7d17-9f29-47f8-9d53-74ba43cc4b33")
	)
	(pad "13" smd roundrect
		(at 5 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "04b8d944-778f-4e39-8531-1a86af51c73d")
	)
	(pad "14" smd roundrect
		(at 6 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1ec60cb6-2038-4dd9-a3d2-5494abea9fda")
	)
	(pad "15" smd roundrect
		(at 7 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "bdcf9695-56b4-4467-8529-0f4b945e21b2")
	)
	(pad "MP" smd roundrect
		(at -8.3 -1.2)
		(size 1.2 1.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2083333333)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "92eb8119-fc61-4e2b-b36c-9733bb8ef663")
	)
	(pad "MP" smd roundrect
		(at 8.3 -1.2)
		(size 1.2 1.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2083333333)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f35db526-8169-44b1-80f7-04a3b66b85fc")
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM15B-SRSS-TB.STEP"
		(offset
			(xyz 0 0.45 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)