(footprint "Self-clinching_standoff_blind_M2x4"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "H1"
		(at 0 -3.7 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "2783301b-9789-4215-a5da-770d00274f2a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "M3"
		(at 0 3.6 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "ef3d4a33-98ce-4046-80a4-6d94bffbbfd7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Hardware:Self-clinching_standoff_blind_M2x4"
		(at -0.625 -12.75 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b31b94e0-79bc-406c-afd9-72b03357a3cf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at -0.625 -12.75 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1afe09bf-1752-4ab9-b4b5-f9e787ef71e4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at -0.625 -12.75 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4991870d-c2cc-412a-af76-042131901975")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(zone_connect 2)
	(attr through_hole exclude_from_bom)
	(fp_circle
		(center 0 0)
		(end 2.4 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "B.CrtYd")
		(uuid "1f299861-5f29-4b25-acbe-a5c440589e97")
	)
	(fp_circle
		(center 0 0)
		(end 3.15 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "57be4ee6-3b24-44d4-b90f-ab2137b55c23")
	)
	(fp_line
		(start -2.771211 0.000122)
		(end -1.385711 2.399878)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.Fab")
		(uuid "d0f662ce-8a13-4e68-b6cf-30f993f8559e")
	)
	(fp_line
		(start -1.385711 -2.399878)
		(end -2.771211 -0.000122)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.Fab")
		(uuid "811e863e-0196-4092-aa99-26d0711573d5")
	)
	(fp_line
		(start -1.3855 2.4)
		(end 1.3855 2.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.Fab")
		(uuid "0ab37fb8-78f3-4517-8efa-ab09cd8cb4a5")
	)
	(fp_line
		(start 1.3855 -2.4)
		(end -1.3855 -2.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.Fab")
		(uuid "12b031c4-7f22-4a11-b195-986537c72bcc")
	)
	(fp_line
		(start 1.385711 2.399878)
		(end 2.771211 0.000122)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.Fab")
		(uuid "a10e3255-ee1a-4677-84db-5bf41d8c4469")
	)
	(fp_line
		(start 2.771211 -0.000122)
		(end 1.385711 -2.399878)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.Fab")
		(uuid "6ae60bc0-8bb3-43f9-97e1-0c44d01af94f")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -3.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "cfbccf13-0b8c-45d8-a83b-0bc180e8ec4a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 4.5 4.5)
		(drill 4.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "2467ffbc-48a8-46ce-b186-1cfeba6946de")
	)
	(pad "1" smd circle
		(at 0 0)
		(size 6 6)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 90)
		(uuid "a2bb23ca-bae6-42eb-b4f3-7bc1b1b00098")
	)
	(model "${KICAD6_3DMODEL_DIR}/Hardware.3dshapes/Self-clinching_standoff_blind_M2x4.step"
		(offset
			(xyz 0 0 0.24)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)