(module MOUNT_HOLE_M3 (layer F.Cu) (tedit 550C7CC8)
  (tags "MOUNT HOLE FASTENER SCREW")
  (solder_mask_margin 0.0001)
  (attr virtual)
  (fp_text reference H5 (at 0 -1) (layer F.SilkS) hide
    (effects (font (size 0 0) (thickness 0.15)))
  )
  (fp_text value MOUNT_HOLE (at 0 1) (layer F.SilkS) hide
    (effects (font (size 0 0) (thickness 0.15)))
  )
  (fp_text user "M3 INSERT + PLASTIC WALL 1,75mm" (at 0 3.75) (layer B.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.02)) (justify mirror))
  )
  (fp_circle (center 0 0) (end 4.25 0) (layer B.Fab) (width 0.05))
  (fp_text user M3 (at 2.6 -2.6) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_circle (center 0 0) (end 2.925 0) (layer B.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.1) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad 1 connect circle (at 0 0) (size 6 6) (layers F.Cu F.Mask)
    (zone_connect 2))
)
