(footprint "WSON-6_1.5x1.5mm_P0.5mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "WSON6, http://www.ti.com/lit/ds/symlink/tlv702.pdf")
	(tags "WSON6_1.5x1.5mm_P0.5mm")
	(property "Reference" "U1"
		(at 0 -2 0)
		(layer "F.SilkS")
		(uuid "d1ac1715-8270-4b91-96df-eb511bc86282")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TI_TLV7113333D"
		(at 0 2 0)
		(layer "F.Fab")
		(uuid "218d7178-ad52-4fcd-b884-a6eb030ce5b9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Package_SON:WSON-6_1.5x1.5mm_P0.5mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "489f5802-852f-4078-a6f8-e84ec5bf0903")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8638705e-f287-43b5-9939-9ddbe0956178")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b40d38cd-2abf-48ec-bacd-8ec7103ec614")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "TLV7113333DDSER"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "727ad0f9-7296-4539-952e-2f0a1a798255")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "TI"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ca9b5666-0f89-43ec-aaec-ad9605e6de3d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C2876277"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2b5a0032-c74e-4c02-a8b2-2fc59fc00e40")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.785 0.9)
		(end 0.785 0.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f03163db-6025-427c-a81b-bb2c205ba90f")
	)
	(fp_line
		(start -0.58 -0.9)
		(end 0.78 -0.9)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7072f96a-11d4-4f5e-9399-60087ef670d8")
	)
	(fp_poly
		(pts
			(xy -0.9 -0.9) (xy -1.18 -0.9) (xy -0.9 -1.18) (xy -0.9 -0.9)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "1bcc2425-a8d5-4074-9e58-1bf1c330bac0")
	)
	(fp_line
		(start -1.1 0.55)
		(end -1.1 -0.55)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7f6f8fb6-c4e2-4aad-a07d-77f1eef4ff75")
	)
	(fp_line
		(start -0.75 1)
		(end 0.75 1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "fa0180f2-f52a-4091-a593-4eeaf6fbaf8d")
	)
	(fp_line
		(start 0.75 -1)
		(end -0.75 -1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ffa62027-2463-4c2f-bb4a-b39b221ba029")
	)
	(fp_line
		(start 1.1 -0.55)
		(end 1.1 0.55)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9ec0bcd3-3008-49a6-b2bb-983f293ab081")
	)
	(fp_arc
		(start -1.1 -0.55)
		(mid -1.073607 -0.661803)
		(end -1 -0.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3f8a1feb-ba92-4188-ad6f-15f7dd9fc0fa")
	)
	(fp_arc
		(start -1 -0.75)
		(mid -0.926777 -0.926777)
		(end -0.75 -1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1fae1275-f5b7-44d6-aeec-c61854a1d0fe")
	)
	(fp_arc
		(start -1 0.75)
		(mid -1.073607 0.661803)
		(end -1.1 0.55)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "11adb4de-6316-44c3-bb22-faa428e71427")
	)
	(fp_arc
		(start -0.75 1)
		(mid -0.926777 0.926777)
		(end -1 0.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5d838eae-595f-47cb-b2b9-70f38f0d776f")
	)
	(fp_arc
		(start 0.75 -1)
		(mid 0.926777 -0.926777)
		(end 1 -0.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b6816a0d-dc8b-424b-8dbc-b8ce79d41b89")
	)
	(fp_arc
		(start 1 -0.75)
		(mid 1.073607 -0.661803)
		(end 1.1 -0.55)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bdcec9eb-8512-4733-8b4c-86d99afe5d8f")
	)
	(fp_arc
		(start 1 0.75)
		(mid 0.926777 0.926777)
		(end 0.75 1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "82ee5bfb-80f0-4cc8-add3-83e3b13d4cf5")
	)
	(fp_arc
		(start 1.1 0.55)
		(mid 1.073607 0.661803)
		(end 1 0.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a89bedaa-f81c-4293-a7ee-141de154bb58")
	)
	(fp_line
		(start -0.495 -0.75)
		(end -0.75 -0.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d2ef11b0-b48c-4699-bd53-ed650f189c62")
	)
	(fp_rect
		(start -0.75 -0.75)
		(end 0.75 0.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "befe2cba-c2b0-42c0-b18c-4702cc04671d")
	)
	(fp_text user "${REFERENCE}"
		(at 0.005 0 0)
		(layer "F.Fab")
		(uuid "f3a77b3e-55bf-46da-bd25-4181cf6d62d1")
		(effects
			(font
				(size 0.4 0.4)
				(thickness 0.05)
			)
		)
	)
	(pad "" smd oval
		(at -0.575 -0.5)
		(size 0.6 0.22)
		(layers "F.Paste")
		(uuid "c66f2e44-b2a3-4caf-b100-0bfe756d3736")
	)
	(pad "" smd oval
		(at -0.575 0)
		(size 0.6 0.22)
		(layers "F.Paste")
		(uuid "8c2fe160-c4a7-4add-8424-02bf18012c3a")
	)
	(pad "" smd oval
		(at -0.575 0.5)
		(size 0.6 0.22)
		(layers "F.Paste")
		(uuid "e303b58b-5606-429a-8f05-5007f8ef712e")
	)
	(pad "" smd oval
		(at 0.575 -0.5)
		(size 0.6 0.22)
		(layers "F.Paste")
		(uuid "b0f0e758-8bb1-459c-8fad-d77b8a703cca")
	)
	(pad "" smd oval
		(at 0.575 0)
		(size 0.6 0.22)
		(layers "F.Paste")
		(uuid "528eb8e3-b880-458b-b5cc-d3135e409179")
	)
	(pad "" smd oval
		(at 0.575 0.5)
		(size 0.6 0.22)
		(layers "F.Paste")
		(uuid "de10d55d-47fb-4095-9b06-b022a4d04296")
	)
	(pad "1" smd roundrect
		(at -0.525 -0.5 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(uuid "29939514-092a-49d5-aa07-b114fe801a0c")
	)
	(pad "2" smd roundrect
		(at -0.575 0)
		(size 0.75 0.28)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "2d74cc64-89f9-406d-a50f-220ed2b4d3a4")
	)
	(pad "3" smd roundrect
		(at -0.575 0.5)
		(size 0.75 0.28)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "f555e091-f468-4647-83ec-e2fdfbfdf2c6")
	)
	(pad "4" smd roundrect
		(at 0.575 0.5 180)
		(size 0.75 0.28)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "aedde25c-cb7a-4f69-966f-ebe9ad2b9122")
	)
	(pad "5" smd roundrect
		(at 0.575 0 180)
		(size 0.75 0.28)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "8b2a04f6-5226-4dfd-8639-35906e792a71")
	)
	(pad "6" smd roundrect
		(at 0.575 -0.5 180)
		(size 0.75 0.28)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "b4fd0a75-c295-44c6-ab08-63da4b75d187")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_SON.3dshapes/WSON-6_1.5x1.5mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
