(footprint "XKB_X05C2020TZ_20S_P0.5_Vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.5 -2.075 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "fdea8de6-5e6a-4aff-ae00-44d3e5f7cba1")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "XKB_X05C2020TZ_20S_P0.5_Vertical"
		(at 0.5 1.825 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a914dff8-3af7-472d-aed9-9bcbf87be065")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.0625)
			)
		)
	)
	(property "Footprint" ""
		(at 0.5 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7d49b95d-7f9d-4fec-9dd8-07823f4e7e6a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0.5 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "4caeb9de-d663-4aa4-b552-d6d47253cda4")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0.5 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "6437a9da-8e98-464a-bec6-fcd831e7e7cc")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_arc
		(start -7.775 -1.35)
		(mid -7.753033 -1.403033)
		(end -7.7 -1.425)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a06a2ee8-6574-433e-b5e0-88496655ccdb")
	)
	(fp_arc
		(start -7.7 1.425)
		(mid -7.753033 1.403033)
		(end -7.775 1.35)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "77ae75b3-ccee-4ac9-8481-a113e1d4d5c8")
	)
	(fp_arc
		(start 7.7 -1.425)
		(mid 7.753033 -1.403033)
		(end 7.775 -1.35)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "85439d7f-62d5-4115-9f3a-a0974b8cbc23")
	)
	(fp_arc
		(start 7.775 1.35)
		(mid 7.753033 1.403033)
		(end 7.7 1.425)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0e7391b0-8068-423a-93b5-0d0fd8aa56ff")
	)
	(fp_poly
		(pts
			(xy -4.575 2) (xy -4.925 2) (xy -4.75 1.65)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "2b35a38d-9181-44d0-8ff1-94454e3f60a9")
	)
	(fp_poly
		(pts
			(xy -6.7 -1.35) (xy -7.7 -1.35) (xy -7.7 1.35) (xy -6.7 1.35) (xy -6.7 1.5) (xy -7.7 1.5) (xy -7.85 1.35)
			(xy -7.85 -1.35) (xy -7.7 -1.5) (xy -6.7 -1.5)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "acc1f89d-13f8-46d4-9a87-8fb7df8cc987")
	)
	(fp_poly
		(pts
			(xy 6.7 1.35) (xy 7.7 1.35) (xy 7.7 -1.35) (xy 6.7 -1.35) (xy 6.7 -1.5) (xy 7.7 -1.5) (xy 7.85 -1.35)
			(xy 7.85 1.35) (xy 7.7 1.5) (xy 6.7 1.5)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "9e2238f5-6ed0-43e0-9efd-8ff4a78d4247")
	)
	(fp_line
		(start -8.15 1.1)
		(end -8.15 -1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "09667bd8-1efd-43a8-8684-806a4f7b8e26")
	)
	(fp_line
		(start -7.45 -1.8)
		(end 7.45 -1.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e51d02c4-a4e6-4442-bad1-20c869dec8cf")
	)
	(fp_line
		(start 7.45 1.8)
		(end -7.45 1.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7312c5c2-6098-488d-8a16-97173a18cf1a")
	)
	(fp_line
		(start 8.15 -1.1)
		(end 8.15 1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "75d89da0-58dd-4d37-ade3-585490429268")
	)
	(fp_arc
		(start -8.15 -1.1)
		(mid -7.944975 -1.594975)
		(end -7.45 -1.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "777d8970-7838-4843-83c1-58c3005b3231")
	)
	(fp_arc
		(start -7.45 1.8)
		(mid -7.944975 1.594975)
		(end -8.15 1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3242b275-17f4-456d-aacf-5611c80cf328")
	)
	(fp_arc
		(start 7.45 -1.8)
		(mid 7.944975 -1.594975)
		(end 8.15 -1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9321415c-e5dd-4496-b267-3821ba23791b")
	)
	(fp_arc
		(start 8.15 1.1)
		(mid 7.944975 1.594975)
		(end 7.45 1.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "449b18a4-477c-4d8a-a410-ecbc033e123b")
	)
	(fp_line
		(start -7.8 -1)
		(end -7 -1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "2960ce21-84f5-4df1-82da-785de48ec0fb")
	)
	(fp_line
		(start -7.8 1)
		(end -7.8 -1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "e94b81b7-9e98-4a56-989b-6ecb37b7c6d7")
	)
	(fp_line
		(start -7 1)
		(end -7.8 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "4ca1f169-0c4f-43c0-a727-3d78ac6b0505")
	)
	(fp_line
		(start 7 -1)
		(end 7.8 -1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "2ade3bb3-f0d3-4e8f-abe1-65e46e2de153")
	)
	(fp_line
		(start 7.8 -1)
		(end 7.8 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "458fc4ca-2d2e-430f-8c63-089207d4b3a8")
	)
	(fp_line
		(start 7.8 1)
		(end 7 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "16130a96-2de2-4465-af0c-f445bba4d643")
	)
	(fp_rect
		(start -6.75 -1)
		(end 6.75 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "19ef6e31-d98b-4f89-92ea-f64d1a27b66b")
	)
	(fp_text user "${REFERENCE}"
		(at 4.875 0.025 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "8178711a-83ed-410c-8e4a-25efd16e1ac9")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.0625)
			)
		)
	)
	(pad "1" smd roundrect
		(at -4.75 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "528bc1dc-3783-472e-8551-f3ae144fa3df")
	)
	(pad "2" smd roundrect
		(at -4.25 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "12a5d048-a826-4a6d-b7e4-716d73e116c5")
	)
	(pad "3" smd roundrect
		(at -3.75 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "46910f7d-a141-45d9-8bf8-d58ee1862f0d")
	)
	(pad "4" smd roundrect
		(at -3.25 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "80a0e5ad-6785-4dd2-98eb-0eecd5f38d4a")
	)
	(pad "5" smd roundrect
		(at -2.75 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "1f0edc3f-d288-450e-a6c9-b76c124a8820")
	)
	(pad "6" smd roundrect
		(at -2.25 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "91c83b2a-abb4-49b7-a5c8-f3812d9d088f")
	)
	(pad "7" smd roundrect
		(at -1.75 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "76e30d60-2fe2-4956-9304-339358eb8abd")
	)
	(pad "8" smd roundrect
		(at -1.25 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "a1f6995d-a2e0-4768-9aac-9707aeb5b8da")
	)
	(pad "9" smd roundrect
		(at -0.75 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "fd4346c2-9fc6-4ece-af2f-ab4309bc818b")
	)
	(pad "10" smd roundrect
		(at -0.25 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "61e0cd6a-6f03-42ab-bb74-97187818e56a")
	)
	(pad "11" smd roundrect
		(at 0.25 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "1c340d4c-1888-4fb3-9f98-ad89039d0850")
	)
	(pad "12" smd roundrect
		(at 0.75 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "315a8158-3581-4bf2-a354-cd65c1251b1d")
	)
	(pad "13" smd roundrect
		(at 1.25 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "2bc4da90-351a-42e7-8c09-b552f19d98ee")
	)
	(pad "14" smd roundrect
		(at 1.75 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "334d55c8-8065-494d-812d-688b37c2330e")
	)
	(pad "15" smd roundrect
		(at 2.25 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "f22750e4-4b07-4d8a-9f75-741fdecb85ea")
	)
	(pad "16" smd roundrect
		(at 2.75 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "aae741bd-a0b0-4603-a8aa-f849705d6282")
	)
	(pad "17" smd roundrect
		(at 3.25 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "66cbaba1-e965-405a-9cc5-10fab47003a4")
	)
	(pad "18" smd roundrect
		(at 3.75 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "02013653-18cf-481b-904c-b9b03c73576d")
	)
	(pad "19" smd roundrect
		(at 4.25 0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "2606ff1a-25ff-4103-aa9e-ad6be0b3a3d5")
	)
	(pad "20" smd roundrect
		(at 4.75 -0.975)
		(size 0.4 1.15)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
		(uuid "a0484981-2c3b-44fd-8532-19366e0456b5")
	)
	(pad "MP" smd roundrect
		(at -6.55 0)
		(size 2 2.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "5aeec327-8b6a-4a33-901e-3a87a55b1e40")
	)
	(pad "MP" smd roundrect
		(at 6.55 0)
		(size 2 2.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "43e142f2-72e1-4622-95bc-c99dddd7fbad")
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/X05C2020XZ.stp"
		(hide yes)
		(offset
			(xyz 0 0 4.4)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/FPC-SMD_20P-P0.50X05C2020TZ.step"
		(offset
			(xyz 0 2.95 2.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
