(module Program_Pogo_5P_2mm (layer F.Cu) (tedit 547DF31A)
  (fp_text reference Program_5P_2mm (at -2 0 90) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value VAL** (at 2 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user 1 (at 1.5 -4) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (pad 1 thru_hole circle (at 0 -4) (size 1.7 1.7) (drill 0.78) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 -2) (size 1.7 1.7) (drill 0.78) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 0.78) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 2) (size 1.7 1.7) (drill 0.78) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 4) (size 1.7 1.7) (drill 0.78) (layers *.Cu *.Mask))
)
