(footprint "WLCSP-9_1.21x1.21mm_P0.4mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "LCSC" "C891247")
  (property "MFG" "ONSemi")
  (property "MPN" "FPF2495CUCX")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (attr smd)
  (fp_text reference "U28" (at 0 -1.45 unlocked) (layer "F.SilkS") hide
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp dfd4a888-d20b-4f2c-a0c5-af0a2edb3d17)
  )
  (fp_text value "FPF2495C" (at 0 1.05 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)))
    (tstamp 0aec2410-7e03-4ee6-b448-83b1298cfc68)
  )
  (fp_text user "${REFERENCE}" (at 0 -1 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)))
    (tstamp e195adea-b1b5-4b56-8ad5-d254ef495cc1)
  )
  (fp_arc (start -0.7 0.775) (mid -0.753033 0.753033) (end -0.775 0.7)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 31fab9d6-f567-4ec0-84cf-f3d8b0846366))
  (fp_arc (start 0.7 -0.775) (mid 0.753033 -0.753033) (end 0.775 -0.7)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 726f31a9-dc69-40c8-a5e5-b2f6b706c466))
  (fp_arc (start 0.775 0.7) (mid 0.753033 0.753033) (end 0.7 0.775)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 2bda5d6a-f7fe-4c29-bc24-7c8fe06dd9ec))
  (fp_poly
    (pts
      (xy -0.4 -0.7)
      (xy 0.7 -0.7)
      (xy 0.7 0.7)
      (xy -0.7 0.7)
      (xy -0.7 -0.4)
      (xy -0.85 -0.4)
      (xy -0.85 0.7)
      (xy -0.7 0.85)
      (xy 0.7 0.85)
      (xy 0.85 0.7)
      (xy 0.85 -0.7)
      (xy 0.7 -0.85)
      (xy -0.4 -0.85)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 54c6705a-b9c8-4530-a43b-66489ba3fdb4))
  (fp_line (start -0.85 -0.6) (end -0.85 0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 07b21614-2093-4a4c-87d2-09bd2945b685))
  (fp_line (start -0.6 0.85) (end 0.6 0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 12d17512-1653-451c-94b0-754a78c0657d))
  (fp_line (start 0.6 -0.85) (end -0.6 -0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 693d42a2-2fcc-4727-b06e-78a7d6faa486))
  (fp_line (start 0.85 0.6) (end 0.85 -0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9442b3c5-689b-4296-b4ed-dc3849cbfcab))
  (fp_arc (start -0.85 -0.6) (mid -0.776777 -0.776777) (end -0.6 -0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4d92b5ce-4416-47bf-aa45-42c5426a38f5))
  (fp_arc (start -0.6 0.85) (mid -0.776777 0.776777) (end -0.85 0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d03a6297-efa3-4a49-8a3f-cab54f2b3b7f))
  (fp_arc (start 0.6 -0.85) (mid 0.776777 -0.776777) (end 0.85 -0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b208c4d8-c53d-4233-9f0d-771eb29dfc7a))
  (fp_arc (start 0.85 0.6) (mid 0.776777 0.776777) (end 0.6 0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1125847c-fc8f-434a-918d-4f0dcc462a9e))
  (fp_rect (start -0.605 -0.605) (end 0.605 0.605)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.Fab") (tstamp b5895b0d-6f6c-4ae9-bf1a-181910512575))
  (pad "" smd roundrect (at -0.4 -0.4) (size 0.25 0.25) (layers "F.Paste") (roundrect_rratio 0.2)
    (clearance 0.05) (tstamp 65e36c20-48a6-4088-bbec-afcfb9e2a822))
  (pad "" smd roundrect (at -0.4 0) (size 0.25 0.25) (layers "F.Paste") (roundrect_rratio 0.2)
    (clearance 0.05) (tstamp dd9ed6a0-044a-47b8-9b37-e71e42f05d4b))
  (pad "" smd roundrect (at -0.4 0.4) (size 0.25 0.25) (layers "F.Paste") (roundrect_rratio 0.2)
    (clearance 0.05) (tstamp d3d652bd-ae38-4aa7-88e0-fd8049e309e7))
  (pad "" smd roundrect (at 0 -0.4) (size 0.25 0.25) (layers "F.Paste") (roundrect_rratio 0.2)
    (clearance 0.05) (tstamp a7479116-97e3-42ab-9be7-bf8c25536e6e))
  (pad "" smd roundrect (at 0 0) (size 0.25 0.25) (layers "F.Paste") (roundrect_rratio 0.2)
    (clearance 0.05) (tstamp 10ca34c8-a53e-4f0b-b578-85484d0bb198))
  (pad "" smd roundrect (at 0 0.4) (size 0.25 0.25) (layers "F.Paste") (roundrect_rratio 0.2)
    (clearance 0.05) (tstamp aa86fdaa-033a-4eb6-a3ba-7713124eb1fb))
  (pad "" smd roundrect (at 0.4 -0.4) (size 0.25 0.25) (layers "F.Paste") (roundrect_rratio 0.2)
    (clearance 0.05) (tstamp d257f9c1-c09d-4a9c-819c-132a2f654cbd))
  (pad "" smd roundrect (at 0.4 0) (size 0.25 0.25) (layers "F.Paste") (roundrect_rratio 0.2)
    (clearance 0.05) (tstamp 0e8a0a90-42fd-409a-9da4-ac83869412e4))
  (pad "" smd roundrect (at 0.4 0.4) (size 0.25 0.25) (layers "F.Paste") (roundrect_rratio 0.2)
    (clearance 0.05) (tstamp 7f6b10fd-6078-4bbf-8e40-8a2c75805c7b))
  (pad "A1" smd circle (at -0.4 -0.4) (size 0.2 0.2) (layers "F.Cu" "F.Mask")
    (clearance 0.05) (tstamp 84a79f39-afbe-4ba3-95ac-ce75b2cb20cb))
  (pad "A2" smd circle (at 0 -0.4) (size 0.2 0.2) (layers "F.Cu" "F.Mask")
    (clearance 0.05) (tstamp 5b3d39ed-9796-4570-9349-a1f13a24cd34))
  (pad "A3" smd circle (at 0.4 -0.4) (size 0.2 0.2) (layers "F.Cu" "F.Mask")
    (clearance 0.05) (tstamp f55bdd35-5ce9-4b3f-8030-c4fc91075ec5))
  (pad "B1" smd circle (at -0.4 0) (size 0.2 0.2) (layers "F.Cu" "F.Mask")
    (clearance 0.05) (tstamp d1681192-df62-4a55-b65c-87d3f5fb404b))
  (pad "B2" smd circle (at 0 0) (size 0.2 0.2) (layers "F.Cu" "F.Mask")
    (clearance 0.05) (tstamp 6e00622f-aec1-4d75-8d5f-694a210cfe3b))
  (pad "B3" smd circle (at 0.4 0) (size 0.2 0.2) (layers "F.Cu" "F.Mask")
    (clearance 0.05) (tstamp 5020ee84-06e7-4d6d-9c0d-2d85d34ea9be))
  (pad "C1" smd circle (at -0.4 0.4) (size 0.2 0.2) (layers "F.Cu" "F.Mask")
    (clearance 0.05) (tstamp 156c7fe3-ebac-47a3-9de9-c5592ab925a4))
  (pad "C2" smd circle (at 0 0.4) (size 0.2 0.2) (layers "F.Cu" "F.Mask")
    (clearance 0.05) (tstamp b26ca77c-8517-4b7d-9191-da5bd4d01bd8))
  (pad "C3" smd circle (at 0.4 0.4) (size 0.2 0.2) (layers "F.Cu" "F.Mask")
    (clearance 0.05) (tstamp 2ff8d1fe-e311-4a10-9547-e3718b3098ad))
  (model ":KICAD7_3DMODEL_DIR:Package_WL-CSP.3dshapes/WLCSP-9_1.21x1.21_P0.4.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
