(module MOUNT_HOLE_M5 (layer F.Cu) (tedit 54F750FE)
  (tags "MOUNT HOLE FASTENER SCREW")
  (solder_mask_margin 0.0001)
  (attr virtual)
  (fp_text reference H5 (at 0 -1) (layer F.SilkS) hide
    (effects (font (size 0 0) (thickness 0.15)))
  )
  (fp_text value MOUNT_HOLE (at 0 1) (layer F.SilkS) hide
    (effects (font (size 0 0) (thickness 0.15)))
  )
  (fp_text user M5 (at 3.4 -4.6) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_circle (center 0 0) (end 4.925 0) (layer B.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 5.1) (layers *.Cu *.Mask)
    (zone_connect 2))
  (pad 1 connect circle (at 0 0) (size 10 10) (layers F.Cu F.Mask)
    (zone_connect 2))
)
