(footprint "Solder_Bridge_NC"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "JP2"
		(at 2.25 0.5 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "0c178a6f-894b-4df8-8684-8b560c147b63")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "UVLO"
		(at 0 1.399999 180)
		(layer "F.Fab")
		(uuid "1547b417-5897-4fb2-a991-3bdcbde738a7")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Solder_Bridge_NC"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4f99d6a7-0209-4380-951d-39fcfb6b637b")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "be09ffe9-444c-478e-b69d-14aa258990d8")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" "Solder Jumper, 2-pole, closed/bridged"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7511ac47-c0fe-494a-bb46-f26298377d0e")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Sim.Enable" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6968af87-c8ed-4d73-b4d4-fc288a43fa2c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.01)
	(attr exclude_from_pos_files exclude_from_bom)
	(pad "" connect oval
		(at 0 0)
		(size 1.4 0.2)
		(layers "F.Mask")
		(solder_mask_margin 0.4)
		(uuid "7eb67a61-cb8c-4bc4-ab73-fb88ee49e243")
	)
	(pad "" smd oval
		(at 0 0)
		(size 2.2 1)
		(layers "F.Paste")
		(uuid "3ca51051-f564-42d0-88f7-00f1dc738f17")
	)
	(pad "1" connect custom
		(at -1 0)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 0 0)
				(mid 0.010648 -0.09168)
				(end 0.042026 -0.178479)
				(width 0.2)
			)
			(gr_arc
				(start 0.042026 0.178479)
				(mid 0.010648 0.09168)
				(end 0 0)
				(width 0.2)
			)
			(gr_line
				(start 0 0)
				(end 1.6 0)
				(width 0.2)
			)
		)
		(uuid "d6d19d54-0ec9-40a8-a842-be4f0bdc858f")
	)
	(pad "2" connect custom
		(at 1 0)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.4 -0.4)
				(mid 0 0)
				(end -0.4 0.4)
				(width 0.2)
			)
			(gr_line
				(start -0.4 0.4)
				(end -1.6 0.4)
				(width 0.2)
			)
			(gr_line
				(start -0.4 -0.4)
				(end -1.6 -0.4)
				(width 0.2)
			)
		)
		(uuid "d0cd775c-7b80-46dd-a805-70793331dbe4")
	)
)
